Bid Addendum 01 for Forklifts for Day labor and Central Sign Shop, 2018-15

April 18, 2018

The specification 183-60-01 titled 3,500 Pound Electric Powered Counterbalanced, Material-Handling Forklift listed on the subject solicitation has been amended as follows:

Page No. 2:

**Currently Reads:**

**Capacities and Dimensions:**

The forklift shall be a four-wheel design, with rubber, polyurethane drive/steer tires.

Complies:  Yes   No

**Should Read:**

**Capacities and Dimensions:**

The forklift shall be a four-wheel design, with rubber cushion style drive/steer tires.

Complies:  Yes   No

Page No. 4:

**Currently Reads:**

**Batteries:**

The battery compartment shall be the largest offered for a machine of this rating.

Complies:  Yes   No

|  |  |
| --- | --- |
| Describe: |  |

|  |  |
| --- | --- |
|  |  |

The fork lift shall operate on 36-volts and include a battery charger for recharging the batterie(s) operating on 110-volts.

Complies:  Yes   No

Provide the amp hour rating of the battery pack for the specified machine.

|  |  |
| --- | --- |
| Describe: |  |

|  |  |
| --- | --- |
|  |  |

**Should Read:**

**Batteries:**

The battery compartment shall be the largest offered for a machine of this rating.

Complies:  Yes   No

|  |  |
| --- | --- |
| Describe: |  |

|  |  |
| --- | --- |
|  |  |

The fork lift shall operate on 36-volts and include a battery charger for recharging the batterie(s).  The charger shall be compatible with 208-volt, 3-phase electrical circuitry.  All wiring and connections will be completed by others.

Complies:  Yes   No

Provide the amp hour rating of the battery pack for the specified machine.

|  |  |
| --- | --- |
| Describe: |  |

|  |  |
| --- | --- |
|  |  |