## Pay Items
| PAY ITEM | August 2, 2018 LETTING | UNIT OF | PAY ITEM.1 | COUNTY | D | CONTRACT | LETTING |
| --- | --- | --- | --- | --- | --- | --- | --- |
| NUMBER | PAY ITEM DESCRIPTION | MEASURE | QUANTITY | NaN | O | NUMBER | ITEM # |
| X0783300 | P.S. ELECTRICAL WORK | L SUM | 1 | MADISON | 8 | 46526 | 50 |
| 67100100 | MOBILIZATION | L SUM | 1 | MADISON | 8 | 46526 | 50 |
| X0335700 | P.S. GENERAL WORK | L SUM | 1 | LOGAN | 6 | 46528 | 51 |
| X0783300 | P.S. ELECTRICAL WORK | L SUM | 1 | LOGAN | 6 | 46528 | 51 |
| Z0007101 | C&D LEAD PT CL RS N1 | L SUM | 1 | LOGAN | 6 | 46528 | 51 |
| Z0012754 | STR REP CON DP = < 5 | SQ FT | 0.8 | LOGAN | 6 | 46528 | 51 |
| Z0034100 | MASONRY WALL CONSTR | SQ FT | 130 | LOGAN | 6 | 46528 | 51 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | LOGAN | 6 | 46528 | 51 |
| 50500405 | F & E STRUCT STEEL | POUND | 186 | LOGAN | 6 | 46528 | 51 |
| 58700300 | CONCRETE SEALER | SQ FT | 330 | LOGAN | 6 | 46528 | 51 |
| 67100100 | MOBILIZATION | L SUM | 1 | LOGAN | 6 | 46528 | 51 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | LOGAN | 6 | 46528 | 51 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 12749 | VARIOUS | 2 | 46530 | 1 |
| 78100300 | REPLACEMENT REFLECTOR | EACH | 21130 | VARIOUS | 2 | 46530 | 1 |
| 78300200 | RAISED REF PVT MK REM | EACH | 7500 | VARIOUS | 2 | 46530 | 1 |
| X4401198 | HMA SURF REM VAR DP | SQ YD | 2903 | KNOX | 4 | 68758 | 13 |
| X4810200 | AGGREGATE SHLD REMOVL | CU YD | 14 | KNOX | 4 | 68758 | 13 |
| X6060097 | CLASS SI CONC OUT SPL | CU YD | 25 | KNOX | 4 | 68758 | 13 |
| X6062700 | CONC GUTTER TA SPL | FOOT | 830 | KNOX | 4 | 68758 | 13 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | KNOX | 4 | 68758 | 13 |
| Z0001002 | GDRL AGG EROS CONT | TON | 218 | KNOX | 4 | 68758 | 13 |
| Z0001900 | ASB BEARING PAD REMOV | EACH | 24 | KNOX | 4 | 68758 | 13 |
| Z0004638 | PAVT BREAKING | SQ YD | 634 | KNOX | 4 | 68758 | 13 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | KNOX | 4 | 68758 | 13 |
| Z0022800 | FENCE REMOVAL | FOOT | 329 | KNOX | 4 | 68758 | 13 |
| Z0046304 | P UNDR FOR STRUCT 4 | FOOT | 133 | KNOX | 4 | 68758 | 13 |
| Z0054400 | ROCK FILL | CU YD | 82 | KNOX | 4 | 68758 | 13 |
| Z0076600 | TRAINEES | HOUR | 1000 | KNOX | 4 | 68758 | 13 |
| Z0076604 | TRAINEES TPG | HOUR | 1000 | KNOX | 4 | 68758 | 13 |
| 20100110 | TREE REMOV 6-15 | UNIT | 26 | KNOX | 4 | 68758 | 13 |
| 20100500 | TREE REMOV ACRES | ACRE | 0.4 | KNOX | 4 | 68758 | 13 |
| 20200100 | EARTH EXCAVATION | CU YD | 5906 | KNOX | 4 | 68758 | 13 |
| 20200500 | EARTH EXC WID | CU YD | 17.5 | KNOX | 4 | 68758 | 13 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 615.7 | KNOX | 4 | 68758 | 13 |
| 20900110 | POROUS GRAN BACKFILL | CU YD | 470 | KNOX | 4 | 68758 | 13 |
| 21101615 | TOPSOIL F & P 4 | SQ YD | 10412 | KNOX | 4 | 68758 | 13 |
| 25000210 | SEEDING CL 2A | ACRE | 2.57 | KNOX | 4 | 68758 | 13 |
| 25000400 | NITROGEN FERT NUTR | POUND | 194.3 | KNOX | 4 | 68758 | 13 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 194.3 | KNOX | 4 | 68758 | 13 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 194.3 | KNOX | 4 | 68758 | 13 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 9679 | KNOX | 4 | 68758 | 13 |
| 25100635 | HD EROS CONTR BLANKET | SQ YD | 404 | KNOX | 4 | 68758 | 13 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 52 | KNOX | 4 | 68758 | 13 |
| 28000400 | PERIMETER EROS BAR | FOOT | 3607 | KNOX | 4 | 68758 | 13 |
| 28000500 | INLET & PIPE PROTECT | EACH | 3 | KNOX | 4 | 68758 | 13 |
| 28100107 | STONE RIPRAP CL A4 | SQ YD | 2084 | KNOX | 4 | 68758 | 13 |
| 28100125 | STONE RIPRAP CL B3 | SQ YD | 204 | KNOX | 4 | 68758 | 13 |
| 28100127 | STONE RIPRAP CL B4 | SQ YD | 34 | KNOX | 4 | 68758 | 13 |
| 28200200 | FILTER FABRIC | SQ YD | 2322 | KNOX | 4 | 68758 | 13 |
| 31100100 | SUB GRAN MAT A | TON | 1440 | KNOX | 4 | 68758 | 13 |
| 40200700 | AGG SURF CSE A 8 | SQ YD | 100 | KNOX | 4 | 68758 | 13 |
| 40600295 | P BIT MATLS TACK CT | POUND | 7655 | KNOX | 4 | 68758 | 13 |
| 40600825 | P LEV BIND MM N50 | TON | 261 | KNOX | 4 | 68758 | 13 |
| 40600982 | HMA SURF REM BUTT JT | SQ YD | 280.7 | KNOX | 4 | 68758 | 13 |
| 40600990 | TEMPORARY RAMP | SQ YD | 149 | KNOX | 4 | 68758 | 13 |
| 40603080 | HMA BC IL-19.0 N50 | TON | 35 | KNOX | 4 | 68758 | 13 |
| 40603310 | HMA SC "C" N50 | TON | 60 | KNOX | 4 | 68758 | 13 |
| 40603535 | P HMA SC "D" N50 | TON | 261 | KNOX | 4 | 68758 | 13 |
| 40701886 | HMA PAVT FD 10 1/4 | SQ YD | 1328 | KNOX | 4 | 68758 | 13 |
| 40800050 | INCIDENTAL HMA SURF | TON | 19 | KNOX | 4 | 68758 | 13 |
| 42000080 | PVT CON PCC BR APP SL | SQ YD | 71 | KNOX | 4 | 68758 | 13 |
| 44000100 | PAVEMENT REM | SQ YD | 953 | KNOX | 4 | 68758 | 13 |
| 44000157 | HMA SURF REM 2 | SQ YD | 395 | KNOX | 4 | 68758 | 13 |
| 44000400 | GUTTER REM | FOOT | 540 | KNOX | 4 | 68758 | 13 |
| 44004250 | PAVED SHLD REMOVAL | SQ YD | 226 | KNOX | 4 | 68758 | 13 |
| 44200050 | WELDED WIRE REINF | SQ YD | 38 | KNOX | 4 | 68758 | 13 |
| 44201796 | CL D PATCH T4 12 | SQ YD | 202 | KNOX | 4 | 68758 | 13 |
| 48100500 | AGGREGATE SHLDS A 6 | SQ YD | 233 | KNOX | 4 | 68758 | 13 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 50 | KNOX | 4 | 68758 | 13 |
| 48203100 | HMA SHOULDERS | TON | 315 | KNOX | 4 | 68758 | 13 |
| 50100300 | REM EXIST STRUCT N1 | EACH | 1 | KNOX | 4 | 68758 | 13 |
| 50100400 | REM EXIST STRUCT N2 | EACH | 1 | KNOX | 4 | 68758 | 13 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 69 | KNOX | 4 | 68758 | 13 |
| 50200300 | COFFERDAM EXCAVATION | CU YD | 369 | KNOX | 4 | 68758 | 13 |
| 50201121 | COFFERDAM TYP 2 LOC 1 | EACH | 1 | KNOX | 4 | 68758 | 13 |
| 50201122 | COFFERDAM TYP 2 LOC 2 | EACH | 1 | KNOX | 4 | 68758 | 13 |
| 50300225 | CONC STRUCT | CU YD | 156.1 | KNOX | 4 | 68758 | 13 |
| 50300255 | CONC SUP-STR | CU YD | 146.8 | KNOX | 4 | 68758 | 13 |
| 50300260 | BR DECK GROOVING | SQ YD | 565 | KNOX | 4 | 68758 | 13 |
| 50300265 | SEAL COAT CONC | CU YD | 92.4 | KNOX | 4 | 68758 | 13 |
| 50300300 | PROTECTIVE COAT | SQ YD | 723 | KNOX | 4 | 68758 | 13 |
| 50301350 | CONC SUPSTR APP SLAB | CU YD | 99 | KNOX | 4 | 68758 | 13 |
| 50500105 | F & E STRUCT STEEL | L SUM | 1 | KNOX | 4 | 68758 | 13 |
| 50500505 | STUD SHEAR CONNECTORS | EACH | 3402 | KNOX | 4 | 68758 | 13 |
| 50800105 | REINFORCEMENT BARS | POUND | 1220 | KNOX | 4 | 68758 | 13 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 76630 | KNOX | 4 | 68758 | 13 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 310 | KNOX | 4 | 68758 | 13 |
| 51201610 | FUR STL PILE HP12X63 | FOOT | 320 | KNOX | 4 | 68758 | 13 |
| 51202305 | DRIVING PILES | FOOT | 630 | KNOX | 4 | 68758 | 13 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 2 | KNOX | 4 | 68758 | 13 |
| 51203610 | TEST PILE ST HP12X63 | EACH | 2 | KNOX | 4 | 68758 | 13 |
| 51500100 | NAME PLATES | EACH | 2 | KNOX | 4 | 68758 | 13 |
| 52100505 | ANCHOR BOLTS 5/8 | EACH | 24 | KNOX | 4 | 68758 | 13 |
| 52100520 | ANCHOR BOLTS 1 | EACH | 24 | KNOX | 4 | 68758 | 13 |
| 54001001 | BOX CUL END SEC C1 | EACH | 1 | KNOX | 4 | 68758 | 13 |
| 54003000 | CONC BOX CUL | CU YD | 6.4 | KNOX | 4 | 68758 | 13 |
| 54010705 | PCBC 7X5 | FOOT | 102 | KNOX | 4 | 68758 | 13 |
| 542D0223 | P CUL CL D 1 18 | FOOT | 19 | KNOX | 4 | 68758 | 13 |
| 542D0229 | P CUL CL D 1 24 | FOOT | 68 | KNOX | 4 | 68758 | 13 |
| 54260315 | TRVRS PIPE GRT CON ES | FOOT | 57 | KNOX | 4 | 68758 | 13 |
| 54262718 | METAL FL END SEC 18" | EACH | 2 | KNOX | 4 | 68758 | 13 |
| 54262724 | METAL FL END SEC 24" | EACH | 4 | KNOX | 4 | 68758 | 13 |
| 58600101 | GRANULAR BACKFILL STR | CU YD | 70 | KNOX | 4 | 68758 | 13 |
| 59100100 | GEOCOMPOSITE WALL DR | SQ YD | 66 | KNOX | 4 | 68758 | 13 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 800 | KNOX | 4 | 68758 | 13 |
| 63100085 | TRAF BAR TERM T6 | EACH | 4 | KNOX | 4 | 68758 | 13 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 2 | KNOX | 4 | 68758 | 13 |
| 63200310 | GUARDRAIL REMOV | FOOT | 1237 | KNOX | 4 | 68758 | 13 |
| 66600105 | FUR ERECT ROW MARKERS | EACH | 12 | KNOX | 4 | 68758 | 13 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 8 | KNOX | 4 | 68758 | 13 |
| 67100100 | MOBILIZATION | L SUM | 1 | KNOX | 4 | 68758 | 13 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 182.5 | KNOX | 4 | 68758 | 13 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 60 | KNOX | 4 | 68758 | 13 |
| 72501000 | TERMINAL MARKER - DA | EACH | 2 | KNOX | 4 | 68758 | 13 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 4138 | KNOX | 4 | 68758 | 13 |
| 78001180 | PAINT PVT MK LINE 24 | FOOT | 12 | KNOX | 4 | 68758 | 13 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 16 | KNOX | 4 | 68758 | 13 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 9 | KNOX | 4 | 68758 | 13 |
| 78200010 | BARR WALL REF TYPE B | EACH | 4 | KNOX | 4 | 68758 | 13 |
| X0322936 | REMOV EX FLAR END SEC | EACH | 1 | LAWRENCE | 7 | 74894 | 23 |
| X4811900 | AGGREGATE SHLDS SPL | TON | 219 | LAWRENCE | 7 | 74894 | 23 |
| X6310088 | TRAF BAR TERM T6A SPL | EACH | 9 | LAWRENCE | 7 | 74894 | 23 |
| X6311217 | TRAF BAR TERM T6B SPL | EACH | 4 | LAWRENCE | 7 | 74894 | 23 |
| X6330725 | SPBGR (SHORT RADIUS) | FOOT | 25 | LAWRENCE | 7 | 74894 | 23 |
| Z0049790 | RELOC NAME PLATES | EACH | 1 | LAWRENCE | 7 | 74894 | 23 |
| 50800105 | REINFORCEMENT BARS | POUND | 142 | LAWRENCE | 7 | 74894 | 23 |
| 54001002 | BOX CUL END SEC C2 | EACH | 2 | LAWRENCE | 7 | 74894 | 23 |
| 54001006 | BOX CUL END SEC C6 | EACH | 2 | LAWRENCE | 7 | 74894 | 23 |
| 54002020 | EXPAN BOLTS 3/4 | EACH | 76 | LAWRENCE | 7 | 74894 | 23 |
| 54010503 | PCBC 5X3 | FOOT | 6 | LAWRENCE | 7 | 74894 | 23 |
| 54248510 | CONCRETE COLLAR | CU YD | 2 | LAWRENCE | 7 | 74894 | 23 |
| 550A0120 | STORM SEW CL A 1 24 | FOOT | 10 | LAWRENCE | 7 | 74894 | 23 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 6725 | LAWRENCE | 7 | 74894 | 23 |
| 63000003 | SPBGR TY A 9FT POSTS | FOOT | 3813 | LAWRENCE | 7 | 74894 | 23 |
| 63100045 | TRAF BAR TERM T2 | EACH | 4 | LAWRENCE | 7 | 74894 | 23 |
| 63100085 | TRAF BAR TERM T6 | EACH | 22 | LAWRENCE | 7 | 74894 | 23 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 60 | LAWRENCE | 7 | 74894 | 23 |
| 63100169 | TR BAR TRM T1 SPL FLR | EACH | 2 | LAWRENCE | 7 | 74894 | 23 |
| 63200310 | GUARDRAIL REMOV | FOOT | 16337 | LAWRENCE | 7 | 74894 | 23 |
| 67100100 | MOBILIZATION | L SUM | 1 | LAWRENCE | 7 | 74894 | 23 |
| 72501000 | TERMINAL MARKER - DA | EACH | 62 | LAWRENCE | 7 | 74894 | 23 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 186 | LAWRENCE | 7 | 74894 | 23 |
| X6330900 | VERT ADJ OF GUARDRAIL | FOOT | 25 | VARIOUS | 7 | 74918 | 24 |
| Z0012754 | STR REP CON DP = < 5 | SQ FT | 10 | VARIOUS | 7 | 74918 | 24 |
| 50102400 | CONC REM | CU YD | 2.3 | VARIOUS | 7 | 74918 | 24 |
| 50300255 | CONC SUP-STR | CU YD | 2.3 | VARIOUS | 7 | 74918 | 24 |
| 50300300 | PROTECTIVE COAT | SQ YD | 15.8 | VARIOUS | 7 | 74918 | 24 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 365 | VARIOUS | 7 | 74918 | 24 |
| 50800530 | MECHANICAL SPLICERS | EACH | 20 | VARIOUS | 7 | 74918 | 24 |
| 63100085 | TRAF BAR TERM T6 | EACH | 1 | VARIOUS | 7 | 74918 | 24 |
| 63200310 | GUARDRAIL REMOV | FOOT | 38 | VARIOUS | 7 | 74918 | 24 |
| 67100100 | MOBILIZATION | L SUM | 1 | VARIOUS | 7 | 74918 | 24 |
| 70100207 | TRAF CONT-PROT 701402 | EACH | 2 | VARIOUS | 7 | 74918 | 24 |
| 70102630 | TR CONT & PROT 701601 | L SUM | 1 | VARIOUS | 7 | 74918 | 24 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | VARIOUS | 7 | 74918 | 24 |
| 70107007 | PAVT MK BLKOUT TAPE 7 | FOOT | 1444 | VARIOUS | 7 | 74918 | 24 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 42 | VARIOUS | 7 | 74918 | 24 |
| 70400100 | TEMP CONC BARRIER | FOOT | 487.5 | VARIOUS | 7 | 74918 | 24 |
| 70600250 | IMP ATTN TEMP NRD TL3 | EACH | 2 | VARIOUS | 7 | 74918 | 24 |
| A2C021G3 | T-CARYA LACINIO CG 3G | EACH | 60 | SALINE | 9 | 78734 | 29 |
| A2C022G3 | T-CARYA ILLINOI CG 3G | EACH | 60 | SALINE | 9 | 78734 | 29 |
| A2C050G3 | T-QUERC BICOL CG 3G | EACH | 60 | SALINE | 9 | 78734 | 29 |
| A2C060G3 | T-QUERC PALUS CG 3G | EACH | 60 | SALINE | 9 | 78734 | 29 |
| A2C062G3 | T-QUERC SHUMARD CG 3G | EACH | 60 | SALINE | 9 | 78734 | 29 |
| K0029632 | WEED CONT N SEL/N RES | GALLON | 44 | SALINE | 9 | 78734 | 29 |
| X1200225 | STEEL PLATE WEIR | EACH | 2 | SALINE | 9 | 78734 | 29 |
| 67100100 | MOBILIZATION | L SUM | 1 | SALINE | 9 | 78734 | 29 |
| 72000100 | SIGN PANEL T1 | SQ FT | 56 | SALINE | 9 | 78734 | 29 |
| 72800100 | TELES STL SIN SUPPORT | FOOT | 336 | SALINE | 9 | 78734 | 29 |
| X0326887 | WOOD POLE 25 CL 4 | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| X0327294 | STORM SEWERS GROUTED | CU YD | 37 | LASALLE | 3 | 87703 | 38 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | LASALLE | 3 | 87703 | 38 |
| X7200105 | SIGN PANEL T1 SPL | SQ FT | 8 | LASALLE | 3 | 87703 | 38 |
| X8620200 | UNINTER POWER SUP SPL | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | LASALLE | 3 | 87703 | 38 |
| Z0032900 | LAND SECTION MARKERS | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 4003 | LASALLE | 3 | 87703 | 38 |
| Z0055500 | RUMBLE STRIP | SQ FT | 1650 | LASALLE | 3 | 87703 | 38 |
| 20200100 | EARTH EXCAVATION | CU YD | 1103 | LASALLE | 3 | 87703 | 38 |
| 20800150 | TRENCH BACKFILL | CU YD | 24 | LASALLE | 3 | 87703 | 38 |
| 21301060 | EXPLOR TRENCH 60 | FOOT | 200 | LASALLE | 3 | 87703 | 38 |
| 25000210 | SEEDING CL 2A | ACRE | 0.75 | LASALLE | 3 | 87703 | 38 |
| 25000400 | NITROGEN FERT NUTR | POUND | 64 | LASALLE | 3 | 87703 | 38 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 64 | LASALLE | 3 | 87703 | 38 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 64 | LASALLE | 3 | 87703 | 38 |
| 25100115 | MULCH METHOD 2 | ACRE | 1.5 | LASALLE | 3 | 87703 | 38 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 3115 | LASALLE | 3 | 87703 | 38 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 193 | LASALLE | 3 | 87703 | 38 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 102 | LASALLE | 3 | 87703 | 38 |
| 28000400 | PERIMETER EROS BAR | FOOT | 1556 | LASALLE | 3 | 87703 | 38 |
| 28000500 | INLET & PIPE PROTECT | EACH | 4 | LASALLE | 3 | 87703 | 38 |
| 31100910 | SUB GRAN MAT A 12 | SQ YD | 687 | LASALLE | 3 | 87703 | 38 |
| 35600702 | HMA BC WID 6 1/2 | SQ YD | 659 | LASALLE | 3 | 87703 | 38 |
| 40200500 | AGG SURF CSE A 6 | SQ YD | 156 | LASALLE | 3 | 87703 | 38 |
| 40600275 | BIT MATLS PR CT | POUND | 5260 | LASALLE | 3 | 87703 | 38 |
| 40600627 | LB MM IL-9.5FG N50 | TON | 592 | LASALLE | 3 | 87703 | 38 |
| 40600982 | HMA SURF REM BUTT JT | SQ YD | 666 | LASALLE | 3 | 87703 | 38 |
| 40603310 | HMA SC "C" N50 | TON | 959 | LASALLE | 3 | 87703 | 38 |
| 40800050 | INCIDENTAL HMA SURF | TON | 16 | LASALLE | 3 | 87703 | 38 |
| 42001300 | PROTECTIVE COAT | SQ YD | 36 | LASALLE | 3 | 87703 | 38 |
| 44201803 | CL D PATCH T2 13 | SQ YD | 45 | LASALLE | 3 | 87703 | 38 |
| 44201807 | CL D PATCH T3 13 | SQ YD | 34 | LASALLE | 3 | 87703 | 38 |
| 48101200 | AGGREGATE SHLDS B | TON | 365 | LASALLE | 3 | 87703 | 38 |
| 48203021 | HMA SHOULDERS 6 | SQ YD | 627 | LASALLE | 3 | 87703 | 38 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 24 | LASALLE | 3 | 87703 | 38 |
| 54001001 | BOX CUL END SEC C1 | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 54010602 | PCBC 6X2 | FOOT | 48 | LASALLE | 3 | 87703 | 38 |
| 542A0223 | P CUL CL A 1 18 | FOOT | 54 | LASALLE | 3 | 87703 | 38 |
| 542A0229 | P CUL CL A 1 24 | FOOT | 50 | LASALLE | 3 | 87703 | 38 |
| 542D0220 | P CUL CL D 1 15 | FOOT | 34 | LASALLE | 3 | 87703 | 38 |
| 54213663 | PRC FLAR END SEC 18 | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 54213669 | PRC FLAR END SEC 24 | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 54262715 | METAL FL END SEC 15" | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 60100935 | PIPE DRAINS 10 | FOOT | 96 | LASALLE | 3 | 87703 | 38 |
| 60260400 | INLETS ADJ NEW T1F CL | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| 60622800 | CONC MED TSM6.12 | SQ FT | 316 | LASALLE | 3 | 87703 | 38 |
| 61133100 | FLD TILE JUN VAULT 2D | EACH | 4 | LASALLE | 3 | 87703 | 38 |
| 66600105 | FUR ERECT ROW MARKERS | EACH | 8 | LASALLE | 3 | 87703 | 38 |
| 67100100 | MOBILIZATION | L SUM | 1 | LASALLE | 3 | 87703 | 38 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 506 | LASALLE | 3 | 87703 | 38 |
| 72000100 | SIGN PANEL T1 | SQ FT | 116 | LASALLE | 3 | 87703 | 38 |
| 73000100 | WOOD SIN SUPPORT | FOOT | 220 | LASALLE | 3 | 87703 | 38 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 14491 | LASALLE | 3 | 87703 | 38 |
| 78001150 | PAINT PVT MK LINE 12 | FOOT | 35 | LASALLE | 3 | 87703 | 38 |
| 78004280 | PREF PL PM TB INL L24 | FOOT | 36 | LASALLE | 3 | 87703 | 38 |
| 78200020 | CURB REFLECTORS | EACH | 34 | LASALLE | 3 | 87703 | 38 |
| 80500100 | SERV INSTALL TY A | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| 81028190 | UNDRGRD C GALVS 1 1/2 | FOOT | 98 | LASALLE | 3 | 87703 | 38 |
| 81028200 | UNDRGRD C GALVS 2 | FOOT | 95 | LASALLE | 3 | 87703 | 38 |
| 81028220 | UNDRGRD C GALVS 3 | FOOT | 132 | LASALLE | 3 | 87703 | 38 |
| 81028350 | UNDRGRD C PVC 2 | FOOT | 1307 | LASALLE | 3 | 87703 | 38 |
| 81028390 | UNDRGRD C PVC 4 | FOOT | 44 | LASALLE | 3 | 87703 | 38 |
| 81100500 | CON AT ST 1 1/2 GALVS | FOOT | 144 | LASALLE | 3 | 87703 | 38 |
| 81400700 | HANDHOLE PCC | EACH | 12 | LASALLE | 3 | 87703 | 38 |
| 81400710 | HD HANDHOLE PCC | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 81603010 | UD 2#10#10GXLPUSE 3/4 | FOOT | 474 | LASALLE | 3 | 87703 | 38 |
| 82110005 | LUM LED RDWY E | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 82500310 | LT CONT PM 240V 60 | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| 83000600 | LT P A 30MH 15DA | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 83600300 | LIGHT POLE FDN 30D | FOOT | 26 | LASALLE | 3 | 87703 | 38 |
| 83800205 | BKWY DEV TR B 15BC | EACH | 2 | LASALLE | 3 | 87703 | 38 |
| 85800100 | FL CONT | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| 87301225 | ELCBL C SIGNAL 14 3C | FOOT | 4291 | LASALLE | 3 | 87703 | 38 |
| 87301805 | ELCBL C SERV 6 2C | FOOT | 15 | LASALLE | 3 | 87703 | 38 |
| 87301900 | ELCBL C EGRDC 6 1C | FOOT | 1900 | LASALLE | 3 | 87703 | 38 |
| 88040030 | SH P LED 1F 1S PM | EACH | 8 | LASALLE | 3 | 87703 | 38 |
| 89502400 | REM EX FB INSTAL COMP | EACH | 1 | LASALLE | 3 | 87703 | 38 |
| K1005421 | SEEDING SPL | ACRE | 6 | VERMILION | 5 | 91581 | 30 |
| XX000882 | WOOD FENCE | FOOT | 1149 | VERMILION | 5 | 91581 | 30 |
| XX002007 | AGG BICYCLE PATH | SQ YD | 7101 | VERMILION | 5 | 91581 | 30 |
| X0322135 | BOLLARD QUICK RELEASE | EACH | 3 | VERMILION | 5 | 91581 | 30 |
| X0322508 | PED TRUSS SUPERSTR | SQ FT | 12864 | VERMILION | 5 | 91581 | 30 |
| X0327009 | REMOVE SIGN SPECIAL | EACH | 5 | VERMILION | 5 | 91581 | 30 |
| X0327395 | ID DISP EXIST RR TIES | L SUM | 1 | VERMILION | 5 | 91581 | 30 |
| X5537900 | SS CLEANED 15 | FOOT | 50 | VERMILION | 5 | 91581 | 30 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | VERMILION | 5 | 91581 | 30 |
| Z0012754 | STR REP CON DP = < 5 | SQ FT | 200 | VERMILION | 5 | 91581 | 30 |
| Z0012755 | STR REP CON DP OVER 5 | SQ FT | 200 | VERMILION | 5 | 91581 | 30 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | VERMILION | 5 | 91581 | 30 |
| Z0076600 | TRAINEES | HOUR | 1000 | VERMILION | 5 | 91581 | 30 |
| Z0076604 | TRAINEES TPG | HOUR | 1000 | VERMILION | 5 | 91581 | 30 |
| Z0078002 | WOOD RAIL SPL | FOOT | 96 | VERMILION | 5 | 91581 | 30 |
| 20100500 | TREE REMOV ACRES | ACRE | 2.75 | VERMILION | 5 | 91581 | 30 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 2802 | VERMILION | 5 | 91581 | 30 |
| 21101610 | TOPSOIL F & P 3 | SQ YD | 13381 | VERMILION | 5 | 91581 | 30 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 11048 | VERMILION | 5 | 91581 | 30 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 242 | VERMILION | 5 | 91581 | 30 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 42 | VERMILION | 5 | 91581 | 30 |
| 28000400 | PERIMETER EROS BAR | FOOT | 3049 | VERMILION | 5 | 91581 | 30 |
| 28000500 | INLET & PIPE PROTECT | EACH | 4 | VERMILION | 5 | 91581 | 30 |
| 28100107 | STONE RIPRAP CL A4 | SQ YD | 11 | VERMILION | 5 | 91581 | 30 |
| 28200200 | FILTER FABRIC | SQ YD | 11 | VERMILION | 5 | 91581 | 30 |
| 35100500 | AGG BASE CSE A 6 | SQ YD | 200 | VERMILION | 5 | 91581 | 30 |
| 35102100 | AGG BASE CSE B 9 | SQ YD | 7101 | VERMILION | 5 | 91581 | 30 |
| 40600275 | BIT MATLS PR CT | POUND | 450 | VERMILION | 5 | 91581 | 30 |
| 40600290 | BIT MATLS TACK CT | POUND | 45 | VERMILION | 5 | 91581 | 30 |
| 40603310 | HMA SC "C" N50 | TON | 34 | VERMILION | 5 | 91581 | 30 |
| 42400300 | PC CONC SIDEWALK 6 | SQ FT | 150 | VERMILION | 5 | 91581 | 30 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 54 | VERMILION | 5 | 91581 | 30 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 220 | VERMILION | 5 | 91581 | 30 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 65 | VERMILION | 5 | 91581 | 30 |
| 50300225 | CONC STRUCT | CU YD | 8.5 | VERMILION | 5 | 91581 | 30 |
| 50300255 | CONC SUP-STR | CU YD | 14.9 | VERMILION | 5 | 91581 | 30 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 3220 | VERMILION | 5 | 91581 | 30 |
| 542D0220 | P CUL CL D 1 15 | FOOT | 70 | VERMILION | 5 | 91581 | 30 |
| 542D0223 | P CUL CL D 1 18 | FOOT | 102 | VERMILION | 5 | 91581 | 30 |
| 54213450 | END SECTIONS 15 | EACH | 1 | VERMILION | 5 | 91581 | 30 |
| 54213453 | END SECTIONS 18 | EACH | 4 | VERMILION | 5 | 91581 | 30 |
| 66300105 | CALCIUM CHLORIDE APLD | TON | 4.3 | VERMILION | 5 | 91581 | 30 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 935 | VERMILION | 5 | 91581 | 30 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 1 | VERMILION | 5 | 91581 | 30 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | VERMILION | 5 | 91581 | 30 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 2 | VERMILION | 5 | 91581 | 30 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | VERMILION | 5 | 91581 | 30 |
| 67100100 | MOBILIZATION | L SUM | 1 | VERMILION | 5 | 91581 | 30 |
| 72000100 | SIGN PANEL T1 | SQ FT | 59 | VERMILION | 5 | 91581 | 30 |
| 72900100 | METAL POST TY A | FOOT | 150 | VERMILION | 5 | 91581 | 30 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 42 | VERMILION | 5 | 91581 | 30 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 80 | VERMILION | 5 | 91581 | 30 |
| B2001166 | T-CERCIS CAN CL 6' | EACH | 27 | SANGAMON | 6 | 93719 | 31 |
| D2000148 | E-ABIES CONCOLOR 4' | EACH | 17 | SANGAMON | 6 | 93719 | 31 |
| X0322936 | REMOV EX FLAR END SEC | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| X0322939 | RELOC EX FLAR END SEC | EACH | 3 | SANGAMON | 6 | 93719 | 31 |
| X0323265 | REMOVE EXIST RIPRAP | SQ YD | 114 | SANGAMON | 6 | 93719 | 31 |
| X0323389 | STORM SEW CONNECTION | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| X0325402 | MODIFY SPRINKLER SYST | L SUM | 1 | SANGAMON | 6 | 93719 | 31 |
| X0325528 | REM REINST LGTG EQPT | L SUM | 1 | SANGAMON | 6 | 93719 | 31 |
| X0325714 | FL BEACON P MTD SP IN | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 3478 | SANGAMON | 6 | 93719 | 31 |
| X6026050 | SANITARY MANHOLE ADJ | EACH | 8 | SANGAMON | 6 | 93719 | 31 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | SANGAMON | 6 | 93719 | 31 |
| X7030005 | TEMP PAVT MKING REMOV | SQ FT | 11732 | SANGAMON | 6 | 93719 | 31 |
| X7200105 | SIGN PANEL T1 SPL | SQ FT | 13 | SANGAMON | 6 | 93719 | 31 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | SANGAMON | 6 | 93719 | 31 |
| Z0016702 | DETOUR SIGNING | L SUM | 1 | SANGAMON | 6 | 93719 | 31 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 19256 | SANGAMON | 6 | 93719 | 31 |
| Z0054404 | ROCK FILL - EMBANK | CU YD | 300 | SANGAMON | 6 | 93719 | 31 |
| Z0056608 | STORM SEW WM REQ 12 | FOOT | 315 | SANGAMON | 6 | 93719 | 31 |
| Z0056610 | STORM SEW WM REQ 15 | FOOT | 208 | SANGAMON | 6 | 93719 | 31 |
| Z0056612 | STORM SEW WM REQ 18 | FOOT | 548 | SANGAMON | 6 | 93719 | 31 |
| Z0056618 | STORM SEW WM REQ 27 | FOOT | 178 | SANGAMON | 6 | 93719 | 31 |
| Z0076600 | TRAINEES | HOUR | 2000 | SANGAMON | 6 | 93719 | 31 |
| Z0076604 | TRAINEES TPG | HOUR | 2000 | SANGAMON | 6 | 93719 | 31 |
| Z0076870 | UNDR CONNECT TO STR | EACH | 5 | SANGAMON | 6 | 93719 | 31 |
| 20100110 | TREE REMOV 6-15 | UNIT | 353 | SANGAMON | 6 | 93719 | 31 |
| 20100210 | TREE REMOV OVER 15 | UNIT | 180 | SANGAMON | 6 | 93719 | 31 |
| 20101100 | TREE TRUNK PROTECTION | EACH | 59 | SANGAMON | 6 | 93719 | 31 |
| 20101300 | TREE PRUN 1-10 | EACH | 17 | SANGAMON | 6 | 93719 | 31 |
| 20101350 | TREE PRUN OVER 10 | EACH | 49 | SANGAMON | 6 | 93719 | 31 |
| 20101700 | SUPPLE WATERING | UNIT | 131 | SANGAMON | 6 | 93719 | 31 |
| 20200100 | EARTH EXCAVATION | CU YD | 17909 | SANGAMON | 6 | 93719 | 31 |
| 20201200 | REM & DISP UNS MATL | CU YD | 300 | SANGAMON | 6 | 93719 | 31 |
| 20800150 | TRENCH BACKFILL | CU YD | 1286 | SANGAMON | 6 | 93719 | 31 |
| 21001000 | GEOTECH FAB F/GR STAB | SQ YD | 600 | SANGAMON | 6 | 93719 | 31 |
| 21101505 | TOPSOIL EXC & PLAC | CU YD | 2946 | SANGAMON | 6 | 93719 | 31 |
| 25000200 | SEEDING CL 2 | ACRE | 4.75 | SANGAMON | 6 | 93719 | 31 |
| 25000400 | NITROGEN FERT NUTR | POUND | 431 | SANGAMON | 6 | 93719 | 31 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 431 | SANGAMON | 6 | 93719 | 31 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 431 | SANGAMON | 6 | 93719 | 31 |
| 25000700 | AGR GROUND LIMESTONE | TON | 9.5 | SANGAMON | 6 | 93719 | 31 |
| 25100125 | MULCH METHOD 3 | ACRE | 4.75 | SANGAMON | 6 | 93719 | 31 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 2600 | SANGAMON | 6 | 93719 | 31 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 475 | SANGAMON | 6 | 93719 | 31 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 264 | SANGAMON | 6 | 93719 | 31 |
| 28000400 | PERIMETER EROS BAR | FOOT | 4499 | SANGAMON | 6 | 93719 | 31 |
| 28000500 | INLET & PIPE PROTECT | EACH | 9 | SANGAMON | 6 | 93719 | 31 |
| 28000510 | INLET FILTERS | EACH | 59 | SANGAMON | 6 | 93719 | 31 |
| 28100103 | STONE RIPRAP CL A2 | SQ YD | 50 | SANGAMON | 6 | 93719 | 31 |
| 28100105 | STONE RIPRAP CL A3 | SQ YD | 24 | SANGAMON | 6 | 93719 | 31 |
| 28100107 | STONE RIPRAP CL A4 | SQ YD | 121 | SANGAMON | 6 | 93719 | 31 |
| 28200200 | FILTER FABRIC | SQ YD | 121 | SANGAMON | 6 | 93719 | 31 |
| 31100910 | SUB GRAN MAT A 12 | SQ YD | 27395 | SANGAMON | 6 | 93719 | 31 |
| 40201000 | AGGREGATE-TEMP ACCESS | TON | 636 | SANGAMON | 6 | 93719 | 31 |
| 40600275 | BIT MATLS PR CT | POUND | 55578 | SANGAMON | 6 | 93719 | 31 |
| 40600290 | BIT MATLS TACK CT | POUND | 11118 | SANGAMON | 6 | 93719 | 31 |
| 40600990 | TEMPORARY RAMP | SQ YD | 157 | SANGAMON | 6 | 93719 | 31 |
| 40701881 | HMA PAVT FD 10 | SQ YD | 24619 | SANGAMON | 6 | 93719 | 31 |
| 42300200 | PCC DRIVEWAY PAVT 6 | SQ YD | 69 | SANGAMON | 6 | 93719 | 31 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 46722 | SANGAMON | 6 | 93719 | 31 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 220 | SANGAMON | 6 | 93719 | 31 |
| 44000100 | PAVEMENT REM | SQ YD | 3016 | SANGAMON | 6 | 93719 | 31 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 550 | SANGAMON | 6 | 93719 | 31 |
| 44000600 | SIDEWALK REM | SQ FT | 604 | SANGAMON | 6 | 93719 | 31 |
| 48203021 | HMA SHOULDERS 6 | SQ YD | 269 | SANGAMON | 6 | 93719 | 31 |
| 50104400 | CONC HDWL REM | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 366 | SANGAMON | 6 | 93719 | 31 |
| 54213660 | PRC FLAR END SEC 15 | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| 54213672 | PRC FLAR END SEC 27 | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 54213699 | PRC FLAR END SEC 54 | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 54214719 | PRCF END S EL EQRS 24 | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| 54214731 | PRCF END S EL EQRS 36 | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 54248510 | CONCRETE COLLAR | CU YD | 1.2 | SANGAMON | 6 | 93719 | 31 |
| 550A0050 | STORM SEW CL A 1 12 | FOOT | 1609 | SANGAMON | 6 | 93719 | 31 |
| 550A0070 | STORM SEW CL A 1 15 | FOOT | 506 | SANGAMON | 6 | 93719 | 31 |
| 550A0090 | STORM SEW CL A 1 18 | FOOT | 609 | SANGAMON | 6 | 93719 | 31 |
| 550A0120 | STORM SEW CL A 1 24 | FOOT | 10 | SANGAMON | 6 | 93719 | 31 |
| 550A0130 | STORM SEW CL A 1 27 | FOOT | 21 | SANGAMON | 6 | 93719 | 31 |
| 550A0140 | STORM SEW CL A 1 30 | FOOT | 43 | SANGAMON | 6 | 93719 | 31 |
| 550A0200 | STORM SEW CL A 1 54 | FOOT | 23 | SANGAMON | 6 | 93719 | 31 |
| 550A0360 | STORM SEW CL A 2 15 | FOOT | 32 | SANGAMON | 6 | 93719 | 31 |
| 550A0380 | STORM SEW CL A 2 18 | FOOT | 484 | SANGAMON | 6 | 93719 | 31 |
| 550A0430 | STORM SEW CL A 2 30 | FOOT | 11 | SANGAMON | 6 | 93719 | 31 |
| 550A4000 | SS CL A 1 EQRS 18 | FOOT | 19 | SANGAMON | 6 | 93719 | 31 |
| 550A4100 | SS CL A 1 EQRS 24 | FOOT | 887 | SANGAMON | 6 | 93719 | 31 |
| 550A4200 | SS CL A 1 EQRS 27 | FOOT | 228 | SANGAMON | 6 | 93719 | 31 |
| 550A4500 | SS CL A 1 EQRS 36 | FOOT | 14 | SANGAMON | 6 | 93719 | 31 |
| 55100500 | STORM SEWER REM 12 | FOOT | 11 | SANGAMON | 6 | 93719 | 31 |
| 59300100 | CONTR LOW-STRENG MATL | CU YD | 25 | SANGAMON | 6 | 93719 | 31 |
| 60108100 | PIPE UNDERDRAIN 4 SP | FOOT | 250 | SANGAMON | 6 | 93719 | 31 |
| 60108200 | PIPE UNDERDRAIN 6 SP | FOOT | 250 | SANGAMON | 6 | 93719 | 31 |
| 60218400 | MAN TA 4 DIA T1F CL | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| 60218500 | MAN TA 4 DIA T3F&G | EACH | 14 | SANGAMON | 6 | 93719 | 31 |
| 60221100 | MAN TA 5 DIA T1F CL | EACH | 3 | SANGAMON | 6 | 93719 | 31 |
| 60221200 | MAN TA 5 DIA T3F&G | EACH | 5 | SANGAMON | 6 | 93719 | 31 |
| 60223800 | MAN TA 6 DIA T1F CL | EACH | 6 | SANGAMON | 6 | 93719 | 31 |
| 60223810 | MAN TA 6 DIA T3F&G | EACH | 3 | SANGAMON | 6 | 93719 | 31 |
| 60224447 | MAN TA 7 DIA T3F&G | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 60224459 | MAN TA 8 DIA T1F CL | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 60235700 | INLETS TA T3F&G | EACH | 23 | SANGAMON | 6 | 93719 | 31 |
| 60236200 | INLETS TA T8G | EACH | 2 | SANGAMON | 6 | 93719 | 31 |
| 60240220 | INLETS TB T3F&G | EACH | 10 | SANGAMON | 6 | 93719 | 31 |
| 60255500 | MAN ADJUST | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 60266600 | VALVE BOX ADJ | EACH | 16 | SANGAMON | 6 | 93719 | 31 |
| 60500060 | REMOV INLETS | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 60604400 | COMB CC&G TB6.18 | FOOT | 9079 | SANGAMON | 6 | 93719 | 31 |
| 61100500 | EXPLOR TRENCH 52 | FOOT | 500 | SANGAMON | 6 | 93719 | 31 |
| 61100605 | MISC CONCRETE | CU YD | 4 | SANGAMON | 6 | 93719 | 31 |
| 61101007 | STORM SEW PROT A 6 | FOOT | 50 | SANGAMON | 6 | 93719 | 31 |
| 61101009 | STORM SEW PROT A 8 | FOOT | 50 | SANGAMON | 6 | 93719 | 31 |
| 61139900 | STORM SEWER SPEC 6 | FOOT | 50 | SANGAMON | 6 | 93719 | 31 |
| 61140000 | STORM SEWER SPEC 8 | FOOT | 50 | SANGAMON | 6 | 93719 | 31 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 350 | SANGAMON | 6 | 93719 | 31 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 1 | SANGAMON | 6 | 93719 | 31 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | SANGAMON | 6 | 93719 | 31 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 5 | SANGAMON | 6 | 93719 | 31 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | SANGAMON | 6 | 93719 | 31 |
| 67100100 | MOBILIZATION | L SUM | 1 | SANGAMON | 6 | 93719 | 31 |
| 70300210 | TEMP PVT MK LTR & SYM | SQ FT | 1110 | SANGAMON | 6 | 93719 | 31 |
| 70300230 | TEMP PVT MK LINE 5 | FOOT | 22472 | SANGAMON | 6 | 93719 | 31 |
| 70300240 | TEMP PVT MK LINE 6 | FOOT | 985 | SANGAMON | 6 | 93719 | 31 |
| 70300250 | TEMP PVT MK LINE 8 | FOOT | 628 | SANGAMON | 6 | 93719 | 31 |
| 70300260 | TEMP PVT MK LINE 12 | FOOT | 227 | SANGAMON | 6 | 93719 | 31 |
| 70300280 | TEMP PVT MK LINE 24 | FOOT | 140 | SANGAMON | 6 | 93719 | 31 |
| 72000100 | SIGN PANEL T1 | SQ FT | 30 | SANGAMON | 6 | 93719 | 31 |
| 72400500 | RELOC SIN PAN ASSY TA | EACH | 16 | SANGAMON | 6 | 93719 | 31 |
| 72400710 | RELOC SIGN PANEL T1 | SQ FT | 9 | SANGAMON | 6 | 93719 | 31 |
| 72800100 | TELES STL SIN SUPPORT | FOOT | 61 | SANGAMON | 6 | 93719 | 31 |
| 78000300 | THPL PVT MK LINE 5 | FOOT | 22472 | SANGAMON | 6 | 93719 | 31 |
| 78000400 | THPL PVT MK LINE 6 | FOOT | 985 | SANGAMON | 6 | 93719 | 31 |
| 78000500 | THPL PVT MK LINE 8 | FOOT | 628 | SANGAMON | 6 | 93719 | 31 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 227 | SANGAMON | 6 | 93719 | 31 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 140 | SANGAMON | 6 | 93719 | 31 |
| 78008200 | POLYUREA PM T1 LTR-SY | SQ FT | 1110 | SANGAMON | 6 | 93719 | 31 |
| X2501000 | SEEDING CL 2 SPL | ACRE | 1.2 | HANCOCK | 6 | 93731 | 39 |
| X2830495 | AGGREGATE DITCH SPL | TON | 141 | HANCOCK | 6 | 93731 | 39 |
| X5021510 | COFFERDAMS SPL | EACH | 2 | HANCOCK | 6 | 93731 | 39 |
| X7011800 | TRAF CONT-PROT BLR 21 | L SUM | 1 | HANCOCK | 6 | 93731 | 39 |
| Z0065000 | SET PILES IN ROCK | EACH | 12 | HANCOCK | 6 | 93731 | 39 |
| Z0076600 | TRAINEES | HOUR | 500 | HANCOCK | 6 | 93731 | 39 |
| Z0076604 | TRAINEES TPG | HOUR | 500 | HANCOCK | 6 | 93731 | 39 |
| 20100500 | TREE REMOV ACRES | ACRE | 1.3 | HANCOCK | 6 | 93731 | 39 |
| 20200100 | EARTH EXCAVATION | CU YD | 899 | HANCOCK | 6 | 93731 | 39 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 1500 | HANCOCK | 6 | 93731 | 39 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 6456 | HANCOCK | 6 | 93731 | 39 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 147 | HANCOCK | 6 | 93731 | 39 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 140 | HANCOCK | 6 | 93731 | 39 |
| 28000400 | PERIMETER EROS BAR | FOOT | 1823 | HANCOCK | 6 | 93731 | 39 |
| 28100207 | STONE RIPRAP CL A4 | TON | 758 | HANCOCK | 6 | 93731 | 39 |
| 28200200 | FILTER FABRIC | SQ YD | 1094 | HANCOCK | 6 | 93731 | 39 |
| 40200800 | AGG SURF CSE B | TON | 675 | HANCOCK | 6 | 93731 | 39 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | HANCOCK | 6 | 93731 | 39 |
| 50300225 | CONC STRUCT | CU YD | 156.8 | HANCOCK | 6 | 93731 | 39 |
| 50300280 | CONCRETE ENCASEMENT | CU YD | 2.8 | HANCOCK | 6 | 93731 | 39 |
| 50400505 | P P CONC DK BM 27 DP | SQ FT | 4860 | HANCOCK | 6 | 93731 | 39 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 16640 | HANCOCK | 6 | 93731 | 39 |
| 50900205 | STEEL RAILING TY S1 | FOOT | 360 | HANCOCK | 6 | 93731 | 39 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 678 | HANCOCK | 6 | 93731 | 39 |
| 51202305 | DRIVING PILES | FOOT | 222 | HANCOCK | 6 | 93731 | 39 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 1 | HANCOCK | 6 | 93731 | 39 |
| 51500100 | NAME PLATES | EACH | 1 | HANCOCK | 6 | 93731 | 39 |
| 63100075 | TRAF BAR TERM T5A | EACH | 2 | HANCOCK | 6 | 93731 | 39 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 2 | HANCOCK | 6 | 93731 | 39 |
| 67100100 | MOBILIZATION | L SUM | 1 | HANCOCK | 6 | 93731 | 39 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | HANCOCK | 6 | 93731 | 39 |
| XX008948 | F&E STRUCT STEEL BR 1 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| XX008949 | F&E STRUCT STEEL BR 2 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| XX008952 | LUM DEC LIGHT TAPE | FOOT | 581 | SANGAMON | 6 | 93733 | 40 |
| XX009183 | F&E STRUCT STEEL BR 3 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| XX009184 | F&E STRUCT STEEL BR 4 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| XX009316 | SEWER METAL LINER 48 | FOOT | 70 | SANGAMON | 6 | 93733 | 40 |
| XZ127900 | RETAINING WALL REMOV | FOOT | 3 | SANGAMON | 6 | 93733 | 40 |
| X0320000 | DRAINAGE SYSTEM, N1 | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X0320002 | DRAINAGE SYSTEM, N2 | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X0320008 | DRAINAGE SYSTEM, N3 | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X0320009 | DRAINAGE SYSTEM, N4 | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X0320051 | CROS SONIC LOG A DUCT | FOOT | 5274 | SANGAMON | 6 | 93733 | 40 |
| X0322924 | RETAINING WALL REMOV | SQ FT | 406 | SANGAMON | 6 | 93733 | 40 |
| X0323099 | RETAINING WALL REMOV | CU YD | 13.2 | SANGAMON | 6 | 93733 | 40 |
| X0324752 | STORM SEWER FILLED | CU YD | 120 | SANGAMON | 6 | 93733 | 40 |
| X0326671 | CONC SURF COLOR TRMNT | SQ FT | 1110 | SANGAMON | 6 | 93733 | 40 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 288 | SANGAMON | 6 | 93733 | 40 |
| X1200075 | GRATING-C FL END S 18 | EACH | 4 | SANGAMON | 6 | 93733 | 40 |
| X1200107 | PIPE UNDERDRAIN 6 MOD | FOOT | 949 | SANGAMON | 6 | 93733 | 40 |
| X1400238 | LUMINAIRE LED SPECIAL | EACH | 24 | SANGAMON | 6 | 93733 | 40 |
| X2200018 | ORNAMENTAL FENCE | FOOT | 812 | SANGAMON | 6 | 93733 | 40 |
| X5800110 | MEMBRANE WATERPRF SPL | SQ FT | 24368 | SANGAMON | 6 | 93733 | 40 |
| X6012108 | PIPE DRAINS 18 SPL | FOOT | 585 | SANGAMON | 6 | 93733 | 40 |
| X6020084 | MANHOLE SPECIAL | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X6020101 | MAN TA 9 DIA T1F CL S | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X6024240 | INLETS SPL | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| X6640300 | CH LK FENCE REMOV | FOOT | 750 | SANGAMON | 6 | 93733 | 40 |
| X6640308 | CH LK GATES SPL | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| X6640570 | CH LK FENCE 8 SPL | FOOT | 245 | SANGAMON | 6 | 93733 | 40 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| X7030005 | TEMP PAVT MKING REMOV | SQ FT | 1555 | SANGAMON | 6 | 93733 | 40 |
| X8211000 | UNDERPASS LUM (SP) | EACH | 24 | SANGAMON | 6 | 93733 | 40 |
| Z0002300 | BALLAST | CU YD | 201 | SANGAMON | 6 | 93733 | 40 |
| Z0007124 | STEEL RAILING SPL | FOOT | 882 | SANGAMON | 6 | 93733 | 40 |
| Z0007601 | BLDG REMOV NO 1 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007602 | BLDG REMOV NO 2 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007603 | BLDG REMOV NO 3 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007604 | BLDG REMOV NO 4 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007605 | BLDG REMOV NO 5 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007606 | BLDG REMOV NO 6 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007607 | BLDG REMOV NO 7 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007608 | BLDG REMOV NO 8 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007609 | BLDG REMOV NO 9 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007610 | BLDG REMOV NO 10 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007611 | BLDG REMOV NO 11 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007612 | BLDG REMOV NO 12 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007613 | BLDG REMOV NO 13 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007614 | BLDG REMOV NO 14 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007615 | BLDG REMOV NO 15 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007616 | BLDG REMOV NO 16 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007617 | BLDG REMOV NO 17 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007618 | BLDG REMOV NO 18 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007619 | BLDG REMOV NO 19 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007620 | BLDG REMOV NO 20 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007621 | BLDG REMOV NO 21 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007622 | BLDG REMOV NO 22 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007623 | BLDG REMOV NO 23 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007624 | BLDG REMOV NO 24 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007625 | BLDG REMOV NO 25 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0007626 | BLDG REMOV NO 26 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0012455 | CONC STEP REMOV | EACH | 13 | SANGAMON | 6 | 93733 | 40 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0016702 | DETOUR SIGNING | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0022800 | FENCE REMOVAL | FOOT | 2736 | SANGAMON | 6 | 93733 | 40 |
| Z0046304 | P UNDR FOR STRUCT 4 | FOOT | 1220 | SANGAMON | 6 | 93733 | 40 |
| Z0046306 | P UNDR FOR STRUCT 6 | FOOT | 713 | SANGAMON | 6 | 93733 | 40 |
| Z0048665 | RR PROT LIABILITY INS | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049801 | R&D FRIABL ASB BLD 1 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049802 | R&D FRIABL ASB BLD 2 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049803 | R&D FRIABL ASB BLD 3 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049806 | R&D FRIABL ASB BLD 6 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049808 | R&D FRIABL ASB BLD 8 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049809 | R&D FRIABL ASB BLD 9 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049811 | R&D FRIABL ASB BLD 11 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049813 | R&D FRIABL ASB BLD 13 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049815 | R&D FRIABL ASB BLD 15 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049816 | R&D FRIABL ASB BLD 16 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049818 | R&D FRIABL ASB BLD 18 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049824 | R&D FRIABL ASB BLD 24 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049826 | R&D FRIABL ASB BLD 26 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049901 | R&D NON-FR ASB BLD 1 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049905 | R&D NON-FR ASB BLD 5 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049906 | R&D NON-FR ASB BLD 6 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049908 | R&D NON-FR ASB BLD 8 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049913 | R&D NON-FR ASB BLD 13 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049916 | R&D NON-FR ASB BLD 16 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049918 | R&D NON-FR ASB BLD 18 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049921 | R&D NON-FR ASB BLD 21 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0049926 | R&D NON-FR ASB BLD 26 | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| Z0056648 | SS 1 WAT MN 12 | FOOT | 23 | SANGAMON | 6 | 93733 | 40 |
| Z0057100 | SAN SEW 12 | FOOT | 38 | SANGAMON | 6 | 93733 | 40 |
| Z0058000 | SAN SEW SPL | FOOT | 67 | SANGAMON | 6 | 93733 | 40 |
| Z0069700 | SUB-BALLAST | CU YD | 14173 | SANGAMON | 6 | 93733 | 40 |
| Z0076100 | TRACK REMOVAL | FOOT | 3910 | SANGAMON | 6 | 93733 | 40 |
| Z0076600 | TRAINEES | HOUR | 5000 | SANGAMON | 6 | 93733 | 40 |
| Z0076604 | TRAINEES TPG | HOUR | 5000 | SANGAMON | 6 | 93733 | 40 |
| 20100500 | TREE REMOV ACRES | ACRE | 14.75 | SANGAMON | 6 | 93733 | 40 |
| 20200100 | EARTH EXCAVATION | CU YD | 10330 | SANGAMON | 6 | 93733 | 40 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 49900 | SANGAMON | 6 | 93733 | 40 |
| 20700220 | POROUS GRAN EMBANK | CU YD | 3062 | SANGAMON | 6 | 93733 | 40 |
| 20800150 | TRENCH BACKFILL | CU YD | 776 | SANGAMON | 6 | 93733 | 40 |
| 20900110 | POROUS GRAN BACKFILL | CU YD | 113 | SANGAMON | 6 | 93733 | 40 |
| 25000110 | SEEDING CL 1A | ACRE | 9.75 | SANGAMON | 6 | 93733 | 40 |
| 25000400 | NITROGEN FERT NUTR | POUND | 882 | SANGAMON | 6 | 93733 | 40 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 882 | SANGAMON | 6 | 93733 | 40 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 882 | SANGAMON | 6 | 93733 | 40 |
| 25000700 | AGR GROUND LIMESTONE | TON | 19.6 | SANGAMON | 6 | 93733 | 40 |
| 25100115 | MULCH METHOD 2 | ACRE | 4.5 | SANGAMON | 6 | 93733 | 40 |
| 25100125 | MULCH METHOD 3 | ACRE | 2.75 | SANGAMON | 6 | 93733 | 40 |
| 25100635 | HD EROS CONTR BLANKET | SQ YD | 11479 | SANGAMON | 6 | 93733 | 40 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 975 | SANGAMON | 6 | 93733 | 40 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 207 | SANGAMON | 6 | 93733 | 40 |
| 28000400 | PERIMETER EROS BAR | FOOT | 2572 | SANGAMON | 6 | 93733 | 40 |
| 28000500 | INLET & PIPE PROTECT | EACH | 34 | SANGAMON | 6 | 93733 | 40 |
| 28001200 | TEMP HD EROS CONTR BL | SQ YD | 2255 | SANGAMON | 6 | 93733 | 40 |
| 31101200 | SUB GRAN MAT B 4 | SQ YD | 383 | SANGAMON | 6 | 93733 | 40 |
| 35101100 | AGG BASE CSE A 12 | SQ YD | 1250 | SANGAMON | 6 | 93733 | 40 |
| 40600275 | BIT MATLS PR CT | POUND | 2463 | SANGAMON | 6 | 93733 | 40 |
| 40600290 | BIT MATLS TACK CT | POUND | 1353 | SANGAMON | 6 | 93733 | 40 |
| 40600982 | HMA SURF REM BUTT JT | SQ YD | 173 | SANGAMON | 6 | 93733 | 40 |
| 40603080 | HMA BC IL-19.0 N50 | TON | 103 | SANGAMON | 6 | 93733 | 40 |
| 40603310 | HMA SC "C" N50 | TON | 228 | SANGAMON | 6 | 93733 | 40 |
| 42300200 | PCC DRIVEWAY PAVT 6 | SQ YD | 54 | SANGAMON | 6 | 93733 | 40 |
| 42300400 | PCC DRIVEWAY PAVT 8 | SQ YD | 702 | SANGAMON | 6 | 93733 | 40 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 8424 | SANGAMON | 6 | 93733 | 40 |
| 44000100 | PAVEMENT REM | SQ YD | 7016 | SANGAMON | 6 | 93733 | 40 |
| 44000200 | DRIVE PAVEMENT REM | SQ YD | 1065 | SANGAMON | 6 | 93733 | 40 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 1828 | SANGAMON | 6 | 93733 | 40 |
| 44000600 | SIDEWALK REM | SQ FT | 11212 | SANGAMON | 6 | 93733 | 40 |
| 44201349 | CL C PATCH T1 10 | SQ YD | 52 | SANGAMON | 6 | 93733 | 40 |
| 44201353 | CL C PATCH T2 10 | SQ YD | 125 | SANGAMON | 6 | 93733 | 40 |
| 44201357 | CL C PATCH T3 10 | SQ YD | 218 | SANGAMON | 6 | 93733 | 40 |
| 44201359 | CL C PATCH T4 10 | SQ YD | 896 | SANGAMON | 6 | 93733 | 40 |
| 48101500 | AGGREGATE SHLDS B 6 | SQ YD | 58 | SANGAMON | 6 | 93733 | 40 |
| 50100400 | REM EXIST STRUCT N2 | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 50100600 | REM EXIST STRUCT N4 | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 50102400 | CONC REM | CU YD | 5.7 | SANGAMON | 6 | 93733 | 40 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 30 | SANGAMON | 6 | 93733 | 40 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 2064 | SANGAMON | 6 | 93733 | 40 |
| 50300225 | CONC STRUCT | CU YD | 1127.7 | SANGAMON | 6 | 93733 | 40 |
| 50300285 | FORM LINER TEX SURF | SQ FT | 7149 | SANGAMON | 6 | 93733 | 40 |
| 50500505 | STUD SHEAR CONNECTORS | EACH | 1138 | SANGAMON | 6 | 93733 | 40 |
| 50800105 | REINFORCEMENT BARS | POUND | 865030 | SANGAMON | 6 | 93733 | 40 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 242310 | SANGAMON | 6 | 93733 | 40 |
| 51100100 | SLOPE WALL 4 | SQ YD | 601 | SANGAMON | 6 | 93733 | 40 |
| 51500100 | NAME PLATES | EACH | 4 | SANGAMON | 6 | 93733 | 40 |
| 51603000 | DRILLED SHAFT IN SOIL | CU YD | 1073.6 | SANGAMON | 6 | 93733 | 40 |
| 51604000 | DRILLED SHAFT IN ROCK | CU YD | 690 | SANGAMON | 6 | 93733 | 40 |
| 52200010 | TEMP SHT PILING | SQ FT | 314 | SANGAMON | 6 | 93733 | 40 |
| 52200015 | PERM SHT PILING | SQ FT | 566 | SANGAMON | 6 | 93733 | 40 |
| 52200020 | TEMP SOIL RETEN SYSTM | SQ FT | 3313 | SANGAMON | 6 | 93733 | 40 |
| 52200105 | FUR SOLDIER PILES WS | FOOT | 5866 | SANGAMON | 6 | 93733 | 40 |
| 52200200 | DRILL SET SLD PI SOIL | CU FT | 37467.9 | SANGAMON | 6 | 93733 | 40 |
| 52200205 | DRILL SET SLD PI ROCK | CU FT | 34367.8 | SANGAMON | 6 | 93733 | 40 |
| 52200250 | UNTREATED TIMBER LAG | SQ FT | 6093 | SANGAMON | 6 | 93733 | 40 |
| 52200265 | SECANT LAG | CU FT | 11739 | SANGAMON | 6 | 93733 | 40 |
| 52200900 | CONC STR RETAIN WALL | CU YD | 504.4 | SANGAMON | 6 | 93733 | 40 |
| 54213663 | PRC FLAR END SEC 18 | EACH | 10 | SANGAMON | 6 | 93733 | 40 |
| 550A0050 | STORM SEW CL A 1 12 | FOOT | 320 | SANGAMON | 6 | 93733 | 40 |
| 550A0070 | STORM SEW CL A 1 15 | FOOT | 8 | SANGAMON | 6 | 93733 | 40 |
| 550A0090 | STORM SEW CL A 1 18 | FOOT | 544 | SANGAMON | 6 | 93733 | 40 |
| 550A0190 | STORM SEW CL A 1 48 | FOOT | 291 | SANGAMON | 6 | 93733 | 40 |
| 550B0490 | STORM SEW CL B 2 54 | FOOT | 113 | SANGAMON | 6 | 93733 | 40 |
| 55100500 | STORM SEWER REM 12 | FOOT | 916 | SANGAMON | 6 | 93733 | 40 |
| 55100900 | STORM SEWER REM 18 | FOOT | 15 | SANGAMON | 6 | 93733 | 40 |
| 55201600 | STORM SEWERS JKD 48 | FOOT | 110 | SANGAMON | 6 | 93733 | 40 |
| 58600101 | GRANULAR BACKFILL STR | CU YD | 716 | SANGAMON | 6 | 93733 | 40 |
| 58700300 | CONCRETE SEALER | SQ FT | 16737 | SANGAMON | 6 | 93733 | 40 |
| 59100100 | GEOCOMPOSITE WALL DR | SQ YD | 699 | SANGAMON | 6 | 93733 | 40 |
| 59300100 | CONTR LOW-STRENG MATL | CU YD | 71 | SANGAMON | 6 | 93733 | 40 |
| 60100915 | PIPE DRAINS 6 | FOOT | 284 | SANGAMON | 6 | 93733 | 40 |
| 60108210 | PIPE UNDERDR T 2 10 | FOOT | 2859 | SANGAMON | 6 | 93733 | 40 |
| 60218400 | MAN TA 4 DIA T1F CL | EACH | 9 | SANGAMON | 6 | 93733 | 40 |
| 60219000 | MAN TA 4 DIA T8G | EACH | 3 | SANGAMON | 6 | 93733 | 40 |
| 60221700 | MAN TA 5 DIA T8G | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| 60224448 | MAN TA 7 DIA T8G | EACH | 5 | SANGAMON | 6 | 93733 | 40 |
| 60224458 | MAN TA 8 DIA T8G | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 60224459 | MAN TA 8 DIA T1F CL | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 60235700 | INLETS TA T3F&G | EACH | 7 | SANGAMON | 6 | 93733 | 40 |
| 60236200 | INLETS TA T8G | EACH | 10 | SANGAMON | 6 | 93733 | 40 |
| 60240220 | INLETS TB T3F&G | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 60240301 | INLETS TB T8G | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| 60255500 | MAN ADJUST | EACH | 4 | SANGAMON | 6 | 93733 | 40 |
| 60261000 | INLETS ADJ NEW T8G | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 60263100 | INL RECON NEW T3F&G | EACH | 4 | SANGAMON | 6 | 93733 | 40 |
| 60500040 | REMOV MANHOLES | EACH | 8 | SANGAMON | 6 | 93733 | 40 |
| 60500060 | REMOV INLETS | EACH | 11 | SANGAMON | 6 | 93733 | 40 |
| 60602800 | CONC GUTTER TB | FOOT | 147 | SANGAMON | 6 | 93733 | 40 |
| 60604400 | COMB CC&G TB6.18 | FOOT | 1383 | SANGAMON | 6 | 93733 | 40 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 25 | SANGAMON | 6 | 93733 | 40 |
| 63200310 | GUARDRAIL REMOV | FOOT | 55 | SANGAMON | 6 | 93733 | 40 |
| 66500105 | WOV W FENCE 4 | FOOT | 5145 | SANGAMON | 6 | 93733 | 40 |
| 66501600 | WOV W GATES 4X16 DBL | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| 66502000 | WOV W GATES 4X24 DBL | EACH | 1 | SANGAMON | 6 | 93733 | 40 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 12 | SANGAMON | 6 | 93733 | 40 |
| 67100100 | MOBILIZATION | L SUM | 1 | SANGAMON | 6 | 93733 | 40 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 700 | SANGAMON | 6 | 93733 | 40 |
| 70300230 | TEMP PVT MK LINE 5 | FOOT | 3697 | SANGAMON | 6 | 93733 | 40 |
| 70400100 | TEMP CONC BARRIER | FOOT | 1630 | SANGAMON | 6 | 93733 | 40 |
| 70600255 | IMP ATTN TEMP FRN TL2 | EACH | 4 | SANGAMON | 6 | 93733 | 40 |
| 72000100 | SIGN PANEL T1 | SQ FT | 63 | SANGAMON | 6 | 93733 | 40 |
| 72000200 | SIGN PANEL T2 | SQ FT | 10 | SANGAMON | 6 | 93733 | 40 |
| 72400100 | REMOV SIN PAN ASSY TA | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| 72400200 | REMOV SIN PAN ASSY TB | EACH | 7 | SANGAMON | 6 | 93733 | 40 |
| 72400310 | REMOV SIGN PANEL T1 | SQ FT | 2 | SANGAMON | 6 | 93733 | 40 |
| 72800100 | TELES STL SIN SUPPORT | FOOT | 108 | SANGAMON | 6 | 93733 | 40 |
| 78000300 | THPL PVT MK LINE 5 | FOOT | 3923 | SANGAMON | 6 | 93733 | 40 |
| 78000400 | THPL PVT MK LINE 6 | FOOT | 16 | SANGAMON | 6 | 93733 | 40 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 132 | SANGAMON | 6 | 93733 | 40 |
| 80400100 | ELECT SERV INSTALL | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| 81028320 | UNDRGRD C PVC 1 | FOOT | 104 | SANGAMON | 6 | 93733 | 40 |
| 81100320 | CON AT ST 1 PVC GS | FOOT | 644 | SANGAMON | 6 | 93733 | 40 |
| 81200200 | CON EMB STR 3/4 PVC | FOOT | 201 | SANGAMON | 6 | 93733 | 40 |
| 81200210 | CON EMB STR 1 PVC | FOOT | 375 | SANGAMON | 6 | 93733 | 40 |
| 81300220 | JUN BX SS AS 6X6X4 | EACH | 6 | SANGAMON | 6 | 93733 | 40 |
| 81300530 | JUN BX SS AS 12X10X6 | EACH | 4 | SANGAMON | 6 | 93733 | 40 |
| 81702450 | EC C XLP USE 3-1C 10 | FOOT | 1354 | SANGAMON | 6 | 93733 | 40 |
| 82500350 | LT CONT BASEM 240V100 | EACH | 2 | SANGAMON | 6 | 93733 | 40 |
| LR420021 | PCC PVMT 6 SPL | SQ YD | 380 | COLES | 7 | 95849 | 32 |
| X0327979 | PAVMT MRKG REM GRIND | SQ FT | 1880 | COLES | 7 | 95849 | 32 |
| X0350810 | BOLLARD REMOVAL | EACH | 5 | COLES | 7 | 95849 | 32 |
| X2020110 | GRADING & SHAP SHLDRS | UNIT | 925 | COLES | 7 | 95849 | 32 |
| X2020410 | EARTH EXCAVATION SPL | CU YD | 1039 | COLES | 7 | 95849 | 32 |
| X4240800 | DETECTABLE WARN SPL | SQ FT | 194 | COLES | 7 | 95849 | 32 |
| Z0051398 | REM EX SIGN POST | EACH | 23 | COLES | 7 | 95849 | 32 |
| 20200100 | EARTH EXCAVATION | CU YD | 316 | COLES | 7 | 95849 | 32 |
| 20800150 | TRENCH BACKFILL | CU YD | 182 | COLES | 7 | 95849 | 32 |
| 21101600 | TOPSOIL F & P VAR DP | SQ YD | 9076 | COLES | 7 | 95849 | 32 |
| 25000100 | SEEDING CL 1 | ACRE | 1.9 | COLES | 7 | 95849 | 32 |
| 25000312 | SEEDING CL 4A | ACRE | 3.3 | COLES | 7 | 95849 | 32 |
| 25000400 | NITROGEN FERT NUTR | POUND | 463 | COLES | 7 | 95849 | 32 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 463 | COLES | 7 | 95849 | 32 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 463 | COLES | 7 | 95849 | 32 |
| 25100115 | MULCH METHOD 2 | ACRE | 5.2 | COLES | 7 | 95849 | 32 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 6 | COLES | 7 | 95849 | 32 |
| 28000400 | PERIMETER EROS BAR | FOOT | 1400 | COLES | 7 | 95849 | 32 |
| 28000500 | INLET & PIPE PROTECT | EACH | 9 | COLES | 7 | 95849 | 32 |
| 31101200 | SUB GRAN MAT B 4 | SQ YD | 466 | COLES | 7 | 95849 | 32 |
| 35101400 | AGG BASE CSE B | TON | 370 | COLES | 7 | 95849 | 32 |
| 35800100 | PREPARATION OF BASE | SQ YD | 62588 | COLES | 7 | 95849 | 32 |
| 40603315 | HMA SC "C" N70 | TON | 6144 | COLES | 7 | 95849 | 32 |
| 42400200 | PC CONC SIDEWALK 5 | SQ FT | 2158 | COLES | 7 | 95849 | 32 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 296 | COLES | 7 | 95849 | 32 |
| 44000100 | PAVEMENT REM | SQ YD | 1331 | COLES | 7 | 95849 | 32 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 42 | COLES | 7 | 95849 | 32 |
| 44000600 | SIDEWALK REM | SQ FT | 1638 | COLES | 7 | 95849 | 32 |
| 44200094 | PAVT PATCH T2 8 | SQ YD | 7 | COLES | 7 | 95849 | 32 |
| 44200108 | PAVT PATCH T2 9 | SQ YD | 5 | COLES | 7 | 95849 | 32 |
| 44200114 | PAVT PATCH T4 9 | SQ YD | 33 | COLES | 7 | 95849 | 32 |
| 48101200 | AGGREGATE SHLDS B | TON | 29 | COLES | 7 | 95849 | 32 |
| 50102400 | CONC REM | CU YD | 7 | COLES | 7 | 95849 | 32 |
| 550B0040 | STORM SEW CL B 1 10 | FOOT | 535 | COLES | 7 | 95849 | 32 |
| 550B0050 | STORM SEW CL B 1 12 | FOOT | 12 | COLES | 7 | 95849 | 32 |
| 60235300 | INLETS TA T1F CL | EACH | 2 | COLES | 7 | 95849 | 32 |
| 60236200 | INLETS TA T8G | EACH | 6 | COLES | 7 | 95849 | 32 |
| 60255800 | MAN ADJ NEW T1F CL | EACH | 1 | COLES | 7 | 95849 | 32 |
| 60500060 | REMOV INLETS | EACH | 1 | COLES | 7 | 95849 | 32 |
| 60603800 | COMB CC&G TB6.12 | FOOT | 515 | COLES | 7 | 95849 | 32 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 1082 | COLES | 7 | 95849 | 32 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 7 | COLES | 7 | 95849 | 32 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | COLES | 7 | 95849 | 32 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 65 | COLES | 7 | 95849 | 32 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | COLES | 7 | 95849 | 32 |
| 67100100 | MOBILIZATION | L SUM | 1 | COLES | 7 | 95849 | 32 |
| 72000100 | SIGN PANEL T1 | SQ FT | 867 | COLES | 7 | 95849 | 32 |
| 72400310 | REMOV SIGN PANEL T1 | SQ FT | 539 | COLES | 7 | 95849 | 32 |
| 72900100 | METAL POST TY A | FOOT | 2084 | COLES | 7 | 95849 | 32 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 438 | COLES | 7 | 95849 | 32 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 19224 | COLES | 7 | 95849 | 32 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 165 | COLES | 7 | 95849 | 32 |
| 78000620 | THPL PVT MK LINE 18 | FOOT | 1804 | COLES | 7 | 95849 | 32 |
| 78009000 | MOD URETH PM LTR-SYM | SQ FT | 152 | COLES | 7 | 95849 | 32 |
| 78009012 | MOD URETH PM LINE 12 | FOOT | 30 | COLES | 7 | 95849 | 32 |
| 78009018 | MOD URETH PM LINE 18 | FOOT | 1030 | COLES | 7 | 95849 | 32 |
| LR631020 | TRAF BAR TERM T1 | EACH | 2 | EFFINGHAM | 7 | 95854 | 41 |
| X0325834 | HOR STRIP DRAINS | FOOT | 72 | EFFINGHAM | 7 | 95854 | 41 |
| X2501000 | SEEDING CL 2 SPL | ACRE | 0.95 | EFFINGHAM | 7 | 95854 | 41 |
| X2830495 | AGGREGATE DITCH SPL | TON | 170 | EFFINGHAM | 7 | 95854 | 41 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | EFFINGHAM | 7 | 95854 | 41 |
| 20100110 | TREE REMOV 6-15 | UNIT | 8 | EFFINGHAM | 7 | 95854 | 41 |
| 20100210 | TREE REMOV OVER 15 | UNIT | 144 | EFFINGHAM | 7 | 95854 | 41 |
| 20200100 | EARTH EXCAVATION | CU YD | 620 | EFFINGHAM | 7 | 95854 | 41 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 665 | EFFINGHAM | 7 | 95854 | 41 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 1435 | EFFINGHAM | 7 | 95854 | 41 |
| 20800150 | TRENCH BACKFILL | CU YD | 5 | EFFINGHAM | 7 | 95854 | 41 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 95 | EFFINGHAM | 7 | 95854 | 41 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 175 | EFFINGHAM | 7 | 95854 | 41 |
| 28000500 | INLET & PIPE PROTECT | EACH | 2 | EFFINGHAM | 7 | 95854 | 41 |
| 28100807 | STONE DUMP RIP CL A4 | TON | 760 | EFFINGHAM | 7 | 95854 | 41 |
| 40200800 | AGG SURF CSE B | TON | 950 | EFFINGHAM | 7 | 95854 | 41 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | EFFINGHAM | 7 | 95854 | 41 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 78 | EFFINGHAM | 7 | 95854 | 41 |
| 50300225 | CONC STRUCT | CU YD | 32.8 | EFFINGHAM | 7 | 95854 | 41 |
| 50300280 | CONCRETE ENCASEMENT | CU YD | 3.5 | EFFINGHAM | 7 | 95854 | 41 |
| 50400505 | P P CONC DK BM 27 DP | SQ FT | 1680 | EFFINGHAM | 7 | 95854 | 41 |
| 50800105 | REINFORCEMENT BARS | POUND | 4200 | EFFINGHAM | 7 | 95854 | 41 |
| 50900205 | STEEL RAILING TY S1 | FOOT | 124 | EFFINGHAM | 7 | 95854 | 41 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 585 | EFFINGHAM | 7 | 95854 | 41 |
| 51202305 | DRIVING PILES | FOOT | 585 | EFFINGHAM | 7 | 95854 | 41 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 1 | EFFINGHAM | 7 | 95854 | 41 |
| 51204650 | PILE SHOES | EACH | 9 | EFFINGHAM | 7 | 95854 | 41 |
| 51500100 | NAME PLATES | EACH | 1 | EFFINGHAM | 7 | 95854 | 41 |
| 542D0217 | P CUL CL D 1 12 | FOOT | 56 | EFFINGHAM | 7 | 95854 | 41 |
| 542D0220 | P CUL CL D 1 15 | FOOT | 44 | EFFINGHAM | 7 | 95854 | 41 |
| 59300100 | CONTR LOW-STRENG MATL | CU YD | 60 | EFFINGHAM | 7 | 95854 | 41 |
| 63100075 | TRAF BAR TERM T5A | EACH | 2 | EFFINGHAM | 7 | 95854 | 41 |
| 67100100 | MOBILIZATION | L SUM | 1 | EFFINGHAM | 7 | 95854 | 41 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | EFFINGHAM | 7 | 95854 | 41 |
| X2501000 | SEEDING CL 2 SPL | ACRE | 0.6 | LAWRENCE | 7 | 95855 | 42 |
| X2830495 | AGGREGATE DITCH SPL | TON | 220 | LAWRENCE | 7 | 95855 | 42 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | LAWRENCE | 7 | 95855 | 42 |
| 20200100 | EARTH EXCAVATION | CU YD | 515 | LAWRENCE | 7 | 95855 | 42 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 640 | LAWRENCE | 7 | 95855 | 42 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 60 | LAWRENCE | 7 | 95855 | 42 |
| 28000400 | PERIMETER EROS BAR | FOOT | 370 | LAWRENCE | 7 | 95855 | 42 |
| 28100807 | STONE DUMP RIP CL A4 | TON | 560 | LAWRENCE | 7 | 95855 | 42 |
| 35101400 | AGG BASE CSE B | TON | 80 | LAWRENCE | 7 | 95855 | 42 |
| 40200800 | AGG SURF CSE B | TON | 640 | LAWRENCE | 7 | 95855 | 42 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | LAWRENCE | 7 | 95855 | 42 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 68 | LAWRENCE | 7 | 95855 | 42 |
| 50300225 | CONC STRUCT | CU YD | 32.4 | LAWRENCE | 7 | 95855 | 42 |
| 50300280 | CONCRETE ENCASEMENT | CU YD | 3.5 | LAWRENCE | 7 | 95855 | 42 |
| 50400505 | P P CONC DK BM 27 DP | SQ FT | 1848 | LAWRENCE | 7 | 95855 | 42 |
| 50800105 | REINFORCEMENT BARS | POUND | 4300 | LAWRENCE | 7 | 95855 | 42 |
| 50900205 | STEEL RAILING TY S1 | FOOT | 136 | LAWRENCE | 7 | 95855 | 42 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 765 | LAWRENCE | 7 | 95855 | 42 |
| 51202305 | DRIVING PILES | FOOT | 765 | LAWRENCE | 7 | 95855 | 42 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 1 | LAWRENCE | 7 | 95855 | 42 |
| 51204650 | PILE SHOES | EACH | 9 | LAWRENCE | 7 | 95855 | 42 |
| 51500100 | NAME PLATES | EACH | 1 | LAWRENCE | 7 | 95855 | 42 |
| 542D1060 | P CUL CL D 2 15 | FOOT | 68 | LAWRENCE | 7 | 95855 | 42 |
| 542D1105 | P CUL CL D 2 60 | FOOT | 86 | LAWRENCE | 7 | 95855 | 42 |
| 59300100 | CONTR LOW-STRENG MATL | CU YD | 40 | LAWRENCE | 7 | 95855 | 42 |
| 67100100 | MOBILIZATION | L SUM | 1 | LAWRENCE | 7 | 95855 | 42 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | LAWRENCE | 7 | 95855 | 42 |
| XX127400 | PAVT REM & REPL SPL | TON | 40 | EDWARDS | 7 | 95857 | 33 |
| X4401198 | HMA SURF REM VAR DP | SQ YD | 778 | EDWARDS | 7 | 95857 | 33 |
| 40600290 | BIT MATLS TACK CT | POUND | 42456 | EDWARDS | 7 | 95857 | 33 |
| 40603085 | HMA BC IL-19.0 N70 | TON | 5610 | EDWARDS | 7 | 95857 | 33 |
| 40603315 | HMA SC "C" N70 | TON | 3105 | EDWARDS | 7 | 95857 | 33 |
| 44004000 | PAVED DITCH REMOVAL | FOOT | 15 | EDWARDS | 7 | 95857 | 33 |
| 48101200 | AGGREGATE SHLDS B | TON | 4499 | EDWARDS | 7 | 95857 | 33 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 347 | EDWARDS | 7 | 95857 | 33 |
| 542A0229 | P CUL CL A 1 24 | FOOT | 281 | EDWARDS | 7 | 95857 | 33 |
| 542A0241 | P CUL CL A 1 36 | FOOT | 66 | EDWARDS | 7 | 95857 | 33 |
| 59300100 | CONTR LOW-STRENG MATL | CU YD | 111 | EDWARDS | 7 | 95857 | 33 |
| 67100100 | MOBILIZATION | L SUM | 1 | EDWARDS | 7 | 95857 | 33 |
| 70100460 | TRAF CONT-PROT 701306 | L SUM | 1 | EDWARDS | 7 | 95857 | 33 |
| 70100600 | TRAF CONT-PROT 701336 | L SUM | 1 | EDWARDS | 7 | 95857 | 33 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 3818 | EDWARDS | 7 | 95857 | 33 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 1273 | EDWARDS | 7 | 95857 | 33 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 45982 | EDWARDS | 7 | 95857 | 33 |
| 20100500 | TREE REMOV ACRES | ACRE | 0.7 | SHELBY | 7 | 95858 | 34 |
| 20200100 | EARTH EXCAVATION | CU YD | 118 | SHELBY | 7 | 95858 | 34 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 1103 | SHELBY | 7 | 95858 | 34 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 1062 | SHELBY | 7 | 95858 | 34 |
| 25000200 | SEEDING CL 2 | ACRE | 0.5 | SHELBY | 7 | 95858 | 34 |
| 25000400 | NITROGEN FERT NUTR | POUND | 45 | SHELBY | 7 | 95858 | 34 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 45 | SHELBY | 7 | 95858 | 34 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 45 | SHELBY | 7 | 95858 | 34 |
| 25100115 | MULCH METHOD 2 | ACRE | 0.5 | SHELBY | 7 | 95858 | 34 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 100 | SHELBY | 7 | 95858 | 34 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 110 | SHELBY | 7 | 95858 | 34 |
| 28000400 | PERIMETER EROS BAR | FOOT | 340 | SHELBY | 7 | 95858 | 34 |
| 28000500 | INLET & PIPE PROTECT | EACH | 1 | SHELBY | 7 | 95858 | 34 |
| 28100205 | STONE RIPRAP CL A3 | TON | 5 | SHELBY | 7 | 95858 | 34 |
| 28100207 | STONE RIPRAP CL A4 | TON | 333 | SHELBY | 7 | 95858 | 34 |
| 28200200 | FILTER FABRIC | SQ YD | 480 | SHELBY | 7 | 95858 | 34 |
| 40200800 | AGG SURF CSE B | TON | 578 | SHELBY | 7 | 95858 | 34 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | SHELBY | 7 | 95858 | 34 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 123 | SHELBY | 7 | 95858 | 34 |
| 50300225 | CONC STRUCT | CU YD | 60.2 | SHELBY | 7 | 95858 | 34 |
| 50300280 | CONCRETE ENCASEMENT | CU YD | 34.1 | SHELBY | 7 | 95858 | 34 |
| 50400405 | P P CONC DK BM 21 DP | SQ FT | 2760 | SHELBY | 7 | 95858 | 34 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 7820 | SHELBY | 7 | 95858 | 34 |
| 50900205 | STEEL RAILING TY S1 | FOOT | 236 | SHELBY | 7 | 95858 | 34 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 444 | SHELBY | 7 | 95858 | 34 |
| 51201800 | FUR STL PILE HP14X73 | FOOT | 555 | SHELBY | 7 | 95858 | 34 |
| 51202305 | DRIVING PILES | FOOT | 999 | SHELBY | 7 | 95858 | 34 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 2 | SHELBY | 7 | 95858 | 34 |
| 51203800 | TEST PILE ST HP14X73 | EACH | 2 | SHELBY | 7 | 95858 | 34 |
| 51204650 | PILE SHOES | EACH | 22 | SHELBY | 7 | 95858 | 34 |
| 51500100 | NAME PLATES | EACH | 1 | SHELBY | 7 | 95858 | 34 |
| 542D0220 | P CUL CL D 1 15 | FOOT | 38 | SHELBY | 7 | 95858 | 34 |
| 60603800 | COMB CC&G TB6.12 | FOOT | 153 | SHELBY | 7 | 95858 | 34 |
| 67100100 | MOBILIZATION | L SUM | 1 | SHELBY | 7 | 95858 | 34 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | SHELBY | 7 | 95858 | 34 |
| X2501000 | SEEDING CL 2 SPL | ACRE | 0.1 | EFFINGHAM | 7 | 95859 | 43 |
| 20100500 | TREE REMOV ACRES | ACRE | 0.1 | EFFINGHAM | 7 | 95859 | 43 |
| 20200100 | EARTH EXCAVATION | CU YD | 125 | EFFINGHAM | 7 | 95859 | 43 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 120 | EFFINGHAM | 7 | 95859 | 43 |
| 28100807 | STONE DUMP RIP CL A4 | TON | 219 | EFFINGHAM | 7 | 95859 | 43 |
| 35101500 | AGG BASE CSE B | CU YD | 30 | EFFINGHAM | 7 | 95859 | 43 |
| 40200800 | AGG SURF CSE B | TON | 203 | EFFINGHAM | 7 | 95859 | 43 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | EFFINGHAM | 7 | 95859 | 43 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 56 | EFFINGHAM | 7 | 95859 | 43 |
| 50300225 | CONC STRUCT | CU YD | 22.8 | EFFINGHAM | 7 | 95859 | 43 |
| 50400305 | P P CONC DK BM 17 DP | SQ FT | 916 | EFFINGHAM | 7 | 95859 | 43 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 3000 | EFFINGHAM | 7 | 95859 | 43 |
| 50900205 | STEEL RAILING TY S1 | FOOT | 80 | EFFINGHAM | 7 | 95859 | 43 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 224 | EFFINGHAM | 7 | 95859 | 43 |
| 51202305 | DRIVING PILES | FOOT | 224 | EFFINGHAM | 7 | 95859 | 43 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 1 | EFFINGHAM | 7 | 95859 | 43 |
| 51500100 | NAME PLATES | EACH | 1 | EFFINGHAM | 7 | 95859 | 43 |
| 67100100 | MOBILIZATION | L SUM | 1 | EFFINGHAM | 7 | 95859 | 43 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | EFFINGHAM | 7 | 95859 | 43 |
| X0300015 | CONC WINGWALL REMOV | EACH | 2 | ST CLAIR | 8 | 97689 | 44 |
| X0322939 | RELOC EX FLAR END SEC | EACH | 4 | ST CLAIR | 8 | 97689 | 44 |
| X0900041 | PRECAST WINGWALL | EACH | 2 | ST CLAIR | 8 | 97689 | 44 |
| Z0036200 | PAINT CURB | FOOT | 149 | ST CLAIR | 8 | 97689 | 44 |
| 20200100 | EARTH EXCAVATION | CU YD | 3505 | ST CLAIR | 8 | 97689 | 44 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 2260 | ST CLAIR | 8 | 97689 | 44 |
| 20800150 | TRENCH BACKFILL | CU YD | 93 | ST CLAIR | 8 | 97689 | 44 |
| 25000210 | SEEDING CL 2A | ACRE | 3.75 | ST CLAIR | 8 | 97689 | 44 |
| 25000400 | NITROGEN FERT NUTR | POUND | 367 | ST CLAIR | 8 | 97689 | 44 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 367 | ST CLAIR | 8 | 97689 | 44 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 367 | ST CLAIR | 8 | 97689 | 44 |
| 25100125 | MULCH METHOD 3 | ACRE | 4 | ST CLAIR | 8 | 97689 | 44 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 367 | ST CLAIR | 8 | 97689 | 44 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 66 | ST CLAIR | 8 | 97689 | 44 |
| 28000400 | PERIMETER EROS BAR | FOOT | 2011 | ST CLAIR | 8 | 97689 | 44 |
| 28000500 | INLET & PIPE PROTECT | EACH | 4 | ST CLAIR | 8 | 97689 | 44 |
| 28100725 | STONE DUMP RIP CL B3 | SQ YD | 129 | ST CLAIR | 8 | 97689 | 44 |
| 28200200 | FILTER FABRIC | SQ YD | 129 | ST CLAIR | 8 | 97689 | 44 |
| 31100200 | SUB GRAN MAT A | CU YD | 99 | ST CLAIR | 8 | 97689 | 44 |
| 31100300 | SUB GRAN MAT A 4 | SQ YD | 2887 | ST CLAIR | 8 | 97689 | 44 |
| 31100500 | SUB GRAN MAT A 6 | SQ YD | 3625 | ST CLAIR | 8 | 97689 | 44 |
| 35501308 | HMA BASE CSE 6 | SQ YD | 3624 | ST CLAIR | 8 | 97689 | 44 |
| 40600275 | BIT MATLS PR CT | POUND | 8526 | ST CLAIR | 8 | 97689 | 44 |
| 40600290 | BIT MATLS TACK CT | POUND | 1631 | ST CLAIR | 8 | 97689 | 44 |
| 40600400 | MIX CR JTS FLANGEWYS | TON | 1 | ST CLAIR | 8 | 97689 | 44 |
| 40600982 | HMA SURF REM BUTT JT | SQ YD | 111 | ST CLAIR | 8 | 97689 | 44 |
| 40600990 | TEMPORARY RAMP | SQ YD | 109 | ST CLAIR | 8 | 97689 | 44 |
| 40603345 | HMA SC "D" N90 | TON | 1135 | ST CLAIR | 8 | 97689 | 44 |
| 40800050 | INCIDENTAL HMA SURF | TON | 19 | ST CLAIR | 8 | 97689 | 44 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 1189 | ST CLAIR | 8 | 97689 | 44 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 32 | ST CLAIR | 8 | 97689 | 44 |
| 44300200 | STRIP REF CR CON TR | FOOT | 3127 | ST CLAIR | 8 | 97689 | 44 |
| 48101500 | AGGREGATE SHLDS B 6 | SQ YD | 3284 | ST CLAIR | 8 | 97689 | 44 |
| 542A0223 | P CUL CL A 1 18 | FOOT | 98 | ST CLAIR | 8 | 97689 | 44 |
| 542A5491 | P CUL CL A 1 EQRS 36 | FOOT | 46 | ST CLAIR | 8 | 97689 | 44 |
| 56109210 | WATER VALVES ADJUST | EACH | 1 | ST CLAIR | 8 | 97689 | 44 |
| 60255500 | MAN ADJUST | EACH | 3 | ST CLAIR | 8 | 97689 | 44 |
| 60604400 | COMB CC&G TB6.18 | FOOT | 168 | ST CLAIR | 8 | 97689 | 44 |
| 60610400 | COMB CC&G TM6.24 | FOOT | 152 | ST CLAIR | 8 | 97689 | 44 |
| 60625600 | ISLAND PAVEMENT 6 | SQ YD | 59 | ST CLAIR | 8 | 97689 | 44 |
| 67100100 | MOBILIZATION | L SUM | 1 | ST CLAIR | 8 | 97689 | 44 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | ST CLAIR | 8 | 97689 | 44 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | ST CLAIR | 8 | 97689 | 44 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | ST CLAIR | 8 | 97689 | 44 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 30 | ST CLAIR | 8 | 97689 | 44 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 3222 | ST CLAIR | 8 | 97689 | 44 |
| 70300210 | TEMP PVT MK LTR & SYM | SQ FT | 515 | ST CLAIR | 8 | 97689 | 44 |
| 70300220 | TEMP PVT MK LINE 4 | FOOT | 5096 | ST CLAIR | 8 | 97689 | 44 |
| 70300250 | TEMP PVT MK LINE 8 | FOOT | 461 | ST CLAIR | 8 | 97689 | 44 |
| 70300260 | TEMP PVT MK LINE 12 | FOOT | 597 | ST CLAIR | 8 | 97689 | 44 |
| 70300280 | TEMP PVT MK LINE 24 | FOOT | 53 | ST CLAIR | 8 | 97689 | 44 |
| 72000100 | SIGN PANEL T1 | SQ FT | 183 | ST CLAIR | 8 | 97689 | 44 |
| 72400100 | REMOV SIN PAN ASSY TA | EACH | 45 | ST CLAIR | 8 | 97689 | 44 |
| 72400500 | RELOC SIN PAN ASSY TA | EACH | 12 | ST CLAIR | 8 | 97689 | 44 |
| 72400710 | RELOC SIGN PANEL T1 | SQ FT | 74 | ST CLAIR | 8 | 97689 | 44 |
| 72900100 | METAL POST TY A | FOOT | 462 | ST CLAIR | 8 | 97689 | 44 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 155 | ST CLAIR | 8 | 97689 | 44 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 10192 | ST CLAIR | 8 | 97689 | 44 |
| 78000500 | THPL PVT MK LINE 8 | FOOT | 921 | ST CLAIR | 8 | 97689 | 44 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 1194 | ST CLAIR | 8 | 97689 | 44 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 105 | ST CLAIR | 8 | 97689 | 44 |
| 78200020 | CURB REFLECTORS | EACH | 27 | ST CLAIR | 8 | 97689 | 44 |
| X0326020 | UTILTY PROTECTION PAD | SQ YD | 35 | MADISON | 8 | 97704 | 45 |
| X0326859 | PAVT IMPRINTING | SQ YD | 243 | MADISON | 8 | 97704 | 45 |
| X4240420 | PC CONC SIDEWALK 4 SP | SQ FT | 4455 | MADISON | 8 | 97704 | 45 |
| X7330064 | SIGN SUPPORT SPL | EACH | 8 | MADISON | 8 | 97704 | 45 |
| X7333095 | OVHD SIN STR-SPAN SPL | FOOT | 56 | MADISON | 8 | 97704 | 45 |
| 35300510 | PCC BSE CSE 10 1/2 | SQ YD | 8 | MADISON | 8 | 97704 | 45 |
| 40600290 | BIT MATLS TACK CT | POUND | 113 | MADISON | 8 | 97704 | 45 |
| 40603315 | HMA SC "C" N70 | TON | 50 | MADISON | 8 | 97704 | 45 |
| 40800050 | INCIDENTAL HMA SURF | TON | 3 | MADISON | 8 | 97704 | 45 |
| 42000060 | WELDED WIRE REINF | SQ YD | 8 | MADISON | 8 | 97704 | 45 |
| 42300400 | PCC DRIVEWAY PAVT 8 | SQ YD | 183 | MADISON | 8 | 97704 | 45 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 8546 | MADISON | 8 | 97704 | 45 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 95 | MADISON | 8 | 97704 | 45 |
| 44000100 | PAVEMENT REM | SQ YD | 8 | MADISON | 8 | 97704 | 45 |
| 44000157 | HMA SURF REM 2 | SQ YD | 259 | MADISON | 8 | 97704 | 45 |
| 44000200 | DRIVE PAVEMENT REM | SQ YD | 183 | MADISON | 8 | 97704 | 45 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 195 | MADISON | 8 | 97704 | 45 |
| 44000600 | SIDEWALK REM | SQ FT | 12387 | MADISON | 8 | 97704 | 45 |
| 50901760 | PIPE HANDRAIL | FOOT | 14 | MADISON | 8 | 97704 | 45 |
| 60605000 | COMB CC&G TB6.24 | FOOT | 180 | MADISON | 8 | 97704 | 45 |
| 67100100 | MOBILIZATION | L SUM | 1 | MADISON | 8 | 97704 | 45 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | MADISON | 8 | 97704 | 45 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | MADISON | 8 | 97704 | 45 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 136 | MADISON | 8 | 97704 | 45 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 46 | MADISON | 8 | 97704 | 45 |
| 70300260 | TEMP PVT MK LINE 12 | FOOT | 741 | MADISON | 8 | 97704 | 45 |
| 70300280 | TEMP PVT MK LINE 24 | FOOT | 136 | MADISON | 8 | 97704 | 45 |
| 72000100 | SIGN PANEL T1 | SQ FT | 33 | MADISON | 8 | 97704 | 45 |
| 72400100 | REMOV SIN PAN ASSY TA | EACH | 19 | MADISON | 8 | 97704 | 45 |
| 72400500 | RELOC SIN PAN ASSY TA | EACH | 12 | MADISON | 8 | 97704 | 45 |
| 72900100 | METAL POST TY A | FOOT | 102 | MADISON | 8 | 97704 | 45 |
| 72900200 | METAL POST TY B | FOOT | 120 | MADISON | 8 | 97704 | 45 |
| 73400100 | CONC FOUNDATION | CU YD | 8 | MADISON | 8 | 97704 | 45 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 741 | MADISON | 8 | 97704 | 45 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 136 | MADISON | 8 | 97704 | 45 |
| X2501000 | SEEDING CL 2 SPL | ACRE | 0.6 | WHITE | 9 | 99617 | 35 |
| 20100500 | TREE REMOV ACRES | ACRE | 0.1 | WHITE | 9 | 99617 | 35 |
| 20200100 | EARTH EXCAVATION | CU YD | 685 | WHITE | 9 | 99617 | 35 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 115 | WHITE | 9 | 99617 | 35 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 780 | WHITE | 9 | 99617 | 35 |
| 28100807 | STONE DUMP RIP CL A4 | TON | 490 | WHITE | 9 | 99617 | 35 |
| 40200800 | AGG SURF CSE B | TON | 450 | WHITE | 9 | 99617 | 35 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | WHITE | 9 | 99617 | 35 |
| 50300225 | CONC STRUCT | CU YD | 25.8 | WHITE | 9 | 99617 | 35 |
| 50400605 | P P CONC DK BM 33 DP | SQ FT | 1920 | WHITE | 9 | 99617 | 35 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 2920 | WHITE | 9 | 99617 | 35 |
| 50900205 | STEEL RAILING TY S1 | FOOT | 157 | WHITE | 9 | 99617 | 35 |
| 51201400 | FUR STL PILE HP10X42 | FOOT | 500 | WHITE | 9 | 99617 | 35 |
| 51202305 | DRIVING PILES | FOOT | 500 | WHITE | 9 | 99617 | 35 |
| 51204650 | PILE SHOES | EACH | 10 | WHITE | 9 | 99617 | 35 |
| 51500100 | NAME PLATES | EACH | 1 | WHITE | 9 | 99617 | 35 |
| 67100100 | MOBILIZATION | L SUM | 1 | WHITE | 9 | 99617 | 35 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | WHITE | 9 | 99617 | 35 |
| XX009289 | TRAF CONT-PROT BLR 21 | L SUM | 1 | JEFFERSON | 9 | 99623 | 36 |
| XX009291 | TRAF CONT-PROT BLR 22 | L SUM | 1 | JEFFERSON | 9 | 99623 | 36 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 17580 | JEFFERSON | 9 | 99623 | 36 |
| Z0055500 | RUMBLE STRIP | SQ FT | 825 | JEFFERSON | 9 | 99623 | 36 |
| 40200800 | AGG SURF CSE B | TON | 90 | JEFFERSON | 9 | 99623 | 36 |
| 40600290 | BIT MATLS TACK CT | POUND | 4400 | JEFFERSON | 9 | 99623 | 36 |
| 40600635 | LEV BIND MM N70 | TON | 2150 | JEFFERSON | 9 | 99623 | 36 |
| 40603315 | HMA SC "C" N70 | TON | 4500 | JEFFERSON | 9 | 99623 | 36 |
| 44000157 | HMA SURF REM 2 | SQ YD | 450 | JEFFERSON | 9 | 99623 | 36 |
| 44201759 | CL D PATCH T4 9 | SQ YD | 75 | JEFFERSON | 9 | 99623 | 36 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 1050 | JEFFERSON | 9 | 99623 | 36 |
| 67100100 | MOBILIZATION | L SUM | 1 | JEFFERSON | 9 | 99623 | 36 |
| 70100460 | TRAF CONT-PROT 701306 | L SUM | 1 | JEFFERSON | 9 | 99623 | 36 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 7050 | JEFFERSON | 9 | 99623 | 36 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 1174 | JEFFERSON | 9 | 99623 | 36 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 61000 | JEFFERSON | 9 | 99623 | 36 |
| X0900064 | MEMBR WTRPR SYS B STR | SQ YD | 138 | WHITE | 9 | 99628 | 46 |
| X1200140 | PCBC SPL | FOOT | 52 | WHITE | 9 | 99628 | 46 |
| X2070302 | POROUS GRAN EMB SPEC | TON | 500 | WHITE | 9 | 99628 | 46 |
| X2090210 | POROUS GRAN BACK SPEC | CU YD | 60 | WHITE | 9 | 99628 | 46 |
| X2501000 | SEEDING CL 2 SPL | ACRE | 0.3 | WHITE | 9 | 99628 | 46 |
| 20100110 | TREE REMOV 6-15 | UNIT | 48 | WHITE | 9 | 99628 | 46 |
| 20200100 | EARTH EXCAVATION | CU YD | 280 | WHITE | 9 | 99628 | 46 |
| 28100807 | STONE DUMP RIP CL A4 | TON | 200 | WHITE | 9 | 99628 | 46 |
| 40200800 | AGG SURF CSE B | TON | 415 | WHITE | 9 | 99628 | 46 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | WHITE | 9 | 99628 | 46 |
| 51500100 | NAME PLATES | EACH | 1 | WHITE | 9 | 99628 | 46 |
| 54001001 | BOX CUL END SEC C1 | EACH | 2 | WHITE | 9 | 99628 | 46 |
| 542D0229 | P CUL CL D 1 24 | FOOT | 81 | WHITE | 9 | 99628 | 46 |
| 542D0235 | P CUL CL D 1 30 | FOOT | 52 | WHITE | 9 | 99628 | 46 |
| 67100100 | MOBILIZATION | L SUM | 1 | WHITE | 9 | 99628 | 46 |
| X0322281 | W A VID DET SYS COM | EACH | 3 | PEORIA | 4 | 68E91 | 48 |
| X0323071 | SPARE FUL ACT CONT SP | EACH | 12 | PEORIA | 4 | 68E91 | 48 |
| X0326248 | ATMS SOFTWARE CORE | L SUM | 1 | PEORIA | 4 | 68E91 | 48 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | PEORIA | 4 | 68E91 | 48 |
| X8570215 | FAC IN EXIST CAB | EACH | 116 | PEORIA | 4 | 68E91 | 48 |
| X8570226 | FAC T4 CAB SPL | EACH | 2 | PEORIA | 4 | 68E91 | 48 |
| 67100100 | MOBILIZATION | L SUM | 1 | PEORIA | 4 | 68E91 | 48 |
| 89502210 | MOD EX CONTR CAB | EACH | 132 | PEORIA | 4 | 68E91 | 48 |
| X0556100 | PART DEPTH PATCH SPL | SQ YD | 1038.4 | TAZEWELL | 4 | 68E92 | 14 |
| X4421000 | PARTIAL DEPTH PATCH | TON | 232.6 | TAZEWELL | 4 | 68E92 | 14 |
| Z0033600 | LONG JOINT REPAIR | FOOT | 2074 | TAZEWELL | 4 | 68E92 | 14 |
| 44201827 | CL D PATCH T2 15 | SQ YD | 63.9 | TAZEWELL | 4 | 68E92 | 14 |
| 44201831 | CL D PATCH T3 15 | SQ YD | 16 | TAZEWELL | 4 | 68E92 | 14 |
| 60255500 | MAN ADJUST | EACH | 2 | TAZEWELL | 4 | 68E92 | 14 |
| 60260100 | INLETS ADJUST | EACH | 1 | TAZEWELL | 4 | 68E92 | 14 |
| 60262700 | INLETS RECONST | EACH | 1 | TAZEWELL | 4 | 68E92 | 14 |
| 67100100 | MOBILIZATION | L SUM | 1 | TAZEWELL | 4 | 68E92 | 14 |
| 70102632 | TR CONT & PROT 701602 | L SUM | 1 | TAZEWELL | 4 | 68E92 | 14 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | TAZEWELL | 4 | 68E92 | 14 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 46 | TAZEWELL | 4 | 68E92 | 14 |
| 78001100 | PT PVT MK LTRS & SYMB | SQ FT | 901 | TAZEWELL | 4 | 68E92 | 14 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 25908 | TAZEWELL | 4 | 68E92 | 14 |
| 78001140 | PAINT PVT MK LINE 8 | FOOT | 917 | TAZEWELL | 4 | 68E92 | 14 |
| 78001150 | PAINT PVT MK LINE 12 | FOOT | 380 | TAZEWELL | 4 | 68E92 | 14 |
| 78001180 | PAINT PVT MK LINE 24 | FOOT | 249 | TAZEWELL | 4 | 68E92 | 14 |
| 88600100 | DET LOOP T1 | FOOT | 409 | TAZEWELL | 4 | 68E92 | 14 |
| X0556100 | PART DEPTH PATCH SPL | SQ YD | 1093 | PEORIA | 4 | 68E96 | 47 |
| X4421000 | PARTIAL DEPTH PATCH | TON | 138 | PEORIA | 4 | 68E96 | 47 |
| Z0033600 | LONG JOINT REPAIR | FOOT | 7900 | PEORIA | 4 | 68E96 | 47 |
| 67100100 | MOBILIZATION | L SUM | 1 | PEORIA | 4 | 68E96 | 47 |
| 70102632 | TR CONT & PROT 701602 | L SUM | 1 | PEORIA | 4 | 68E96 | 47 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | PEORIA | 4 | 68E96 | 47 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 10 | PEORIA | 4 | 68E96 | 47 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 23603 | PEORIA | 4 | 68E96 | 47 |
| 78001130 | PAINT PVT MK LINE 6 | FOOT | 4400 | PEORIA | 4 | 68E96 | 47 |
| 78001140 | PAINT PVT MK LINE 8 | FOOT | 4021 | PEORIA | 4 | 68E96 | 47 |
| 78300200 | RAISED REF PVT MK REM | EACH | 25 | PEORIA | 4 | 68E96 | 47 |
| A2003020 | T-CELTIS OC PP 2-1/2 | EACH | 1 | WILL | 1 | 61F18 | 37 |
| A2005020 | T-GYMNOCLA DIO 2-1/2 | EACH | 1 | WILL | 1 | 61F18 | 37 |
| A2005620 | T-OSTRYA VIRG 2-1/2 | EACH | 1 | WILL | 1 | 61F18 | 37 |
| X0322508 | PED TRUSS SUPERSTR | SQ FT | 1424 | WILL | 1 | 61F18 | 37 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 142 | WILL | 1 | 61F18 | 37 |
| X0350805 | FOLD DOWN BOLLARDS | EACH | 1 | WILL | 1 | 61F18 | 37 |
| X4023000 | TEMP ACCESS- ROAD | EACH | 2 | WILL | 1 | 61F18 | 37 |
| Z0004522 | HMA DRIVEWAY PAVT 6 | SQ YD | 85 | WILL | 1 | 61F18 | 37 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | WILL | 1 | 61F18 | 37 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 52 | WILL | 1 | 61F18 | 37 |
| Z0046304 | P UNDR FOR STRUCT 4 | FOOT | 148 | WILL | 1 | 61F18 | 37 |
| 20200100 | EARTH EXCAVATION | CU YD | 314 | WILL | 1 | 61F18 | 37 |
| 20201200 | REM & DISP UNS MATL | CU YD | 11 | WILL | 1 | 61F18 | 37 |
| 21001000 | GEOTECH FAB F/GR STAB | SQ YD | 51 | WILL | 1 | 61F18 | 37 |
| 21101615 | TOPSOIL F & P 4 | SQ YD | 1713 | WILL | 1 | 61F18 | 37 |
| 25000210 | SEEDING CL 2A | ACRE | 0.5 | WILL | 1 | 61F18 | 37 |
| 25000310 | SEEDING CL 4 | ACRE | 0.25 | WILL | 1 | 61F18 | 37 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 1713 | WILL | 1 | 61F18 | 37 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 121 | WILL | 1 | 61F18 | 37 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 55 | WILL | 1 | 61F18 | 37 |
| 28000400 | PERIMETER EROS BAR | FOOT | 529 | WILL | 1 | 61F18 | 37 |
| 28000510 | INLET FILTERS | EACH | 2 | WILL | 1 | 61F18 | 37 |
| 28100107 | STONE RIPRAP CL A4 | SQ YD | 81 | WILL | 1 | 61F18 | 37 |
| 28200200 | FILTER FABRIC | SQ YD | 81 | WILL | 1 | 61F18 | 37 |
| 30300001 | AGG SUBGRADE IMPROVE | CU YD | 17 | WILL | 1 | 61F18 | 37 |
| 35101800 | AGG BASE CSE B 6 | SQ YD | 1111 | WILL | 1 | 61F18 | 37 |
| 40600275 | BIT MATLS PR CT | POUND | 2253 | WILL | 1 | 61F18 | 37 |
| 40603335 | HMA SC "D" N50 | TON | 75 | WILL | 1 | 61F18 | 37 |
| 42000100 | PCC PVT 6 | SQ YD | 160 | WILL | 1 | 61F18 | 37 |
| 42400200 | PC CONC SIDEWALK 5 | SQ FT | 1308 | WILL | 1 | 61F18 | 37 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 112 | WILL | 1 | 61F18 | 37 |
| 44000100 | PAVEMENT REM | SQ YD | 226 | WILL | 1 | 61F18 | 37 |
| 44000200 | DRIVE PAVEMENT REM | SQ YD | 72 | WILL | 1 | 61F18 | 37 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 89 | WILL | 1 | 61F18 | 37 |
| 44000600 | SIDEWALK REM | SQ FT | 330 | WILL | 1 | 61F18 | 37 |
| 44003100 | MEDIAN REMOVAL | SQ FT | 311 | WILL | 1 | 61F18 | 37 |
| 44004250 | PAVED SHLD REMOVAL | SQ YD | 66 | WILL | 1 | 61F18 | 37 |
| 44201705 | CL D PATCH T2 5 | SQ YD | 25 | WILL | 1 | 61F18 | 37 |
| 48101500 | AGGREGATE SHLDS B 6 | SQ YD | 23 | WILL | 1 | 61F18 | 37 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 77 | WILL | 1 | 61F18 | 37 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 75 | WILL | 1 | 61F18 | 37 |
| 50300225 | CONC STRUCT | CU YD | 85 | WILL | 1 | 61F18 | 37 |
| 50300255 | CONC SUP-STR | CU YD | 36 | WILL | 1 | 61F18 | 37 |
| 50300300 | PROTECTIVE COAT | SQ YD | 168 | WILL | 1 | 61F18 | 37 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 9750 | WILL | 1 | 61F18 | 37 |
| 50901720 | BICYCLE RAILING | FOOT | 146 | WILL | 1 | 61F18 | 37 |
| 51201600 | FUR STL PILE HP12X53 | FOOT | 138 | WILL | 1 | 61F18 | 37 |
| 51202305 | DRIVING PILES | FOOT | 138 | WILL | 1 | 61F18 | 37 |
| 51203600 | TEST PILE ST HP12X53 | EACH | 2 | WILL | 1 | 61F18 | 37 |
| 51204650 | PILE SHOES | EACH | 8 | WILL | 1 | 61F18 | 37 |
| 51500100 | NAME PLATES | EACH | 1 | WILL | 1 | 61F18 | 37 |
| 52200015 | PERM SHT PILING | SQ FT | 2187 | WILL | 1 | 61F18 | 37 |
| 52200600 | GEOTEX RETAIN WALL | SQ FT | 170 | WILL | 1 | 61F18 | 37 |
| 542D0220 | P CUL CL D 1 15 | FOOT | 45 | WILL | 1 | 61F18 | 37 |
| 54213663 | PRC FLAR END SEC 18 | EACH | 1 | WILL | 1 | 61F18 | 37 |
| 54262715 | METAL FL END SEC 15" | EACH | 2 | WILL | 1 | 61F18 | 37 |
| 550A0380 | STORM SEW CL A 2 18 | FOOT | 66 | WILL | 1 | 61F18 | 37 |
| 56400300 | FIRE HYDNTS TO BE ADJ | EACH | 1 | WILL | 1 | 61F18 | 37 |
| 58600101 | GRANULAR BACKFILL STR | CU YD | 128 | WILL | 1 | 61F18 | 37 |
| 58700300 | CONCRETE SEALER | SQ FT | 1994 | WILL | 1 | 61F18 | 37 |
| 59100100 | GEOCOMPOSITE WALL DR | SQ YD | 101 | WILL | 1 | 61F18 | 37 |
| 60218400 | MAN TA 4 DIA T1F CL | EACH | 1 | WILL | 1 | 61F18 | 37 |
| 60265700 | VV ADJUST | EACH | 1 | WILL | 1 | 61F18 | 37 |
| 60266600 | VALVE BOX ADJ | EACH | 2 | WILL | 1 | 61F18 | 37 |
| 60603800 | COMB CC&G TB6.12 | FOOT | 115 | WILL | 1 | 61F18 | 37 |
| 60618300 | CONC MEDIAN SURF 4 | SQ FT | 131 | WILL | 1 | 61F18 | 37 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 38 | WILL | 1 | 61F18 | 37 |
| 63100045 | TRAF BAR TERM T2 | EACH | 3 | WILL | 1 | 61F18 | 37 |
| 63200310 | GUARDRAIL REMOV | FOOT | 113 | WILL | 1 | 61F18 | 37 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 185 | WILL | 1 | 61F18 | 37 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 2 | WILL | 1 | 61F18 | 37 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | WILL | 1 | 61F18 | 37 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 1 | WILL | 1 | 61F18 | 37 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | WILL | 1 | 61F18 | 37 |
| 67100100 | MOBILIZATION | L SUM | 1 | WILL | 1 | 61F18 | 37 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | WILL | 1 | 61F18 | 37 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | WILL | 1 | 61F18 | 37 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | WILL | 1 | 61F18 | 37 |
| 72000100 | SIGN PANEL T1 | SQ FT | 214 | WILL | 1 | 61F18 | 37 |
| 72501000 | TERMINAL MARKER - DA | EACH | 3 | WILL | 1 | 61F18 | 37 |
| 72800100 | TELES STL SIN SUPPORT | FOOT | 404 | WILL | 1 | 61F18 | 37 |
| 73100100 | BASE TEL STL SIN SUPP | EACH | 29 | WILL | 1 | 61F18 | 37 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 224 | WILL | 1 | 61F18 | 37 |
| 78000400 | THPL PVT MK LINE 6 | FOOT | 142 | WILL | 1 | 61F18 | 37 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 213 | WILL | 1 | 61F18 | 37 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 44 | WILL | 1 | 61F18 | 37 |
| A2006516 | T-QUERCUS BICOL 2 | EACH | 8 | COOK | 1 | 61F79 | 2 |
| A2007116 | T-QUERCUS RUBRA 2 | EACH | 6 | COOK | 1 | 61F79 | 2 |
| B2001716 | T-CRAT C-I C TF 2 | EACH | 5 | COOK | 1 | 61F79 | 2 |
| X0322936 | REMOV EX FLAR END SEC | EACH | 12 | COOK | 1 | 61F79 | 2 |
| X2010510 | CLEARING & GRUBBING | L SUM | 1 | COOK | 1 | 61F79 | 2 |
| X4240800 | DETECTABLE WARN SPL | SQ FT | 40 | COOK | 1 | 61F79 | 2 |
| X6026050 | SANITARY MANHOLE ADJ | EACH | 1 | COOK | 1 | 61F79 | 2 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | COOK | 1 | 61F79 | 2 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 52 | COOK | 1 | 61F79 | 2 |
| Z0062450 | SAWING PAVEMENT (FD) | FOOT | 142 | COOK | 1 | 61F79 | 2 |
| 20100110 | TREE REMOV 6-15 | UNIT | 159 | COOK | 1 | 61F79 | 2 |
| 20100210 | TREE REMOV OVER 15 | UNIT | 84 | COOK | 1 | 61F79 | 2 |
| 20101100 | TREE TRUNK PROTECTION | EACH | 19 | COOK | 1 | 61F79 | 2 |
| 20101200 | TREE ROOT PRUNING | EACH | 19 | COOK | 1 | 61F79 | 2 |
| 20101300 | TREE PRUN 1-10 | EACH | 8 | COOK | 1 | 61F79 | 2 |
| 20101350 | TREE PRUN OVER 10 | EACH | 11 | COOK | 1 | 61F79 | 2 |
| 20101400 | NITROGEN FERT NUTR | POUND | 15 | COOK | 1 | 61F79 | 2 |
| 20101500 | PHOSPHORUS FERT NUTR | POUND | 15 | COOK | 1 | 61F79 | 2 |
| 20101600 | POTASSIUM FERT NUTR | POUND | 15 | COOK | 1 | 61F79 | 2 |
| 20101700 | SUPPLE WATERING | UNIT | 4 | COOK | 1 | 61F79 | 2 |
| 20200100 | EARTH EXCAVATION | CU YD | 282 | COOK | 1 | 61F79 | 2 |
| 20201200 | REM & DISP UNS MATL | CU YD | 105 | COOK | 1 | 61F79 | 2 |
| 20800150 | TRENCH BACKFILL | CU YD | 80 | COOK | 1 | 61F79 | 2 |
| 21101505 | TOPSOIL EXC & PLAC | CU YD | 300 | COOK | 1 | 61F79 | 2 |
| 21400100 | GRADING & SHAP DITCH | FOOT | 255 | COOK | 1 | 61F79 | 2 |
| 25000400 | NITROGEN FERT NUTR | POUND | 45 | COOK | 1 | 61F79 | 2 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 45 | COOK | 1 | 61F79 | 2 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 45 | COOK | 1 | 61F79 | 2 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 130 | COOK | 1 | 61F79 | 2 |
| 25200100 | SODDING | SQ YD | 3373 | COOK | 1 | 61F79 | 2 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 10 | COOK | 1 | 61F79 | 2 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 70 | COOK | 1 | 61F79 | 2 |
| 28000400 | PERIMETER EROS BAR | FOOT | 1450 | COOK | 1 | 61F79 | 2 |
| 28000510 | INLET FILTERS | EACH | 7 | COOK | 1 | 61F79 | 2 |
| 35101600 | AGG BASE CSE B 4 | SQ YD | 1069 | COOK | 1 | 61F79 | 2 |
| 35102000 | AGG BASE CSE B 8 | SQ YD | 536 | COOK | 1 | 61F79 | 2 |
| 40600275 | BIT MATLS PR CT | POUND | 1425 | COOK | 1 | 61F79 | 2 |
| 40600290 | BIT MATLS TACK CT | POUND | 470 | COOK | 1 | 61F79 | 2 |
| 40600625 | LEV BIND MM N50 | TON | 4 | COOK | 1 | 61F79 | 2 |
| 40603080 | HMA BC IL-19.0 N50 | TON | 71 | COOK | 1 | 61F79 | 2 |
| 40603335 | HMA SC "D" N50 | TON | 55 | COOK | 1 | 61F79 | 2 |
| 42300400 | PCC DRIVEWAY PAVT 8 | SQ YD | 154 | COOK | 1 | 61F79 | 2 |
| 42400200 | PC CONC SIDEWALK 5 | SQ FT | 8238 | COOK | 1 | 61F79 | 2 |
| 42400410 | PC CONC SIDEWALK 8 | SQ FT | 1486 | COOK | 1 | 61F79 | 2 |
| 44000159 | HMA SURF REM 2 1/2 | SQ YD | 93 | COOK | 1 | 61F79 | 2 |
| 44000200 | DRIVE PAVEMENT REM | SQ YD | 5671 | COOK | 1 | 61F79 | 2 |
| 44000300 | CURB REM | FOOT | 16 | COOK | 1 | 61F79 | 2 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 17 | COOK | 1 | 61F79 | 2 |
| 44000600 | SIDEWALK REM | SQ FT | 167 | COOK | 1 | 61F79 | 2 |
| 48101200 | AGGREGATE SHLDS B | TON | 2 | COOK | 1 | 61F79 | 2 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 206 | COOK | 1 | 61F79 | 2 |
| 542A0220 | P CUL CL A 1 15 | FOOT | 335 | COOK | 1 | 61F79 | 2 |
| 54213657 | PRC FLAR END SEC 12 | EACH | 2 | COOK | 1 | 61F79 | 2 |
| 54213660 | PRC FLAR END SEC 15 | EACH | 11 | COOK | 1 | 61F79 | 2 |
| 550A0050 | STORM SEW CL A 1 12 | FOOT | 265 | COOK | 1 | 61F79 | 2 |
| 55100500 | STORM SEWER REM 12 | FOOT | 325 | COOK | 1 | 61F79 | 2 |
| 60200805 | CB TA 4 DIA T8G | EACH | 1 | COOK | 1 | 61F79 | 2 |
| 60219000 | MAN TA 4 DIA T8G | EACH | 1 | COOK | 1 | 61F79 | 2 |
| 60236200 | INLETS TA T8G | EACH | 1 | COOK | 1 | 61F79 | 2 |
| 60300105 | FR & GRATES ADJUST | EACH | 4 | COOK | 1 | 61F79 | 2 |
| 60500040 | REMOV MANHOLES | EACH | 1 | COOK | 1 | 61F79 | 2 |
| 60600095 | CLASS SI CONC OUTLET | CU YD | 3 | COOK | 1 | 61F79 | 2 |
| 60600605 | CONC CURB TB | FOOT | 16 | COOK | 1 | 61F79 | 2 |
| 60605000 | COMB CC&G TB6.24 | FOOT | 17 | COOK | 1 | 61F79 | 2 |
| 67100100 | MOBILIZATION | L SUM | 1 | COOK | 1 | 61F79 | 2 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | COOK | 1 | 61F79 | 2 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | COOK | 1 | 61F79 | 2 |
| 72400600 | RELOC SIN PAN ASSY TB | EACH | 1 | COOK | 1 | 61F79 | 2 |
| 72400710 | RELOC SIGN PANEL T1 | SQ FT | 23 | COOK | 1 | 61F79 | 2 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 50 | COOK | 1 | 61F79 | 2 |
| X0324085 | EM VEH P S LSC 20 3C | FOOT | 264 | COOK | 1 | 62C21 | 3 |
| X1400107 | FAC T SUPER P CAB | EACH | 1 | COOK | 1 | 62C21 | 3 |
| X1400150 | SERV INSTL GR MT MTR | EACH | 1 | COOK | 1 | 62C21 | 3 |
| X1400201 | RADAR VEH DET SY SASB | EACH | 2 | COOK | 1 | 62C21 | 3 |
| X7011015 | TR C-PROT EXPRESSWAYS | L SUM | 1 | COOK | 1 | 62C21 | 3 |
| X8620200 | UNINTER POWER SUP SPL | EACH | 1 | COOK | 1 | 62C21 | 3 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 51.4 | COOK | 1 | 62C21 | 3 |
| Z0076600 | TRAINEES | HOUR | 1000 | COOK | 1 | 62C21 | 3 |
| Z0076604 | TRAINEES TPG | HOUR | 1000 | COOK | 1 | 62C21 | 3 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 887.5 | COOK | 1 | 62C21 | 3 |
| 63100089 | TRAF BAR TERM T6B | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 14 | COOK | 1 | 62C21 | 3 |
| 63200310 | GUARDRAIL REMOV | FOOT | 300 | COOK | 1 | 62C21 | 3 |
| 63500105 | DELINEATORS | EACH | 861 | COOK | 1 | 62C21 | 3 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 6 | COOK | 1 | 62C21 | 3 |
| 67100100 | MOBILIZATION | L SUM | 1 | COOK | 1 | 62C21 | 3 |
| 70100310 | TRAF CONT-PROT 701421 | L SUM | 1 | COOK | 1 | 62C21 | 3 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | COOK | 1 | 62C21 | 3 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | COOK | 1 | 62C21 | 3 |
| 72000200 | SIGN PANEL T2 | SQ FT | 70 | COOK | 1 | 62C21 | 3 |
| 72400500 | RELOC SIN PAN ASSY TA | EACH | 2 | COOK | 1 | 62C21 | 3 |
| 72501000 | TERMINAL MARKER - DA | EACH | 14 | COOK | 1 | 62C21 | 3 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 50 | COOK | 1 | 62C21 | 3 |
| 81028200 | UNDRGRD C GALVS 2 | FOOT | 827 | COOK | 1 | 62C21 | 3 |
| 81028220 | UNDRGRD C GALVS 3 | FOOT | 80 | COOK | 1 | 62C21 | 3 |
| 81028240 | UNDRGRD C GALVS 4 | FOOT | 308 | COOK | 1 | 62C21 | 3 |
| 81400100 | HANDHOLE | EACH | 5 | COOK | 1 | 62C21 | 3 |
| 81400200 | HD HANDHOLE | EACH | 2 | COOK | 1 | 62C21 | 3 |
| 81400300 | DBL HANDHOLE | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 85000200 | MAIN EX TR SIG INSTAL | EACH | 8 | COOK | 1 | 62C21 | 3 |
| 87301225 | ELCBL C SIGNAL 14 3C | FOOT | 264 | COOK | 1 | 62C21 | 3 |
| 87301245 | ELCBL C SIGNAL 14 5C | FOOT | 1062 | COOK | 1 | 62C21 | 3 |
| 87301255 | ELCBL C SIGNAL 14 7C | FOOT | 1396 | COOK | 1 | 62C21 | 3 |
| 87301305 | ELCBL C LEAD 14 1PR | FOOT | 1058 | COOK | 1 | 62C21 | 3 |
| 87301805 | ELCBL C SERV 6 2C | FOOT | 237 | COOK | 1 | 62C21 | 3 |
| 87301900 | ELCBL C EGRDC 6 1C | FOOT | 776 | COOK | 1 | 62C21 | 3 |
| 87502500 | TS POST GALVS 16 | EACH | 4 | COOK | 1 | 62C21 | 3 |
| 87700200 | S MAA & P 32 | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 87700220 | S MAA & P 36 | EACH | 2 | COOK | 1 | 62C21 | 3 |
| 87700230 | S MAA & P 38 | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 87800100 | CONC FDN TY A | FOOT | 20 | COOK | 1 | 62C21 | 3 |
| 87800150 | CONC FDN TY C | FOOT | 4 | COOK | 1 | 62C21 | 3 |
| 87800400 | CONC FDN TY E 30D | FOOT | 54 | COOK | 1 | 62C21 | 3 |
| 88030020 | SH LED 1F 3S MAM | EACH | 6 | COOK | 1 | 62C21 | 3 |
| 88200510 | TS BACKPLATE RET-REFL | EACH | 65 | COOK | 1 | 62C21 | 3 |
| 88500100 | INDUCTIVE LOOP DETECT | EACH | 4 | COOK | 1 | 62C21 | 3 |
| 88600100 | DET LOOP T1 | FOOT | 327 | COOK | 1 | 62C21 | 3 |
| 88700200 | LIGHT DETECTOR | EACH | 2 | COOK | 1 | 62C21 | 3 |
| 88700300 | LIGHT DETECTOR AMP | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 89000100 | TEMP TR SIG INSTALL | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 89500100 | RELOC EX SIG HEAD | EACH | 8 | COOK | 1 | 62C21 | 3 |
| 89502375 | REMOV EX TS EQUIP | EACH | 9 | COOK | 1 | 62C21 | 3 |
| 89502380 | REMOV EX HANDHOLE | EACH | 10 | COOK | 1 | 62C21 | 3 |
| 89502382 | REMOV EX DBL HANDHOLE | EACH | 1 | COOK | 1 | 62C21 | 3 |
| 89502385 | REMOV EX CONC FDN | EACH | 9 | COOK | 1 | 62C21 | 3 |
| X5870005 | BR DK CONC CRACK SEAL | SQ FT | 182473 | VARIOUS | 1 | 62H78 | 49 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 6 | VARIOUS | 1 | 62H78 | 49 |
| 67100100 | MOBILIZATION | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| 70102625 | TR CONT & PROT 701606 | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| 70102630 | TR CONT & PROT 701601 | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| 70102632 | TR CONT & PROT 701602 | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | VARIOUS | 1 | 62H78 | 49 |
| X0322918 | PRO MAN/CB CON OV SS | EACH | 4 | LAKE | 1 | 62H91 | 4 |
| X0326954 | TEMP FIBR OPT CONNECT | L SUM | 1 | LAKE | 1 | 62H91 | 4 |
| X0900075 | COFFERDAM TYP 1 IS WW | EACH | 1 | LAKE | 1 | 62H91 | 4 |
| X5537900 | SS CLEANED 15 | FOOT | 170 | LAKE | 1 | 62H91 | 4 |
| X5538000 | SS CLEANED 18 | FOOT | 20 | LAKE | 1 | 62H91 | 4 |
| X5538200 | SS CLEANED 24 | FOOT | 80 | LAKE | 1 | 62H91 | 4 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | LAKE | 1 | 62H91 | 4 |
| Z0018500 | DRAINAGE STR CLEANED | EACH | 2 | LAKE | 1 | 62H91 | 4 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 51.4 | LAKE | 1 | 62H91 | 4 |
| 20800150 | TRENCH BACKFILL | CU YD | 44 | LAKE | 1 | 62H91 | 4 |
| 21101505 | TOPSOIL EXC & PLAC | CU YD | 71 | LAKE | 1 | 62H91 | 4 |
| 21400100 | GRADING & SHAP DITCH | FOOT | 200 | LAKE | 1 | 62H91 | 4 |
| 25000210 | SEEDING CL 2A | ACRE | 0.05 | LAKE | 1 | 62H91 | 4 |
| 25000312 | SEEDING CL 4A | ACRE | 0.05 | LAKE | 1 | 62H91 | 4 |
| 25000400 | NITROGEN FERT NUTR | POUND | 9 | LAKE | 1 | 62H91 | 4 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 9 | LAKE | 1 | 62H91 | 4 |
| 25100115 | MULCH METHOD 2 | ACRE | 0.1 | LAKE | 1 | 62H91 | 4 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 35 | LAKE | 1 | 62H91 | 4 |
| 28000400 | PERIMETER EROS BAR | FOOT | 270 | LAKE | 1 | 62H91 | 4 |
| 28000500 | INLET & PIPE PROTECT | EACH | 3 | LAKE | 1 | 62H91 | 4 |
| 28001100 | TEMP EROS CONTR BLANK | SQ YD | 425 | LAKE | 1 | 62H91 | 4 |
| 30300112 | AGG SUBGRADE IMPR 12 | SQ YD | 14 | LAKE | 1 | 62H91 | 4 |
| 35101800 | AGG BASE CSE B 6 | SQ YD | 8 | LAKE | 1 | 62H91 | 4 |
| 35501316 | HMA BASE CSE 8 | SQ YD | 14 | LAKE | 1 | 62H91 | 4 |
| 40603340 | HMA SC "D" N70 | TON | 2 | LAKE | 1 | 62H91 | 4 |
| 40700100 | BIT MATLS TACK CT | POUND | 10 | LAKE | 1 | 62H91 | 4 |
| 44000100 | PAVEMENT REM | SQ YD | 20 | LAKE | 1 | 62H91 | 4 |
| 48101600 | AGGREGATE SHLDS B 8 | SQ YD | 5 | LAKE | 1 | 62H91 | 4 |
| 48203021 | HMA SHOULDERS 6 | SQ YD | 4 | LAKE | 1 | 62H91 | 4 |
| 550A0120 | STORM SEW CL A 1 24 | FOOT | 70 | LAKE | 1 | 62H91 | 4 |
| 55100900 | STORM SEWER REM 18 | FOOT | 50 | LAKE | 1 | 62H91 | 4 |
| 60200805 | CB TA 4 DIA T8G | EACH | 1 | LAKE | 1 | 62H91 | 4 |
| 60223800 | MAN TA 6 DIA T1F CL | EACH | 1 | LAKE | 1 | 62H91 | 4 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 78 | LAKE | 1 | 62H91 | 4 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 1 | LAKE | 1 | 62H91 | 4 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | LAKE | 1 | 62H91 | 4 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 6 | LAKE | 1 | 62H91 | 4 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | LAKE | 1 | 62H91 | 4 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 6 | LAKE | 1 | 62H91 | 4 |
| 67100100 | MOBILIZATION | L SUM | 1 | LAKE | 1 | 62H91 | 4 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | LAKE | 1 | 62H91 | 4 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 33 | LAKE | 1 | 62H91 | 4 |
| 70300520 | PAVT MARK TAPE T3 4 | FOOT | 100 | LAKE | 1 | 62H91 | 4 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 100 | LAKE | 1 | 62H91 | 4 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 4 | LAKE | 1 | 62H91 | 4 |
| Z0033072 | VIDEO VEH DET SYS | EACH | 1 | WHITESIDE | 2 | 64N87 | 5 |
| 40600290 | BIT MATLS TACK CT | POUND | 4426 | WHITESIDE | 2 | 64N87 | 5 |
| 40600990 | TEMPORARY RAMP | SQ YD | 200 | WHITESIDE | 2 | 64N87 | 5 |
| 40603335 | HMA SC "D" N50 | TON | 1102 | WHITESIDE | 2 | 64N87 | 5 |
| 44000157 | HMA SURF REM 2 | SQ YD | 9835 | WHITESIDE | 2 | 64N87 | 5 |
| 60255500 | MAN ADJUST | EACH | 7 | WHITESIDE | 2 | 64N87 | 5 |
| 60265700 | VV ADJUST | EACH | 3 | WHITESIDE | 2 | 64N87 | 5 |
| 67100100 | MOBILIZATION | L SUM | 1 | WHITESIDE | 2 | 64N87 | 5 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | WHITESIDE | 2 | 64N87 | 5 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | WHITESIDE | 2 | 64N87 | 5 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 4518 | WHITESIDE | 2 | 64N87 | 5 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 498 | WHITESIDE | 2 | 64N87 | 5 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 447.2 | WHITESIDE | 2 | 64N87 | 5 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 4284 | WHITESIDE | 2 | 64N87 | 5 |
| 78000400 | THPL PVT MK LINE 6 | FOOT | 652 | WHITESIDE | 2 | 64N87 | 5 |
| 78000500 | THPL PVT MK LINE 8 | FOOT | 969 | WHITESIDE | 2 | 64N87 | 5 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 536 | WHITESIDE | 2 | 64N87 | 5 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 173 | WHITESIDE | 2 | 64N87 | 5 |
| 89502210 | MOD EX CONTR CAB | EACH | 1 | WHITESIDE | 2 | 64N87 | 5 |
| X0300004 | BIT MATLS TACK CT SPL | POUND | 11595 | WINNEBAGO | 2 | 64N89 | 6 |
| Z0033072 | VIDEO VEH DET SYS | EACH | 1 | WINNEBAGO | 2 | 64N89 | 6 |
| 40603570 | P HMA SC "E" N90 | TON | 1916 | WINNEBAGO | 2 | 64N89 | 6 |
| 44000157 | HMA SURF REM 2 | SQ YD | 16104 | WINNEBAGO | 2 | 64N89 | 6 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 240 | WINNEBAGO | 2 | 64N89 | 6 |
| 64200116 | SHOULDER RUM STRIP 16 | FOOT | 4515 | WINNEBAGO | 2 | 64N89 | 6 |
| 67100100 | MOBILIZATION | L SUM | 1 | WINNEBAGO | 2 | 64N89 | 6 |
| 70100800 | TRAF CONT-PROT 701401 | L SUM | 1 | WINNEBAGO | 2 | 64N89 | 6 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | WINNEBAGO | 2 | 64N89 | 6 |
| 70200100 | NIGHT WORK ZONE LIGHT | L SUM | 1 | WINNEBAGO | 2 | 64N89 | 6 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 1844 | WINNEBAGO | 2 | 64N89 | 6 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 510 | WINNEBAGO | 2 | 64N89 | 6 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 325.4 | WINNEBAGO | 2 | 64N89 | 6 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 7874 | WINNEBAGO | 2 | 64N89 | 6 |
| 78000500 | THPL PVT MK LINE 8 | FOOT | 1277 | WINNEBAGO | 2 | 64N89 | 6 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 602 | WINNEBAGO | 2 | 64N89 | 6 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 76 | WINNEBAGO | 2 | 64N89 | 6 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 126 | WINNEBAGO | 2 | 64N89 | 6 |
| 78300200 | RAISED REF PVT MK REM | EACH | 126 | WINNEBAGO | 2 | 64N89 | 6 |
| 89502210 | MOD EX CONTR CAB | EACH | 1 | WINNEBAGO | 2 | 64N89 | 6 |
| X4401198 | HMA SURF REM VAR DP | SQ YD | 3993 | BUREAU | 3 | 66A92 | 8 |
| Z0005216 | HMA STAB 6 AT SPBGR | SQ YD | 1147 | BUREAU | 3 | 66A92 | 8 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 42 | BUREAU | 3 | 66A92 | 8 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 30929 | BUREAU | 3 | 66A92 | 8 |
| Z0034105 | MATL TRANSFER DEVICE | TON | 20260 | BUREAU | 3 | 66A92 | 8 |
| Z0048665 | RR PROT LIABILITY INS | L SUM | 1 | BUREAU | 3 | 66A92 | 8 |
| Z0076600 | TRAINEES | HOUR | 2000 | BUREAU | 3 | 66A92 | 8 |
| Z0076604 | TRAINEES TPG | HOUR | 2000 | BUREAU | 3 | 66A92 | 8 |
| 28000315 | AGG DITCH CHECKS | TON | 25 | BUREAU | 3 | 66A92 | 8 |
| 40200800 | AGG SURF CSE B | TON | 202 | BUREAU | 3 | 66A92 | 8 |
| 40600290 | BIT MATLS TACK CT | POUND | 9026 | BUREAU | 3 | 66A92 | 8 |
| 40600400 | MIX CR JTS FLANGEWYS | TON | 28 | BUREAU | 3 | 66A92 | 8 |
| 40600982 | HMA SURF REM BUTT JT | SQ YD | 222 | BUREAU | 3 | 66A92 | 8 |
| 40600990 | TEMPORARY RAMP | SQ YD | 115 | BUREAU | 3 | 66A92 | 8 |
| 40602978 | HMA BC IL-9.5 N50 | TON | 10307 | BUREAU | 3 | 66A92 | 8 |
| 40603080 | HMA BC IL-19.0 N50 | TON | 1390 | BUREAU | 3 | 66A92 | 8 |
| 40603310 | HMA SC "C" N50 | TON | 9710 | BUREAU | 3 | 66A92 | 8 |
| 40800050 | INCIDENTAL HMA SURF | TON | 447 | BUREAU | 3 | 66A92 | 8 |
| 44000155 | HMA SURF REM 1 1/2 | SQ YD | 1213 | BUREAU | 3 | 66A92 | 8 |
| 44000164 | HMA SURF REM 3 3/4 | SQ YD | 89350 | BUREAU | 3 | 66A92 | 8 |
| 44000182 | HMA SURF REM 8 | SQ YD | 669 | BUREAU | 3 | 66A92 | 8 |
| 48101200 | AGGREGATE SHLDS B | TON | 2363 | BUREAU | 3 | 66A92 | 8 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 3237.5 | BUREAU | 3 | 66A92 | 8 |
| 63000350 | LSG OV CUL 12'6" SPAN | FOOT | 75 | BUREAU | 3 | 66A92 | 8 |
| 63000370 | LSG OVER CUL 25' SPAN | FOOT | 200 | BUREAU | 3 | 66A92 | 8 |
| 63100085 | TRAF BAR TERM T6 | EACH | 6 | BUREAU | 3 | 66A92 | 8 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 18 | BUREAU | 3 | 66A92 | 8 |
| 63200310 | GUARDRAIL REMOV | FOOT | 3301 | BUREAU | 3 | 66A92 | 8 |
| 66700205 | PERM SURV MKRS T1 | EACH | 4 | BUREAU | 3 | 66A92 | 8 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 3 | BUREAU | 3 | 66A92 | 8 |
| 67100100 | MOBILIZATION | L SUM | 1 | BUREAU | 3 | 66A92 | 8 |
| 70100460 | TRAF CONT-PROT 701306 | L SUM | 1 | BUREAU | 3 | 66A92 | 8 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | BUREAU | 3 | 66A92 | 8 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 11794 | BUREAU | 3 | 66A92 | 8 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 1297 | BUREAU | 3 | 66A92 | 8 |
| 70300220 | TEMP PVT MK LINE 4 | FOOT | 85850 | BUREAU | 3 | 66A92 | 8 |
| 70300240 | TEMP PVT MK LINE 6 | FOOT | 8736 | BUREAU | 3 | 66A92 | 8 |
| 72501000 | TERMINAL MARKER - DA | EACH | 18 | BUREAU | 3 | 66A92 | 8 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 171700 | BUREAU | 3 | 66A92 | 8 |
| 78001130 | PAINT PVT MK LINE 6 | FOOT | 17472 | BUREAU | 3 | 66A92 | 8 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 437 | BUREAU | 3 | 66A92 | 8 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 61 | BUREAU | 3 | 66A92 | 8 |
| 78300200 | RAISED REF PVT MK REM | EACH | 437 | BUREAU | 3 | 66A92 | 8 |
| X0326887 | WOOD POLE 25 CL 4 | EACH | 1 | KENDALL | 3 | 66H92 | 9 |
| X8620200 | UNINTER POWER SUP SPL | EACH | 1 | KENDALL | 3 | 66H92 | 9 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 84 | KENDALL | 3 | 66H92 | 9 |
| 67100100 | MOBILIZATION | L SUM | 1 | KENDALL | 3 | 66H92 | 9 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | KENDALL | 3 | 66H92 | 9 |
| 80500300 | SERV INSTALL TY C | EACH | 1 | KENDALL | 3 | 66H92 | 9 |
| 81028200 | UNDRGRD C GALVS 2 | FOOT | 254 | KENDALL | 3 | 66H92 | 9 |
| 81028350 | UNDRGRD C PVC 2 | FOOT | 1373 | KENDALL | 3 | 66H92 | 9 |
| 81100500 | CON AT ST 1 1/2 GALVS | FOOT | 63 | KENDALL | 3 | 66H92 | 9 |
| 81400700 | HANDHOLE PCC | EACH | 6 | KENDALL | 3 | 66H92 | 9 |
| 85800100 | FL CONT | EACH | 1 | KENDALL | 3 | 66H92 | 9 |
| 87301215 | ELCBL C SIGNAL 14 2C | FOOT | 1940 | KENDALL | 3 | 66H92 | 9 |
| 87301805 | ELCBL C SERV 6 2C | FOOT | 5 | KENDALL | 3 | 66H92 | 9 |
| 87301900 | ELCBL C EGRDC 6 1C | FOOT | 1940 | KENDALL | 3 | 66H92 | 9 |
| 88040030 | SH P LED 1F 1S PM | EACH | 4 | KENDALL | 3 | 66H92 | 9 |
| X1200050 | BOX CULVERT REMOVAL | FOOT | 60 | FORD | 3 | 66J58 | 10 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 42 | FORD | 3 | 66J58 | 10 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 5.2 | FORD | 3 | 66J58 | 10 |
| 20800150 | TRENCH BACKFILL | CU YD | 12.6 | FORD | 3 | 66J58 | 10 |
| 44201019 | CL B PATCH T2 14 | SQ YD | 32 | FORD | 3 | 66J58 | 10 |
| 44201299 | DOWEL BARS 1 1/2 | EACH | 80 | FORD | 3 | 66J58 | 10 |
| 44213200 | SAW CUTS | FOOT | 156 | FORD | 3 | 66J58 | 10 |
| 48101200 | AGGREGATE SHLDS B | TON | 2 | FORD | 3 | 66J58 | 10 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 50 | FORD | 3 | 66J58 | 10 |
| 542A0223 | P CUL CL A 1 18 | FOOT | 38 | FORD | 3 | 66J58 | 10 |
| 542A5479 | P CUL CL A 1 EQRS 24 | FOOT | 38 | FORD | 3 | 66J58 | 10 |
| 54213663 | PRC FLAR END SEC 18 | EACH | 2 | FORD | 3 | 66J58 | 10 |
| 54214509 | PRC FL END S EQ RS 24 | EACH | 3 | FORD | 3 | 66J58 | 10 |
| 63500310 | REM & REIN DELINEATOR | EACH | 4 | FORD | 3 | 66J58 | 10 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 20 | FORD | 3 | 66J58 | 10 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 2 | FORD | 3 | 66J58 | 10 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | FORD | 3 | 66J58 | 10 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 2 | FORD | 3 | 66J58 | 10 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | FORD | 3 | 66J58 | 10 |
| 67100100 | MOBILIZATION | L SUM | 1 | FORD | 3 | 66J58 | 10 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | FORD | 3 | 66J58 | 10 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 13870 | FORD | 3 | 66K05 | 11 |
| Z0030850 | TEMP INFO SIGNING | SQ FT | 42 | FORD | 3 | 66K05 | 11 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 17989 | FORD | 3 | 66K05 | 11 |
| Z0034105 | MATL TRANSFER DEVICE | TON | 9193 | FORD | 3 | 66K05 | 11 |
| Z0076600 | TRAINEES | HOUR | 2000 | FORD | 3 | 66K05 | 11 |
| Z0076604 | TRAINEES TPG | HOUR | 2000 | FORD | 3 | 66K05 | 11 |
| 40600290 | BIT MATLS TACK CT | POUND | 40854 | FORD | 3 | 66K05 | 11 |
| 40600400 | MIX CR JTS FLANGEWYS | TON | 18 | FORD | 3 | 66K05 | 11 |
| 40600527 | LB HM IL-9.5FG N50 | TON | 30 | FORD | 3 | 66K05 | 11 |
| 40600627 | LB MM IL-9.5FG N50 | TON | 4178 | FORD | 3 | 66K05 | 11 |
| 40600990 | TEMPORARY RAMP | SQ YD | 153 | FORD | 3 | 66K05 | 11 |
| 40603310 | HMA SC "C" N50 | TON | 5015 | FORD | 3 | 66K05 | 11 |
| 40800050 | INCIDENTAL HMA SURF | TON | 70 | FORD | 3 | 66K05 | 11 |
| 44000155 | HMA SURF REM 1 1/2 | SQ YD | 829 | FORD | 3 | 66K05 | 11 |
| 44000160 | HMA SURF REM 2 3/4 | SQ YD | 59696 | FORD | 3 | 66K05 | 11 |
| 44201803 | CL D PATCH T2 13 | SQ YD | 264 | FORD | 3 | 66K05 | 11 |
| 44201807 | CL D PATCH T3 13 | SQ YD | 20 | FORD | 3 | 66K05 | 11 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 660 | FORD | 3 | 66K05 | 11 |
| 67100100 | MOBILIZATION | L SUM | 1 | FORD | 3 | 66K05 | 11 |
| 70100460 | TRAF CONT-PROT 701306 | L SUM | 1 | FORD | 3 | 66K05 | 11 |
| 70100600 | TRAF CONT-PROT 701336 | L SUM | 1 | FORD | 3 | 66K05 | 11 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 9582 | FORD | 3 | 66K05 | 11 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 3194 | FORD | 3 | 66K05 | 11 |
| 70300220 | TEMP PVT MK LINE 4 | FOOT | 34862 | FORD | 3 | 66K05 | 11 |
| 70300240 | TEMP PVT MK LINE 6 | FOOT | 4498 | FORD | 3 | 66K05 | 11 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 70500 | FORD | 3 | 66K05 | 11 |
| 78001130 | PAINT PVT MK LINE 6 | FOOT | 9094 | FORD | 3 | 66K05 | 11 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 227 | FORD | 3 | 66K05 | 11 |
| 78300200 | RAISED REF PVT MK REM | EACH | 227 | FORD | 3 | 66K05 | 11 |
| X0320581 | DRUMS | EACH | 33 | GRUNDY | 3 | 66K25 | 12 |
| X0322936 | REMOV EX FLAR END SEC | EACH | 2 | GRUNDY | 3 | 66K25 | 12 |
| X0325231 | CABLE GUARD MARKER | EACH | 85 | GRUNDY | 3 | 66K25 | 12 |
| X0325667 | WD CTRL MWNG STRP SP | SQ YD | 1124 | GRUNDY | 3 | 66K25 | 12 |
| X0326677 | REM HT CBL MEDIAN BAR | FOOT | 5216 | GRUNDY | 3 | 66K25 | 12 |
| X0326687 | REM HTC MED BAR TERM | EACH | 5 | GRUNDY | 3 | 66K25 | 12 |
| X0326880 | MESSAGE BOARD VEH DRV | HOUR | 352 | GRUNDY | 3 | 66K25 | 12 |
| X0326907 | PORT VHMNT CH MSS SGN | CAL MO | 2 | GRUNDY | 3 | 66K25 | 12 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 11272 | GRUNDY | 3 | 66K25 | 12 |
| X2140100 | GRAD & SHAP DITCH SPL | FOOT | 1626 | GRUNDY | 3 | 66K25 | 12 |
| X2700001 | TEMP RUMBLE STRIPS SP | EACH | 4 | GRUNDY | 3 | 66K25 | 12 |
| X4060006 | P HMA SC SMA 12.5 N80 | TON | 4849 | GRUNDY | 3 | 66K25 | 12 |
| X5420654 | PIPE CULV CLEANED 54 | FOOT | 360 | GRUNDY | 3 | 66K25 | 12 |
| X6350120 | DELINEATOR REMOVAL | EACH | 110 | GRUNDY | 3 | 66K25 | 12 |
| X7010805 | TR C-PROT 701401 SPL | L SUM | 1 | GRUNDY | 3 | 66K25 | 12 |
| X7830070 | GRV RCSD PVT MRKG 5 | FOOT | 30028 | GRUNDY | 3 | 66K25 | 12 |
| X7830074 | GRV RCSD PVT MRKG 7 | FOOT | 2260 | GRUNDY | 3 | 66K25 | 12 |
| X7830076 | GRV RCSD PVT MRKG 9 | FOOT | 974 | GRUNDY | 3 | 66K25 | 12 |
| X7830090 | GRV RCSD PVT MRKG 25 | FOOT | 99 | GRUNDY | 3 | 66K25 | 12 |
| X9700001 | CHANGEABLE MSG SN SPL | CAL WK | 56 | GRUNDY | 3 | 66K25 | 12 |
| X9700002 | SMART TRAF MONIT SYS | CAL WK | 8 | GRUNDY | 3 | 66K25 | 12 |
| X9700005 | SMART TRAF MONIT DEV | CAL WK | 40 | GRUNDY | 3 | 66K25 | 12 |
| X9700013 | REAL-TIME TR CTRL SU | WEEK | 32 | GRUNDY | 3 | 66K25 | 12 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 4490 | GRUNDY | 3 | 66K25 | 12 |
| Z0034105 | MATL TRANSFER DEVICE | TON | 11398 | GRUNDY | 3 | 66K25 | 12 |
| Z0065767 | SLOT DR 15"W/1.75" SL | FOOT | 405 | GRUNDY | 3 | 66K25 | 12 |
| Z0076600 | TRAINEES | HOUR | 3000 | GRUNDY | 3 | 66K25 | 12 |
| Z0076604 | TRAINEES TPG | HOUR | 3000 | GRUNDY | 3 | 66K25 | 12 |
| 20200100 | EARTH EXCAVATION | CU YD | 3562 | GRUNDY | 3 | 66K25 | 12 |
| 25000210 | SEEDING CL 2A | ACRE | 1.75 | GRUNDY | 3 | 66K25 | 12 |
| 25000400 | NITROGEN FERT NUTR | POUND | 140 | GRUNDY | 3 | 66K25 | 12 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 140 | GRUNDY | 3 | 66K25 | 12 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 140 | GRUNDY | 3 | 66K25 | 12 |
| 25100630 | EROSION CONTR BLANKET | SQ YD | 7511 | GRUNDY | 3 | 66K25 | 12 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 126 | GRUNDY | 3 | 66K25 | 12 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 160 | GRUNDY | 3 | 66K25 | 12 |
| 28000500 | INLET & PIPE PROTECT | EACH | 4 | GRUNDY | 3 | 66K25 | 12 |
| 31100910 | SUB GRAN MAT A 12 | SQ YD | 9958 | GRUNDY | 3 | 66K25 | 12 |
| 40600290 | BIT MATLS TACK CT | POUND | 42182 | GRUNDY | 3 | 66K25 | 12 |
| 40600400 | MIX CR JTS FLANGEWYS | TON | 15.9 | GRUNDY | 3 | 66K25 | 12 |
| 40600990 | TEMPORARY RAMP | SQ YD | 889 | GRUNDY | 3 | 66K25 | 12 |
| 40603085 | HMA BC IL-19.0 N70 | TON | 2737 | GRUNDY | 3 | 66K25 | 12 |
| 40603090 | HMA BC IL-19.0 N90 | TON | 5700 | GRUNDY | 3 | 66K25 | 12 |
| 40603240 | P HMA BC IL19.0 N90 | TON | 4519 | GRUNDY | 3 | 66K25 | 12 |
| 40603340 | HMA SC "D" N70 | TON | 2267 | GRUNDY | 3 | 66K25 | 12 |
| 42000521 | PCC PVT 11 JOINTED | SQ YD | 9932 | GRUNDY | 3 | 66K25 | 12 |
| 42001300 | PROTECTIVE COAT | SQ YD | 9932 | GRUNDY | 3 | 66K25 | 12 |
| 44000100 | PAVEMENT REM | SQ YD | 463 | GRUNDY | 3 | 66K25 | 12 |
| 44000157 | HMA SURF REM 2 | SQ YD | 4756 | GRUNDY | 3 | 66K25 | 12 |
| 44000166 | HMA SURF REM 4 1/4 | SQ YD | 19361 | GRUNDY | 3 | 66K25 | 12 |
| 44000173 | HMA SURF REM 6 | SQ YD | 8030 | GRUNDY | 3 | 66K25 | 12 |
| 44000184 | HMA SURF REM 8 1/2 | SQ YD | 23948 | GRUNDY | 3 | 66K25 | 12 |
| 44004250 | PAVED SHLD REMOVAL | SQ YD | 2720 | GRUNDY | 3 | 66K25 | 12 |
| 44213204 | TIE BARS 3/4 | EACH | 2372 | GRUNDY | 3 | 66K25 | 12 |
| 48101500 | AGGREGATE SHLDS B 6 | SQ YD | 762 | GRUNDY | 3 | 66K25 | 12 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 1339 | GRUNDY | 3 | 66K25 | 12 |
| 54213663 | PRC FLAR END SEC 18 | EACH | 2 | GRUNDY | 3 | 66K25 | 12 |
| 63500105 | DELINEATORS | EACH | 130 | GRUNDY | 3 | 66K25 | 12 |
| 64200116 | SHOULDER RUM STRIP 16 | FOOT | 15060 | GRUNDY | 3 | 66K25 | 12 |
| 64401100 | HT CBL MEDIAN BARRIER | FOOT | 3373 | GRUNDY | 3 | 66K25 | 12 |
| 64401300 | HT CBL MED BAR TERM | EACH | 6 | GRUNDY | 3 | 66K25 | 12 |
| 67100100 | MOBILIZATION | L SUM | 1 | GRUNDY | 3 | 66K25 | 12 |
| 70100420 | TRAF CONT-PROT 701411 | EACH | 4 | GRUNDY | 3 | 66K25 | 12 |
| 70100820 | TRAF CONT-PROT 701451 | L SUM | 1 | GRUNDY | 3 | 66K25 | 12 |
| 70100825 | TRAF CONT-PROT 701456 | L SUM | 1 | GRUNDY | 3 | 66K25 | 12 |
| 70103815 | TR CONT SURVEILLANCE | CAL DA | 10 | GRUNDY | 3 | 66K25 | 12 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 44 | GRUNDY | 3 | 66K25 | 12 |
| 70200100 | NIGHT WORK ZONE LIGHT | L SUM | 1 | GRUNDY | 3 | 66K25 | 12 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 2694 | GRUNDY | 3 | 66K25 | 12 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 299 | GRUNDY | 3 | 66K25 | 12 |
| 70300210 | TEMP PVT MK LTR & SYM | SQ FT | 97.2 | GRUNDY | 3 | 66K25 | 12 |
| 70300220 | TEMP PVT MK LINE 4 | FOOT | 55280 | GRUNDY | 3 | 66K25 | 12 |
| 70300240 | TEMP PVT MK LINE 6 | FOOT | 4520 | GRUNDY | 3 | 66K25 | 12 |
| 70300250 | TEMP PVT MK LINE 8 | FOOT | 2046 | GRUNDY | 3 | 66K25 | 12 |
| 70300280 | TEMP PVT MK LINE 24 | FOOT | 198 | GRUNDY | 3 | 66K25 | 12 |
| 72501100 | TERMINAL MARKER - PM | EACH | 5 | GRUNDY | 3 | 66K25 | 12 |
| 78003100 | PREF PL PM TB LTR-SYM | SQ FT | 48.6 | GRUNDY | 3 | 66K25 | 12 |
| 78003130 | PREF PL PM TB LINE 6 | FOOT | 2260 | GRUNDY | 3 | 66K25 | 12 |
| 78003180 | PREF PL PM TB LINE 24 | FOOT | 99 | GRUNDY | 3 | 66K25 | 12 |
| 78008310 | POLYUREA PM T2 LN 4 | FOOT | 30028 | GRUNDY | 3 | 66K25 | 12 |
| 78008340 | POLYUREA PM T2 LN 8 | FOOT | 1023 | GRUNDY | 3 | 66K25 | 12 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 402 | GRUNDY | 3 | 66K25 | 12 |
| 78300200 | RAISED REF PVT MK REM | EACH | 402 | GRUNDY | 3 | 66K25 | 12 |
| X4510100 | CRACK ROUTING/FILLING | POUND | 429349 | VARIOUS | 4 | 68F06 | 15 |
| 67100100 | MOBILIZATION | L SUM | 1 | VARIOUS | 4 | 68F06 | 15 |
| 70100460 | TRAF CONT-PROT 701306 | L SUM | 1 | VARIOUS | 4 | 68F06 | 15 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | VARIOUS | 4 | 68F06 | 15 |
| 70102622 | TR CONT & PROT 701502 | L SUM | 1 | VARIOUS | 4 | 68F06 | 15 |
| X4510100 | CRACK ROUTING/FILLING | POUND | 336978 | VARIOUS | 4 | 68F07 | 16 |
| 67100100 | MOBILIZATION | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| 70100420 | TRAF CONT-PROT 701411 | EACH | 4 | VARIOUS | 4 | 68F07 | 16 |
| 70100460 | TRAF CONT-PROT 701306 | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| 70100700 | TRAF CONT-PROT 701406 | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| 70102622 | TR CONT & PROT 701502 | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| 70102630 | TR CONT & PROT 701601 | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| 70102632 | TR CONT & PROT 701602 | L SUM | 1 | VARIOUS | 4 | 68F07 | 16 |
| XZ193400 | SURVEY MARKER T2 SPL | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0300008 | S C MAA&P DMA 42 & 24 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0300009 | RR FAC & TY V CAB IO | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0301339 | REM EX PARKING BLOCKS | EACH | 20 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0301430 | PREC CONC PARK BLOCK | EACH | 17 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0323344 | VANE DRAINS | FOOT | 24 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0325405 | FILL EX STORM SEWERS | CU YD | 21 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0326225 | PAINT NEW PED P-B PST | EACH | 44 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0326227 | PT NEW MAASSPW/2</>40 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0326266 | ETHERNET SWITCH | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0326617 | PAINT LIGHT POLE UNIT | EACH | 72 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0326885 | VIDEO DETECT SYS | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0327611 | REM & REIN BRIC PAVER | SQ FT | 843 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0327698 | LED IN IL STNAME SIGN | EACH | 4 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0327750 | FOUNDATION REM | CU YD | 42 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 1702 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0327989 | REMOVE EXSTNG BR PAV | SQ FT | 1325 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400012 | REM & REIN FIB OPT CC | FOOT | 866 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400235 | DBL HANDHOLE ADJUST | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400351 | WOOD POLE 35 CL 4 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400352 | S MMA & P 46 LT ARM15 40 MH | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400353 | S MMA & P 48 LT ARM15 40 MH | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400354 | S MMA & P 52 LT ARM15 40 MH | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400355 | S MMA & P 54 LT ARM15 40 MH | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X1400368 | REL EX PTZ CAMERA | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| X2110100 | TOPSOIL F & P SPL | CU YD | 641 | CHAMPAIGN | 5 | 70B53 | 17 |
| X4020500 | AGG SURF CSE B 6 | SQ YD | 91 | CHAMPAIGN | 5 | 70B53 | 17 |
| X4400196 | HMA SURF REM SPL | SQ YD | 3168 | CHAMPAIGN | 5 | 70B53 | 17 |
| X4402020 | CONC MEDIAN SURF REM | SQ FT | 1329 | CHAMPAIGN | 5 | 70B53 | 17 |
| X4403300 | CONC MEDIAN REMOV | SQ FT | 887 | CHAMPAIGN | 5 | 70B53 | 17 |
| X6061005 | CONC CURB TB SPL | FOOT | 487 | CHAMPAIGN | 5 | 70B53 | 17 |
| X6061702 | CONC MED TSM DOW | SQ FT | 2227 | CHAMPAIGN | 5 | 70B53 | 17 |
| X6330725 | SPBGR (SHORT RADIUS) | FOOT | 187.5 | CHAMPAIGN | 5 | 70B53 | 17 |
| X7830060 | GRV RCSD PM LTR & SYM | SQ FT | 2615 | CHAMPAIGN | 5 | 70B53 | 17 |
| X7830070 | GRV RCSD PVT MRKG 5 | FOOT | 28373 | CHAMPAIGN | 5 | 70B53 | 17 |
| X7830074 | GRV RCSD PVT MRKG 7 | FOOT | 1140 | CHAMPAIGN | 5 | 70B53 | 17 |
| X7830078 | GRV RCSD PVT MRKG 13 | FOOT | 7082 | CHAMPAIGN | 5 | 70B53 | 17 |
| X7830090 | GRV RCSD PVT MRKG 25 | FOOT | 1625 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8050115 | SERV INSTALL TY A MOD | EACH | 7 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8100105 | CONDUIT SPLICE | EACH | 17 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8140115 | HANDHOLE TO BE ADJUST | EACH | 11 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8360215 | LIGHT POLE FDN 24D OS | FOOT | 103 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8510850 | PT NEW COM MA&P SPL | EACH | 6 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8710036 | FIB OPT CBL 12F SM | FOOT | 3460 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8730320 | EC C SIGL 20 3C TW SH | FOOT | 6277 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8760200 | ACCESSIBLE PED SIGNAL | EACH | 44 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8950115 | RELOC LIGHT DET | EACH | 24 | CHAMPAIGN | 5 | 70B53 | 17 |
| X8950120 | RELOC LIGHT DET AMP | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0001110 | GAS VALVE ADJUSTED | EACH | 10 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0011500 | COLD MILL EX SURFACE | SQ YD | 117 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0033024 | MAINT EX LTG SYS | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0033700 | LONG JOINT SEALANT | FOOT | 30849 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0038119 | PCC SUR REM 1 1/2 | SQ YD | 372 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0048665 | RR PROT LIABILITY INS | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0070100 | SURV MONUMENT COV ASY | EACH | 7 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0075498 | CONC RETAIN WALL REM | CU YD | 37 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0076600 | TRAINEES | HOUR | 3000 | CHAMPAIGN | 5 | 70B53 | 17 |
| Z0076604 | TRAINEES TPG | HOUR | 3000 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20100110 | TREE REMOV 6-15 | UNIT | 68 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20100210 | TREE REMOV OVER 15 | UNIT | 324 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20101000 | TEMPORARY FENCE | FOOT | 1042 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20101100 | TREE TRUNK PROTECTION | EACH | 65 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20101200 | TREE ROOT PRUNING | EACH | 20 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20101300 | TREE PRUN 1-10 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20101350 | TREE PRUN OVER 10 | EACH | 31 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20200100 | EARTH EXCAVATION | CU YD | 1206 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20800150 | TRENCH BACKFILL | CU YD | 96 | CHAMPAIGN | 5 | 70B53 | 17 |
| 20900110 | POROUS GRAN BACKFILL | CU YD | 5 | CHAMPAIGN | 5 | 70B53 | 17 |
| 25000400 | NITROGEN FERT NUTR | POUND | 140 | CHAMPAIGN | 5 | 70B53 | 17 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 140 | CHAMPAIGN | 5 | 70B53 | 17 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 140 | CHAMPAIGN | 5 | 70B53 | 17 |
| 25200110 | SODDING SALT TOLERANT | SQ YD | 10484 | CHAMPAIGN | 5 | 70B53 | 17 |
| 25200200 | SUPPLE WATERING | UNIT | 127 | CHAMPAIGN | 5 | 70B53 | 17 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 1300 | CHAMPAIGN | 5 | 70B53 | 17 |
| 28000500 | INLET & PIPE PROTECT | EACH | 11 | CHAMPAIGN | 5 | 70B53 | 17 |
| 28000510 | INLET FILTERS | EACH | 83 | CHAMPAIGN | 5 | 70B53 | 17 |
| 35300500 | PCC BSE CSE 10 | SQ YD | 355 | CHAMPAIGN | 5 | 70B53 | 17 |
| 35300720 | PCC BSE CSE 13 | SQ YD | 108 | CHAMPAIGN | 5 | 70B53 | 17 |
| 40600290 | BIT MATLS TACK CT | POUND | 32117 | CHAMPAIGN | 5 | 70B53 | 17 |
| 40600847 | P LB MM IL-9.5FG N90 | TON | 1032 | CHAMPAIGN | 5 | 70B53 | 17 |
| 40600990 | TEMPORARY RAMP | SQ YD | 1064 | CHAMPAIGN | 5 | 70B53 | 17 |
| 40603545 | P HMA SC "D" N90 | TON | 4856 | CHAMPAIGN | 5 | 70B53 | 17 |
| 40800029 | BIT MATLS TACK CT | POUND | 1634 | CHAMPAIGN | 5 | 70B53 | 17 |
| 40800050 | INCIDENTAL HMA SURF | TON | 313 | CHAMPAIGN | 5 | 70B53 | 17 |
| 42300200 | PCC DRIVEWAY PAVT 6 | SQ YD | 2163 | CHAMPAIGN | 5 | 70B53 | 17 |
| 42300400 | PCC DRIVEWAY PAVT 8 | SQ YD | 145 | CHAMPAIGN | 5 | 70B53 | 17 |
| 42400200 | PC CONC SIDEWALK 5 | SQ FT | 91305 | CHAMPAIGN | 5 | 70B53 | 17 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 1616 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44000100 | PAVEMENT REM | SQ YD | 230 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44000155 | HMA SURF REM 1 1/2 | SQ YD | 39396 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44000159 | HMA SURF REM 2 1/2 | SQ YD | 18413 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44000200 | DRIVE PAVEMENT REM | SQ YD | 3287 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 14716 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44000600 | SIDEWALK REM | SQ FT | 65842 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44200050 | WELDED WIRE REINF | SQ YD | 167 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44200976 | CL B PATCH T4 10 | SQ YD | 167 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201299 | DOWEL BARS 1 1/2 | EACH | 100 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201385 | CL C PATCH T1 13 | SQ YD | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201389 | CL C PATCH T2 13 | SQ YD | 65 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201394 | CL C PATCH T3 13 | SQ YD | 126 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201396 | CL C PATCH T4 13 | SQ YD | 177 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201777 | CL D PATCH T2 11 | SQ YD | 203 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201781 | CL D PATCH T3 11 | SQ YD | 22 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201783 | CL D PATCH T4 11 | SQ YD | 368 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201803 | CL D PATCH T2 13 | SQ YD | 75 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44201827 | CL D PATCH T2 15 | SQ YD | 48 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44213200 | SAW CUTS | FOOT | 411 | CHAMPAIGN | 5 | 70B53 | 17 |
| 44213204 | TIE BARS 3/4 | EACH | 84 | CHAMPAIGN | 5 | 70B53 | 17 |
| 50300225 | CONC STRUCT | CU YD | 18 | CHAMPAIGN | 5 | 70B53 | 17 |
| 550A0040 | STORM SEW CL A 1 10 | FOOT | 74 | CHAMPAIGN | 5 | 70B53 | 17 |
| 550A0050 | STORM SEW CL A 1 12 | FOOT | 229 | CHAMPAIGN | 5 | 70B53 | 17 |
| 550A0380 | STORM SEW CL A 2 18 | FOOT | 18 | CHAMPAIGN | 5 | 70B53 | 17 |
| 550A2320 | SS RG CL A 1 12 | FOOT | 305 | CHAMPAIGN | 5 | 70B53 | 17 |
| 550B0070 | STORM SEW CL B 1 15 | FOOT | 28 | CHAMPAIGN | 5 | 70B53 | 17 |
| 55100300 | STORM SEWER REM 8 | FOOT | 92 | CHAMPAIGN | 5 | 70B53 | 17 |
| 55100500 | STORM SEWER REM 12 | FOOT | 160 | CHAMPAIGN | 5 | 70B53 | 17 |
| 55100900 | STORM SEWER REM 18 | FOOT | 12 | CHAMPAIGN | 5 | 70B53 | 17 |
| 55101200 | STORM SEWER REM 24 | FOOT | 6 | CHAMPAIGN | 5 | 70B53 | 17 |
| 56109210 | WATER VALVES ADJUST | EACH | 70 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60100085 | GEO FAB-FRENCH DRAIN | SQ YD | 56 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60108204 | PIPE UNDERDR T 2 4 | FOOT | 95 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60236200 | INLETS TA T8G | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60236800 | INLETS TA T11F&G | EACH | 17 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60240215 | INLETS TB T1F CL | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60240310 | INLETS TB T11F&G | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60255700 | MAN ADJ NEW T1F OL | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60260300 | INLETS ADJ NEW T1F OL | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60261300 | INLETS ADJ NEW T11F&G | EACH | 39 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60261500 | INLETS ADJ NEW T15F&L | EACH | 7 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60300105 | FR & GRATES ADJUST | EACH | 10 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60300305 | FR & LIDS ADJUST | EACH | 73 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60500060 | REMOV INLETS | EACH | 8 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60500105 | FILL MANHOLES | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60500305 | FILL INLETS | EACH | 14 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60600605 | CONC CURB TB | FOOT | 817 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60603900 | COMB CC&G TB6.12 AEP | FOOT | 9555 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60604500 | COMB CC&G TB6.18 AEP | FOOT | 2140 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60604900 | COMB CC&G TB6.18 VWGF | FOOT | 374 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60605100 | COMB CC&G TB6.24 AEP | FOOT | 1643 | CHAMPAIGN | 5 | 70B53 | 17 |
| 60605500 | COMB CC&G TB6.24 VWGF | FOOT | 397 | CHAMPAIGN | 5 | 70B53 | 17 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 287.5 | CHAMPAIGN | 5 | 70B53 | 17 |
| 63000007 | SPBGR TY B 6FT POSTS | FOOT | 87.5 | CHAMPAIGN | 5 | 70B53 | 17 |
| 63000030 | SPGR ATT TO CULVERT | FOOT | 87.5 | CHAMPAIGN | 5 | 70B53 | 17 |
| 63100045 | TRAF BAR TERM T2 | EACH | 5 | CHAMPAIGN | 5 | 70B53 | 17 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 63200310 | GUARDRAIL REMOV | FOOT | 684 | CHAMPAIGN | 5 | 70B53 | 17 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 1600 | CHAMPAIGN | 5 | 70B53 | 17 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 16 | CHAMPAIGN | 5 | 70B53 | 17 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 20 | CHAMPAIGN | 5 | 70B53 | 17 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 67000500 | ENGR FIELD OFFICE B | CAL MO | 22 | CHAMPAIGN | 5 | 70B53 | 17 |
| 67100100 | MOBILIZATION | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70102630 | TR CONT & PROT 701601 | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70102632 | TR CONT & PROT 701602 | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70103815 | TR CONT SURVEILLANCE | CAL DA | 115 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 28 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70200100 | NIGHT WORK ZONE LIGHT | L SUM | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 35640 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 5134 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300210 | TEMP PVT MK LTR & SYM | SQ FT | 2615 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300220 | TEMP PVT MK LINE 4 | FOOT | 28373 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300240 | TEMP PVT MK LINE 6 | FOOT | 1140 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300260 | TEMP PVT MK LINE 12 | FOOT | 7082 | CHAMPAIGN | 5 | 70B53 | 17 |
| 70300280 | TEMP PVT MK LINE 24 | FOOT | 1637 | CHAMPAIGN | 5 | 70B53 | 17 |
| 72501000 | TERMINAL MARKER - DA | EACH | 6 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 2490 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 27644 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78000400 | THPL PVT MK LINE 6 | FOOT | 1140 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 6682 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 1501 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78008300 | POLYUREA PM T2 LTR-SY | SQ FT | 125 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78008310 | POLYUREA PM T2 LN 4 | FOOT | 729 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78008350 | POLYUREA PM T2 LN 12 | FOOT | 400 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78008370 | POLYUREA PM T2 LN 24 | FOOT | 136 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 611 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 14 | CHAMPAIGN | 5 | 70B53 | 17 |
| 78300200 | RAISED REF PVT MK REM | EACH | 611 | CHAMPAIGN | 5 | 70B53 | 17 |
| 80400100 | ELECT SERV INSTALL | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 80500100 | SERV INSTALL TY A | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028350 | UNDRGRD C PVC 2 | FOOT | 1513 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028360 | UNDRGRD C PVC 2 1/2 | FOOT | 314 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028370 | UNDRGRD C PVC 3 | FOOT | 1400 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028390 | UNDRGRD C PVC 4 | FOOT | 985 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028400 | UNDRGRD C PVC 5 | FOOT | 369 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028410 | UNDRGRD C PVC 6 | FOOT | 36 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028750 | UNDRGRD C CNC 2 | FOOT | 3799 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81028760 | UNDRGRD C CNC 2 1/2 | FOOT | 225 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81400100 | HANDHOLE | EACH | 35 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81400300 | DBL HANDHOLE | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81500130 | GULFBOX JUNCTION REM | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81603000 | UD 2#8 #8G XLPUSE 3/4 | FOOT | 8882 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81603010 | UD 2#10#10GXLPUSE 3/4 | FOOT | 7628 | CHAMPAIGN | 5 | 70B53 | 17 |
| 81702110 | EC C XLP USE 1C 10 | FOOT | 11486 | CHAMPAIGN | 5 | 70B53 | 17 |
| 82110007 | LUM LED RDWY G | EACH | 72 | CHAMPAIGN | 5 | 70B53 | 17 |
| 82110008 | LUM LED RDWY H | EACH | 39 | CHAMPAIGN | 5 | 70B53 | 17 |
| 82500350 | LT CONT BASEM 240V100 | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 83001300 | LT P A 35MH 8DA | EACH | 49 | CHAMPAIGN | 5 | 70B53 | 17 |
| 83001600 | LT P A 35MH 15DA | EACH | 23 | CHAMPAIGN | 5 | 70B53 | 17 |
| 83600200 | LIGHT POLE FDN 24D | FOOT | 341 | CHAMPAIGN | 5 | 70B53 | 17 |
| 84200600 | REM LT U NO SALV | EACH | 47 | CHAMPAIGN | 5 | 70B53 | 17 |
| 84200804 | REM POLE FDN | EACH | 47 | CHAMPAIGN | 5 | 70B53 | 17 |
| 84500110 | REMOV LIGHTING CONTR | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 84500120 | REMOV ELECT SERV INST | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 84500130 | REMOV LTG CONTR FDN | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 85100500 | PT NEW TRAF SIG POST | EACH | 63 | CHAMPAIGN | 5 | 70B53 | 17 |
| 85100600 | PT NEW MA&P < 40FT | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 85100800 | PT NEW COM MA&P <40FT | EACH | 17 | CHAMPAIGN | 5 | 70B53 | 17 |
| 85100901 | PT NEW COM MA&P>=40FT | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| 85700200 | FAC T4 CAB | EACH | 8 | CHAMPAIGN | 5 | 70B53 | 17 |
| 86200200 | UNINTER POWER SUP STD | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87301215 | ELCBL C SIGNAL 14 2C | FOOT | 13935 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87301245 | ELCBL C SIGNAL 14 5C | FOOT | 18660 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87301255 | ELCBL C SIGNAL 14 7C | FOOT | 16356 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87301805 | ELCBL C SERV 6 2C | FOOT | 1426 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87301900 | ELCBL C EGRDC 6 1C | FOOT | 6201 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87502640 | TS POST A 10 | EACH | 21 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87502660 | TS POST A 12 | EACH | 8 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87502680 | TS POST A 14 | EACH | 17 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87502700 | TS POST A 16 | EACH | 17 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87601200 | PED P-B POST GALVS T2 | EACH | 44 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87700210 | S MAA & P 34 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702840 | STL COMB MAA&P 22 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702850 | STL COMB MAA&P 24 | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702860 | STL COMB MAA&P 26 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702870 | STL COMB MAA&P 28 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702880 | STL COMB MAA&P 30 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702890 | STL COMB MAA&P 32 | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702900 | STL COMB MAA&P 34 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702910 | STL COMB MAA&P 36 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702920 | STL COMB MAA&P 38 | EACH | 5 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702930 | STL COMB MAA&P 40 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702940 | STL COMB MAA&P 42 | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702950 | STL COMB MAA&P 44 | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702960 | STL COMB MAA&P 46 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702980 | STL COMB MAA&P 50 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702985 | STL COMB MAA&P 52 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87702990 | STL COMB MAA&P 54 | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87800100 | CONC FDN TY A | FOOT | 180 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87800150 | CONC FDN TY C | FOOT | 28 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87800400 | CONC FDN TY E 30D | FOOT | 64 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87800415 | CONC FDN TY E 36D | FOOT | 337 | CHAMPAIGN | 5 | 70B53 | 17 |
| 87900200 | DRILL EX HANDHOLE | EACH | 15 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88030100 | SH LED 1F 5S BM | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88030110 | SH LED 1F 5S MAM | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88030250 | SH LED 2F 1-4 1-5 BM | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040070 | SH P LED 1F 3S BM | EACH | 22 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040090 | SH P LED 1F 3S MAM | EACH | 73 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040110 | SH P LED 1F 4S BM | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040120 | SH P LED 1F 4S MAM | EACH | 22 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040150 | SH P LED 1F 5S BM | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040160 | SH P LED 1F 5S MAM | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040230 | SH P LED 2F 3S BM | EACH | 2 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040250 | SH P LED 2F 1-3 1-4BM | EACH | 14 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040280 | SH P LED 2F 1-4 1-5BM | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040290 | SH P LED 2F 5S BM | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88040332 | SH P LED 3F 2-3 1-4BM | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88102810 | PED SH P LED 1F BM | EACH | 10 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88102825 | PED SH P LED 1F BM CT | EACH | 66 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88200510 | TS BACKPLATE RET-REFL | EACH | 97 | CHAMPAIGN | 5 | 70B53 | 17 |
| 88800100 | PED PUSH-BUTTON | EACH | 40 | CHAMPAIGN | 5 | 70B53 | 17 |
| 89000100 | TEMP TR SIG INSTALL | EACH | 1 | CHAMPAIGN | 5 | 70B53 | 17 |
| 89502300 | REM ELCBL FR CON | FOOT | 26685 | CHAMPAIGN | 5 | 70B53 | 17 |
| 89502375 | REMOV EX TS EQUIP | EACH | 9 | CHAMPAIGN | 5 | 70B53 | 17 |
| 89502380 | REMOV EX HANDHOLE | EACH | 37 | CHAMPAIGN | 5 | 70B53 | 17 |
| 89502382 | REMOV EX DBL HANDHOLE | EACH | 3 | CHAMPAIGN | 5 | 70B53 | 17 |
| 89502385 | REMOV EX CONC FDN | EACH | 98 | CHAMPAIGN | 5 | 70B53 | 17 |
| X0326390 | CONCRETE SLAB REMOVAL | SQ YD | 12 | HANCOCK | 6 | 72J45 | 18 |
| X0327980 | PAVMT MRKG REM WTR BL | SQ FT | 1000 | HANCOCK | 6 | 72J45 | 18 |
| X1200108 | INLET BOX SPL | EACH | 1 | HANCOCK | 6 | 72J45 | 18 |
| X4201410 | BR APPR PAVT CONN SPL | SQ YD | 111 | HANCOCK | 6 | 72J45 | 18 |
| X4402720 | GUTTER REMOV SPL | FOOT | 199 | HANCOCK | 6 | 72J45 | 18 |
| X6061610 | COMB CC&G TB MOD | FOOT | 14 | HANCOCK | 6 | 72J45 | 18 |
| X6430120 | REM IMP ATTEN NO SALV | EACH | 1 | HANCOCK | 6 | 72J45 | 18 |
| X7011800 | TRAF CONT-PROT BLR 21 | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| X7011801 | TRAF CONT-PROT BLR 22 | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| Z0001900 | ASB BEARING PAD REMOV | EACH | 24 | HANCOCK | 6 | 72J45 | 18 |
| Z0003300 | BASE CSE REMOV SPL | SQ YD | 39 | HANCOCK | 6 | 72J45 | 18 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| Z0016702 | DETOUR SIGNING | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| Z0046304 | P UNDR FOR STRUCT 4 | FOOT | 128 | HANCOCK | 6 | 72J45 | 18 |
| Z0054404 | ROCK FILL - EMBANK | CU YD | 280 | HANCOCK | 6 | 72J45 | 18 |
| Z0076600 | TRAINEES | HOUR | 1000 | HANCOCK | 6 | 72J45 | 18 |
| Z0076604 | TRAINEES TPG | HOUR | 1000 | HANCOCK | 6 | 72J45 | 18 |
| 20100210 | TREE REMOV OVER 15 | UNIT | 30 | HANCOCK | 6 | 72J45 | 18 |
| 20100500 | TREE REMOV ACRES | ACRE | 0.5 | HANCOCK | 6 | 72J45 | 18 |
| 20200100 | EARTH EXCAVATION | CU YD | 165 | HANCOCK | 6 | 72J45 | 18 |
| 20200200 | ROCK EXCAVATION | CU YD | 50 | HANCOCK | 6 | 72J45 | 18 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 100 | HANCOCK | 6 | 72J45 | 18 |
| 20400800 | FURNISHED EXCAVATION | CU YD | 1370 | HANCOCK | 6 | 72J45 | 18 |
| 20800150 | TRENCH BACKFILL | CU YD | 4 | HANCOCK | 6 | 72J45 | 18 |
| 25000200 | SEEDING CL 2 | ACRE | 0.75 | HANCOCK | 6 | 72J45 | 18 |
| 25000400 | NITROGEN FERT NUTR | POUND | 68 | HANCOCK | 6 | 72J45 | 18 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 68 | HANCOCK | 6 | 72J45 | 18 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 68 | HANCOCK | 6 | 72J45 | 18 |
| 25000700 | AGR GROUND LIMESTONE | TON | 2 | HANCOCK | 6 | 72J45 | 18 |
| 25100115 | MULCH METHOD 2 | ACRE | 0.75 | HANCOCK | 6 | 72J45 | 18 |
| 25100635 | HD EROS CONTR BLANKET | SQ YD | 250 | HANCOCK | 6 | 72J45 | 18 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 150 | HANCOCK | 6 | 72J45 | 18 |
| 28000400 | PERIMETER EROS BAR | FOOT | 775 | HANCOCK | 6 | 72J45 | 18 |
| 28100209 | STONE RIPRAP CL A5 | TON | 482 | HANCOCK | 6 | 72J45 | 18 |
| 28100807 | STONE DUMP RIP CL A4 | TON | 282 | HANCOCK | 6 | 72J45 | 18 |
| 28200200 | FILTER FABRIC | SQ YD | 829 | HANCOCK | 6 | 72J45 | 18 |
| 31101000 | SUB GRAN MAT B | TON | 78 | HANCOCK | 6 | 72J45 | 18 |
| 35100100 | AGG BASE CSE A | TON | 251 | HANCOCK | 6 | 72J45 | 18 |
| 35101400 | AGG BASE CSE B | TON | 69 | HANCOCK | 6 | 72J45 | 18 |
| 35600716 | HMA BC WID 10 | SQ YD | 131 | HANCOCK | 6 | 72J45 | 18 |
| 40600275 | BIT MATLS PR CT | POUND | 160 | HANCOCK | 6 | 72J45 | 18 |
| 40600290 | BIT MATLS TACK CT | POUND | 548 | HANCOCK | 6 | 72J45 | 18 |
| 40600982 | HMA SURF REM BUTT JT | SQ YD | 210 | HANCOCK | 6 | 72J45 | 18 |
| 40600990 | TEMPORARY RAMP | SQ YD | 70 | HANCOCK | 6 | 72J45 | 18 |
| 40603080 | HMA BC IL-19.0 N50 | TON | 289 | HANCOCK | 6 | 72J45 | 18 |
| 40603310 | HMA SC "C" N50 | TON | 156 | HANCOCK | 6 | 72J45 | 18 |
| 44000100 | PAVEMENT REM | SQ YD | 215 | HANCOCK | 6 | 72J45 | 18 |
| 44000200 | DRIVE PAVEMENT REM | SQ YD | 314 | HANCOCK | 6 | 72J45 | 18 |
| 44000400 | GUTTER REM | FOOT | 260 | HANCOCK | 6 | 72J45 | 18 |
| 44004250 | PAVED SHLD REMOVAL | SQ YD | 312 | HANCOCK | 6 | 72J45 | 18 |
| 48101200 | AGGREGATE SHLDS B | TON | 21 | HANCOCK | 6 | 72J45 | 18 |
| 48203029 | HMA SHOULDERS 8 | SQ YD | 222 | HANCOCK | 6 | 72J45 | 18 |
| 48203100 | HMA SHOULDERS | TON | 61 | HANCOCK | 6 | 72J45 | 18 |
| 50100100 | REM EXIST STRUCT | EACH | 1 | HANCOCK | 6 | 72J45 | 18 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 24 | HANCOCK | 6 | 72J45 | 18 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 16 | HANCOCK | 6 | 72J45 | 18 |
| 50200400 | ROCK EXC STRUCT | CU YD | 90 | HANCOCK | 6 | 72J45 | 18 |
| 50300225 | CONC STRUCT | CU YD | 73.7 | HANCOCK | 6 | 72J45 | 18 |
| 50300255 | CONC SUP-STR | CU YD | 209.3 | HANCOCK | 6 | 72J45 | 18 |
| 50300260 | BR DECK GROOVING | SQ YD | 633 | HANCOCK | 6 | 72J45 | 18 |
| 50300300 | PROTECTIVE COAT | SQ YD | 972 | HANCOCK | 6 | 72J45 | 18 |
| 50301350 | CONC SUPSTR APP SLAB | CU YD | 95.1 | HANCOCK | 6 | 72J45 | 18 |
| 50500105 | F & E STRUCT STEEL | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| 50500505 | STUD SHEAR CONNECTORS | EACH | 1170 | HANCOCK | 6 | 72J45 | 18 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 97650 | HANCOCK | 6 | 72J45 | 18 |
| 51500100 | NAME PLATES | EACH | 1 | HANCOCK | 6 | 72J45 | 18 |
| 51603000 | DRILLED SHAFT IN SOIL | CU YD | 6.3 | HANCOCK | 6 | 72J45 | 18 |
| 51604000 | DRILLED SHAFT IN ROCK | CU YD | 19.7 | HANCOCK | 6 | 72J45 | 18 |
| 52100010 | ELAST BEARING ASSY T1 | EACH | 6 | HANCOCK | 6 | 72J45 | 18 |
| 52100520 | ANCHOR BOLTS 1 | EACH | 24 | HANCOCK | 6 | 72J45 | 18 |
| 54262712 | METAL FL END SEC 12" | EACH | 2 | HANCOCK | 6 | 72J45 | 18 |
| 550A0050 | STORM SEW CL A 1 12 | FOOT | 94 | HANCOCK | 6 | 72J45 | 18 |
| 58600101 | GRANULAR BACKFILL STR | CU YD | 156 | HANCOCK | 6 | 72J45 | 18 |
| 59100100 | GEOCOMPOSITE WALL DR | SQ YD | 93 | HANCOCK | 6 | 72J45 | 18 |
| 60100060 | CONC HDWL FOR P DRAIN | EACH | 2 | HANCOCK | 6 | 72J45 | 18 |
| 60100945 | PIPE DRAINS 12 | FOOT | 24 | HANCOCK | 6 | 72J45 | 18 |
| 60240301 | INLETS TB T8G | EACH | 1 | HANCOCK | 6 | 72J45 | 18 |
| 60500060 | REMOV INLETS | EACH | 1 | HANCOCK | 6 | 72J45 | 18 |
| 60600095 | CLASS SI CONC OUTLET | CU YD | 1.9 | HANCOCK | 6 | 72J45 | 18 |
| 60602800 | CONC GUTTER TB | FOOT | 111 | HANCOCK | 6 | 72J45 | 18 |
| 60603100 | CONC GUTTER TRANS | FOOT | 30 | HANCOCK | 6 | 72J45 | 18 |
| 61000335 | TY G INLET BOX 610001 | EACH | 3 | HANCOCK | 6 | 72J45 | 18 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 137.5 | HANCOCK | 6 | 72J45 | 18 |
| 63100085 | TRAF BAR TERM T6 | EACH | 4 | HANCOCK | 6 | 72J45 | 18 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 4 | HANCOCK | 6 | 72J45 | 18 |
| 63200310 | GUARDRAIL REMOV | FOOT | 387 | HANCOCK | 6 | 72J45 | 18 |
| 66600105 | FUR ERECT ROW MARKERS | EACH | 5 | HANCOCK | 6 | 72J45 | 18 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 12 | HANCOCK | 6 | 72J45 | 18 |
| 67100100 | MOBILIZATION | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | HANCOCK | 6 | 72J45 | 18 |
| 70103815 | TR CONT SURVEILLANCE | CAL DA | 10 | HANCOCK | 6 | 72J45 | 18 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 300 | HANCOCK | 6 | 72J45 | 18 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 112 | HANCOCK | 6 | 72J45 | 18 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 192 | HANCOCK | 6 | 72J45 | 18 |
| 70300230 | TEMP PVT MK LINE 5 | FOOT | 3000 | HANCOCK | 6 | 72J45 | 18 |
| 72501000 | TERMINAL MARKER - DA | EACH | 4 | HANCOCK | 6 | 72J45 | 18 |
| 78001120 | PAINT PVT MK LINE 5 | FOOT | 1150 | HANCOCK | 6 | 72J45 | 18 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 15 | HANCOCK | 6 | 72J45 | 18 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 9 | HANCOCK | 6 | 72J45 | 18 |
| 78300200 | RAISED REF PVT MK REM | EACH | 15 | HANCOCK | 6 | 72J45 | 18 |
| X0325231 | CABLE GUARD MARKER | EACH | 200 | VARIOUS | 6 | 72K06 | 19 |
| X0325899 | REP HTC (GIBRALTAR) | FOOT | 20 | VARIOUS | 6 | 72K06 | 19 |
| X0325900 | R HT TERM (GIBRALTAR) | EACH | 5 | VARIOUS | 6 | 72K06 | 19 |
| X0325901 | REP POSTS (GIBRALTAR) | EACH | 100 | VARIOUS | 6 | 72K06 | 19 |
| X0325902 | R&R POSTS (GIBRALTAR) | EACH | 200 | VARIOUS | 6 | 72K06 | 19 |
| X0327490 | REP HIGH TC NUCABLE | FOOT | 20 | VARIOUS | 6 | 72K06 | 19 |
| X0327491 | REPAIR POST NUCABLE | EACH | 20 | VARIOUS | 6 | 72K06 | 19 |
| X0327492 | REM REPL POST NUCABLE | EACH | 335 | VARIOUS | 6 | 72K06 | 19 |
| X0327493 | REP HT B TERM NUCABLE | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| X6300155 | SPBGR ATT TO STR SPL | FOOT | 50 | VARIOUS | 6 | 72K06 | 19 |
| X6431220 | REM REPL IMP ATTEN SM | EACH | 45 | VARIOUS | 6 | 72K06 | 19 |
| X7011834 | TC-PROT CALL OUT WORK | EACH | 45 | VARIOUS | 6 | 72K06 | 19 |
| X7011836 | TC-PROT XPWY CALL OUT | EACH | 30 | VARIOUS | 6 | 72K06 | 19 |
| Z0008759 | CALL OUT | EACH | 5 | VARIOUS | 6 | 72K06 | 19 |
| Z0008760 | EMER WORK CALL OUT | EACH | 35 | VARIOUS | 6 | 72K06 | 19 |
| Z0052000 | REPAIR SPBGR TY A | FOOT | 2300 | VARIOUS | 6 | 72K06 | 19 |
| Z0052410 | REPAIR TRBT T1 SP TAN | EACH | 60 | VARIOUS | 6 | 72K06 | 19 |
| Z0052415 | REPAIR TRBT T1 SP FLR | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| Z0052600 | REPAIR TR BAR TERM T2 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| Z0053000 | REPAIR TR BAR TERM T5 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| Z0053200 | REPAIR TR BAR TERM T6 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| Z0076604 | TRAINEES TPG | HOUR | 500 | VARIOUS | 6 | 72K06 | 19 |
| 63000001 | SPBGR TY A 6FT POSTS | FOOT | 300 | VARIOUS | 6 | 72K06 | 19 |
| 63000003 | SPBGR TY A 9FT POSTS | FOOT | 100 | VARIOUS | 6 | 72K06 | 19 |
| 63000030 | SPGR ATT TO CULVERT | FOOT | 50 | VARIOUS | 6 | 72K06 | 19 |
| 63100045 | TRAF BAR TERM T2 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| 63100070 | TRAF BAR TERM T5 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| 63100085 | TRAF BAR TERM T6 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| 63100167 | TR BAR TRM T1 SPL TAN | EACH | 22 | VARIOUS | 6 | 72K06 | 19 |
| 63100169 | TR BAR TRM T1 SPL FLR | EACH | 1 | VARIOUS | 6 | 72K06 | 19 |
| 63200310 | GUARDRAIL REMOV | FOOT | 1200 | VARIOUS | 6 | 72K06 | 19 |
| 64300450 | IMP ATTEN NRD TL3 | EACH | 1 | VARIOUS | 6 | 72K06 | 19 |
| 64401300 | HT CBL MED BAR TERM | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| 66400105 | CH LK FENCE 4 | FOOT | 100 | VARIOUS | 6 | 72K06 | 19 |
| 66500105 | WOV W FENCE 4 | FOOT | 1800 | VARIOUS | 6 | 72K06 | 19 |
| 67100100 | MOBILIZATION | L SUM | 1 | VARIOUS | 6 | 72K06 | 19 |
| 70100420 | TRAF CONT-PROT 701411 | EACH | 2 | VARIOUS | 6 | 72K06 | 19 |
| 72501000 | TERMINAL MARKER - DA | EACH | 35 | VARIOUS | 6 | 72K06 | 19 |
| 78200005 | GRDRAIL REF TYPE A | EACH | 75 | VARIOUS | 6 | 72K06 | 19 |
| X0301430 | PREC CONC PARK BLOCK | EACH | 12 | MONTGOMERY | 6 | 72L08 | 20 |
| X0322135 | BOLLARD QUICK RELEASE | EACH | 1 | MONTGOMERY | 6 | 72L08 | 20 |
| X0322330 | HANDICAP SIGN | EACH | 2 | MONTGOMERY | 6 | 72L08 | 20 |
| Z0004002 | BOLLARDS | EACH | 2 | MONTGOMERY | 6 | 72L08 | 20 |
| 20200100 | EARTH EXCAVATION | CU YD | 349 | MONTGOMERY | 6 | 72L08 | 20 |
| 28000400 | PERIMETER EROS BAR | FOOT | 2500 | MONTGOMERY | 6 | 72L08 | 20 |
| 31101180 | SUB GRAN MAT B 2 | SQ YD | 1062 | MONTGOMERY | 6 | 72L08 | 20 |
| 31101400 | SUB GRAN MAT B 6 | SQ YD | 1338 | MONTGOMERY | 6 | 72L08 | 20 |
| 42000100 | PCC PVT 6 | SQ YD | 1338 | MONTGOMERY | 6 | 72L08 | 20 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 9550 | MONTGOMERY | 6 | 72L08 | 20 |
| 48102100 | AGG WEDGE SHLD TYPE B | TON | 165 | MONTGOMERY | 6 | 72L08 | 20 |
| 542A0223 | P CUL CL A 1 18 | FOOT | 44 | MONTGOMERY | 6 | 72L08 | 20 |
| 54213663 | PRC FLAR END SEC 18 | EACH | 2 | MONTGOMERY | 6 | 72L08 | 20 |
| 67100100 | MOBILIZATION | L SUM | 1 | MONTGOMERY | 6 | 72L08 | 20 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | MONTGOMERY | 6 | 72L08 | 20 |
| 78001100 | PT PVT MK LTRS & SYMB | SQ FT | 52 | MONTGOMERY | 6 | 72L08 | 20 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 610 | MONTGOMERY | 6 | 72L08 | 20 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | CHRISTIAN | 6 | 72L34 | 21 |
| 44201377 | CL C PATCH T2 12 | SQ YD | 392 | CHRISTIAN | 6 | 72L34 | 21 |
| 44201381 | CL C PATCH T3 12 | SQ YD | 140 | CHRISTIAN | 6 | 72L34 | 21 |
| 44201383 | CL C PATCH T4 12 | SQ YD | 75 | CHRISTIAN | 6 | 72L34 | 21 |
| 44201415 | CL C PATCH T2 15 | SQ YD | 64 | CHRISTIAN | 6 | 72L34 | 21 |
| 44201419 | CL C PATCH T3 15 | SQ YD | 60 | CHRISTIAN | 6 | 72L34 | 21 |
| 44201421 | CL C PATCH T4 15 | SQ YD | 75 | CHRISTIAN | 6 | 72L34 | 21 |
| 67100100 | MOBILIZATION | L SUM | 1 | CHRISTIAN | 6 | 72L34 | 21 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | CHRISTIAN | 6 | 72L34 | 21 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | CHRISTIAN | 6 | 72L34 | 21 |
| X4406625 | PART DEP REM T4 2.5 | SQ YD | 22507 | SANGAMON | 6 | 72L35 | 22 |
| X4421000 | PARTIAL DEPTH PATCH | TON | 3151 | SANGAMON | 6 | 72L35 | 22 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | SANGAMON | 6 | 72L35 | 22 |
| Z0076604 | TRAINEES TPG | HOUR | 500 | SANGAMON | 6 | 72L35 | 22 |
| 67100100 | MOBILIZATION | L SUM | 1 | SANGAMON | 6 | 72L35 | 22 |
| 70100820 | TRAF CONT-PROT 701451 | L SUM | 1 | SANGAMON | 6 | 72L35 | 22 |
| 70102630 | TR CONT & PROT 701601 | L SUM | 1 | SANGAMON | 6 | 72L35 | 22 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 74 | SANGAMON | 6 | 72L35 | 22 |
| 70200100 | NIGHT WORK ZONE LIGHT | L SUM | 1 | SANGAMON | 6 | 72L35 | 22 |
| 70300100 | SHORT TERM PAVT MKING | FOOT | 1720 | SANGAMON | 6 | 72L35 | 22 |
| 70300150 | SHRT TRM PAVT MK REM | SQ FT | 573 | SANGAMON | 6 | 72L35 | 22 |
| 78009005 | MOD URETH PM LINE 5 | FOOT | 14888 | SANGAMON | 6 | 72L35 | 22 |
| 78009006 | MOD URETH PM LINE 6 | FOOT | 1324 | SANGAMON | 6 | 72L35 | 22 |
| 78009024 | MOD URETH PM LINE 24 | FOOT | 336 | SANGAMON | 6 | 72L35 | 22 |
| 78300200 | RAISED REF PVT MK REM | EACH | 194 | SANGAMON | 6 | 72L35 | 22 |
| X0327979 | PAVMT MRKG REM GRIND | SQ FT | 1861 | MADISON | 8 | 76J86 | 26 |
| X1400031 | REM PED PUSH-BUTTON | EACH | 1 | MADISON | 8 | 76J86 | 26 |
| X6660445 | ROW/PROPERTY CORNERS | EACH | 12 | MADISON | 8 | 76J86 | 26 |
| X7030005 | TEMP PAVT MKING REMOV | SQ FT | 1629 | MADISON | 8 | 76J86 | 26 |
| X7800100 | PT PVT MK- RAISED MED | SQ FT | 86 | MADISON | 8 | 76J86 | 26 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | MADISON | 8 | 76J86 | 26 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 2209 | MADISON | 8 | 76J86 | 26 |
| 42400800 | DETECTABLE WARNINGS | SQ FT | 383 | MADISON | 8 | 76J86 | 26 |
| 44000100 | PAVEMENT REM | SQ YD | 5 | MADISON | 8 | 76J86 | 26 |
| 44000500 | COMB CURB GUTTER REM | FOOT | 401 | MADISON | 8 | 76J86 | 26 |
| 44000600 | SIDEWALK REM | SQ FT | 2209 | MADISON | 8 | 76J86 | 26 |
| 44003100 | MEDIAN REMOVAL | SQ FT | 462 | MADISON | 8 | 76J86 | 26 |
| 44200050 | WELDED WIRE REINF | SQ YD | 4 | MADISON | 8 | 76J86 | 26 |
| 44201003 | CL B PATCH T1 13 | SQ YD | 4 | MADISON | 8 | 76J86 | 26 |
| 44201299 | DOWEL BARS 1 1/2 | EACH | 50 | MADISON | 8 | 76J86 | 26 |
| 44213200 | SAW CUTS | FOOT | 30 | MADISON | 8 | 76J86 | 26 |
| 60603500 | COMB CC&G TB6.06 | FOOT | 81 | MADISON | 8 | 76J86 | 26 |
| 60605000 | COMB CC&G TB6.24 | FOOT | 528 | MADISON | 8 | 76J86 | 26 |
| 60618300 | CONC MEDIAN SURF 4 | SQ FT | 594 | MADISON | 8 | 76J86 | 26 |
| 66900105 | UNDERGR STOR TANK REM | EACH | 1 | MADISON | 8 | 76J86 | 26 |
| 66900200 | NON SPL WASTE DISPOSL | CU YD | 55 | MADISON | 8 | 76J86 | 26 |
| 66900530 | SOIL DISPOSAL ANALY | EACH | 4 | MADISON | 8 | 76J86 | 26 |
| 66901001 | REG SUB P-CONST PLAN | LSUM | 1 | MADISON | 8 | 76J86 | 26 |
| 66901002 | ON-SITE MON REG SUB | CAL DA | 1 | MADISON | 8 | 76J86 | 26 |
| 66901003 | REG SUB F CON REPORT | LSUM | 1 | MADISON | 8 | 76J86 | 26 |
| 67000400 | ENGR FIELD OFFICE A | CAL MO | 6 | MADISON | 8 | 76J86 | 26 |
| 67100100 | MOBILIZATION | L SUM | 1 | MADISON | 8 | 76J86 | 26 |
| 70102620 | TR CONT & PROT 701501 | L SUM | 1 | MADISON | 8 | 76J86 | 26 |
| 70102632 | TR CONT & PROT 701602 | L SUM | 1 | MADISON | 8 | 76J86 | 26 |
| 70102635 | TR CONT & PROT 701701 | L SUM | 1 | MADISON | 8 | 76J86 | 26 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | MADISON | 8 | 76J86 | 26 |
| 70103815 | TR CONT SURVEILLANCE | CAL DA | 180 | MADISON | 8 | 76J86 | 26 |
| 70300220 | TEMP PVT MK LINE 4 | FOOT | 140 | MADISON | 8 | 76J86 | 26 |
| 70300250 | TEMP PVT MK LINE 8 | FOOT | 369 | MADISON | 8 | 76J86 | 26 |
| 70300260 | TEMP PVT MK LINE 12 | FOOT | 1605 | MADISON | 8 | 76J86 | 26 |
| 70300280 | TEMP PVT MK LINE 24 | FOOT | 12 | MADISON | 8 | 76J86 | 26 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 140 | MADISON | 8 | 76J86 | 26 |
| 78000500 | THPL PVT MK LINE 8 | FOOT | 369 | MADISON | 8 | 76J86 | 26 |
| 78000650 | THPL PVT MK LINE 24 | FOOT | 1296 | MADISON | 8 | 76J86 | 26 |
| 78001100 | PT PVT MK LTRS & SYMB | SQ FT | 43 | MADISON | 8 | 76J86 | 26 |
| 78100100 | RAISED REFL PAVT MKR | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 78200020 | CURB REFLECTORS | EACH | 35 | MADISON | 8 | 76J86 | 26 |
| 78300200 | RAISED REF PVT MK REM | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 81028340 | UNDRGRD C PVC 1 1/2 | FOOT | 131 | MADISON | 8 | 76J86 | 26 |
| 87301215 | ELCBL C SIGNAL 14 2C | FOOT | 479 | MADISON | 8 | 76J86 | 26 |
| 87301225 | ELCBL C SIGNAL 14 3C | FOOT | 1006 | MADISON | 8 | 76J86 | 26 |
| 87502640 | TS POST A 10 | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 87600100 | PED PUSH-BUT POST T1 | EACH | 4 | MADISON | 8 | 76J86 | 26 |
| 87800100 | CONC FDN TY A | FOOT | 9 | MADISON | 8 | 76J86 | 26 |
| 87900200 | DRILL EX HANDHOLE | EACH | 6 | MADISON | 8 | 76J86 | 26 |
| 88102810 | PED SH P LED 1F BM | EACH | 3 | MADISON | 8 | 76J86 | 26 |
| 88102850 | PED SH P LED 3F BM | EACH | 1 | MADISON | 8 | 76J86 | 26 |
| 88800100 | PED PUSH-BUTTON | EACH | 6 | MADISON | 8 | 76J86 | 26 |
| 89500100 | RELOC EX SIG HEAD | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 89500400 | RELOC EX PED PUSH-BUT | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 89502200 | MOD EX CONTR | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 89502210 | MOD EX CONTR CAB | EACH | 2 | MADISON | 8 | 76J86 | 26 |
| 89502350 | REM & RE ELCBL FR CON | FOOT | 4276 | MADISON | 8 | 76J86 | 26 |
| 89502376 | REBUILD EX HANDHOLE | EACH | 3 | MADISON | 8 | 76J86 | 26 |
| 89502385 | REMOV EX CONC FDN | EACH | 1 | MADISON | 8 | 76J86 | 26 |
| K1005421 | SEEDING SPL | ACRE | 0.25 | JERSEY | 8 | 76L56 | 27 |
| XX009289 | TRAF CONT-PROT BLR 21 | L SUM | 1 | JERSEY | 8 | 76L56 | 27 |
| X0200007 | C R HES PCC PVT 12 | SQ YD | 1858 | JERSEY | 8 | 76L56 | 27 |
| X0327108 | RELOC FERRY DOCKS | EACH | 3 | JERSEY | 8 | 76L56 | 27 |
| X0900083 | PERM ST SHT PILE SPL | SQ FT | 11534 | JERSEY | 8 | 76L56 | 27 |
| X0900084 | CONC SSTR AP SLB SPL | CU YD | 192.6 | JERSEY | 8 | 76L56 | 27 |
| X2300020 | CABLE RD GD 1 STR SPL | FOOT | 1537 | JERSEY | 8 | 76L56 | 27 |
| X5012502 | CONC REM SPEC | CU YD | 68 | JERSEY | 8 | 76L56 | 27 |
| X7010216 | TRAF CONT & PROT SPL | L SUM | 1 | JERSEY | 8 | 76L56 | 27 |
| X7030005 | TEMP PAVT MKING REMOV | SQ FT | 373 | JERSEY | 8 | 76L56 | 27 |
| Z0013798 | CONSTRUCTION LAYOUT | L SUM | 1 | JERSEY | 8 | 76L56 | 27 |
| Z0054406 | ROCK FILL - FOUNDATN | CU YD | 112 | JERSEY | 8 | 76L56 | 27 |
| Z0062456 | TEMP PAVEMENT | SQ YD | 195 | JERSEY | 8 | 76L56 | 27 |
| Z0076600 | TRAINEES | HOUR | 1000 | JERSEY | 8 | 76L56 | 27 |
| Z0076604 | TRAINEES TPG | HOUR | 1000 | JERSEY | 8 | 76L56 | 27 |
| 20101000 | TEMPORARY FENCE | FOOT | 606 | JERSEY | 8 | 76L56 | 27 |
| 20200100 | EARTH EXCAVATION | CU YD | 1080 | JERSEY | 8 | 76L56 | 27 |
| 20201200 | REM & DISP UNS MATL | CU YD | 140 | JERSEY | 8 | 76L56 | 27 |
| 20300100 | CHANNEL EXCAVATION | CU YD | 5200 | JERSEY | 8 | 76L56 | 27 |
| 20800150 | TRENCH BACKFILL | CU YD | 116 | JERSEY | 8 | 76L56 | 27 |
| 25000400 | NITROGEN FERT NUTR | POUND | 20 | JERSEY | 8 | 76L56 | 27 |
| 25000500 | PHOSPHORUS FERT NUTR | POUND | 20 | JERSEY | 8 | 76L56 | 27 |
| 25000600 | POTASSIUM FERT NUTR | POUND | 20 | JERSEY | 8 | 76L56 | 27 |
| 25100115 | MULCH METHOD 2 | ACRE | 0.25 | JERSEY | 8 | 76L56 | 27 |
| 25100900 | TURF REINF MAT | SQ YD | 164 | JERSEY | 8 | 76L56 | 27 |
| 28000250 | TEMP EROS CONTR SEED | POUND | 30 | JERSEY | 8 | 76L56 | 27 |
| 28000305 | TEMP DITCH CHECKS | FOOT | 48 | JERSEY | 8 | 76L56 | 27 |
| 28000400 | PERIMETER EROS BAR | FOOT | 407 | JERSEY | 8 | 76L56 | 27 |
| 28100107 | STONE RIPRAP CL A4 | SQ YD | 136 | JERSEY | 8 | 76L56 | 27 |
| 28200200 | FILTER FABRIC | SQ YD | 136 | JERSEY | 8 | 76L56 | 27 |
| 31100300 | SUB GRAN MAT A 4 | SQ YD | 2041 | JERSEY | 8 | 76L56 | 27 |
| 31100700 | SUB GRAN MAT A 8 | SQ YD | 643 | JERSEY | 8 | 76L56 | 27 |
| 40201000 | AGGREGATE-TEMP ACCESS | TON | 35 | JERSEY | 8 | 76L56 | 27 |
| 40600275 | BIT MATLS PR CT | POUND | 1176 | JERSEY | 8 | 76L56 | 27 |
| 40603085 | HMA BC IL-19.0 N70 | TON | 279 | JERSEY | 8 | 76L56 | 27 |
| 40603340 | HMA SC "D" N70 | TON | 1027 | JERSEY | 8 | 76L56 | 27 |
| 40700100 | BIT MATLS TACK CT | POUND | 4078 | JERSEY | 8 | 76L56 | 27 |
| 42100615 | PAVT REINFORCEMENT | SQ YD | 1858 | JERSEY | 8 | 76L56 | 27 |
| 42101300 | PROTECTIVE COAT | SQ YD | 2285 | JERSEY | 8 | 76L56 | 27 |
| 42300400 | PCC DRIVEWAY PAVT 8 | SQ YD | 22 | JERSEY | 8 | 76L56 | 27 |
| 42400100 | PC CONC SIDEWALK 4 | SQ FT | 460 | JERSEY | 8 | 76L56 | 27 |
| 44000100 | PAVEMENT REM | SQ YD | 2255 | JERSEY | 8 | 76L56 | 27 |
| 44000157 | HMA SURF REM 2 | SQ YD | 8543 | JERSEY | 8 | 76L56 | 27 |
| 44000600 | SIDEWALK REM | SQ FT | 462 | JERSEY | 8 | 76L56 | 27 |
| 44004000 | PAVED DITCH REMOVAL | FOOT | 62 | JERSEY | 8 | 76L56 | 27 |
| 48100100 | AGGREGATE SHLDS A | TON | 11 | JERSEY | 8 | 76L56 | 27 |
| 48203045 | HMA SHOULDERS 12 | SQ YD | 160 | JERSEY | 8 | 76L56 | 27 |
| 50104400 | CONC HDWL REM | EACH | 1 | JERSEY | 8 | 76L56 | 27 |
| 50105220 | PIPE CULVERT REMOV | FOOT | 19 | JERSEY | 8 | 76L56 | 27 |
| 50200100 | STRUCTURE EXCAVATION | CU YD | 104 | JERSEY | 8 | 76L56 | 27 |
| 50300225 | CONC STRUCT | CU YD | 56.6 | JERSEY | 8 | 76L56 | 27 |
| 50500505 | STUD SHEAR CONNECTORS | EACH | 112 | JERSEY | 8 | 76L56 | 27 |
| 50800105 | REINFORCEMENT BARS | POUND | 62 | JERSEY | 8 | 76L56 | 27 |
| 50800205 | REINF BARS, EPOXY CTD | POUND | 80450 | JERSEY | 8 | 76L56 | 27 |
| 50901760 | PIPE HANDRAIL | FOOT | 21 | JERSEY | 8 | 76L56 | 27 |
| 51201610 | FUR STL PILE HP12X63 | FOOT | 455 | JERSEY | 8 | 76L56 | 27 |
| 51202305 | DRIVING PILES | FOOT | 455 | JERSEY | 8 | 76L56 | 27 |
| 51203610 | TEST PILE ST HP12X63 | EACH | 2 | JERSEY | 8 | 76L56 | 27 |
| 51204650 | PILE SHOES | EACH | 16 | JERSEY | 8 | 76L56 | 27 |
| 542A1099 | P CUL CL A 2 54 | FOOT | 17 | JERSEY | 8 | 76L56 | 27 |
| 54248510 | CONCRETE COLLAR | CU YD | 1.4 | JERSEY | 8 | 76L56 | 27 |
| 54261254 | CONC ES 542001 54 1:2 | EACH | 1 | JERSEY | 8 | 76L56 | 27 |
| 60600095 | CLASS SI CONC OUTLET | CU YD | 4.7 | JERSEY | 8 | 76L56 | 27 |
| 60602500 | CONC GUTTER TA | FOOT | 127 | JERSEY | 8 | 76L56 | 27 |
| 63200400 | CABLE ROAD GD REM | FOOT | 1595 | JERSEY | 8 | 76L56 | 27 |
| 67100100 | MOBILIZATION | L SUM | 1 | JERSEY | 8 | 76L56 | 27 |
| 70100450 | TRAF CONT-PROT 701201 | L SUM | 1 | JERSEY | 8 | 76L56 | 27 |
| 70102640 | TR CONT & PROT 701801 | L SUM | 1 | JERSEY | 8 | 76L56 | 27 |
| 70107005 | PAVT MK BLKOUT TAPE 5 | FOOT | 720 | JERSEY | 8 | 76L56 | 27 |
| 70107025 | CHANGEABLE MESSAGE SN | CAL DA | 110 | JERSEY | 8 | 76L56 | 27 |
| 70300520 | PAVT MARK TAPE T3 4 | FOOT | 1120 | JERSEY | 8 | 76L56 | 27 |
| 72000100 | SIGN PANEL T1 | SQ FT | 2 | JERSEY | 8 | 76L56 | 27 |
| 72400100 | REMOV SIN PAN ASSY TA | EACH | 2 | JERSEY | 8 | 76L56 | 27 |
| 72400710 | RELOC SIGN PANEL T1 | SQ FT | 55 | JERSEY | 8 | 76L56 | 27 |
| 72800100 | TELES STL SIN SUPPORT | FOOT | 137 | JERSEY | 8 | 76L56 | 27 |
| 78000100 | THPL PVT MK LTR & SYM | SQ FT | 98 | JERSEY | 8 | 76L56 | 27 |
| 78000200 | THPL PVT MK LINE 4 | FOOT | 3715 | JERSEY | 8 | 76L56 | 27 |
| 78000500 | THPL PVT MK LINE 8 | FOOT | 104 | JERSEY | 8 | 76L56 | 27 |
| 78000600 | THPL PVT MK LINE 12 | FOOT | 552 | JERSEY | 8 | 76L56 | 27 |
| 78001100 | PT PVT MK LTRS & SYMB | SQ FT | 20 | JERSEY | 8 | 76L56 | 27 |
| 78001110 | PAINT PVT MK LINE 4 | FOOT | 274 | JERSEY | 8 | 76L56 | 27 |
| 78001140 | PAINT PVT MK LINE 8 | FOOT | 405 | JERSEY | 8 | 76L56 | 27 |
| 78001150 | PAINT PVT MK LINE 12 | FOOT | 42 | JERSEY | 8 | 76L56 | 27 |
| 80300100 | LOCATE UNDERGR CABLE | FOOT | 761 | JERSEY | 8 | 76L56 | 27 |
| 81028750 | UNDRGRD C CNC 2 | FOOT | 1087 | JERSEY | 8 | 76L56 | 27 |
| 81603010 | UD 2#10#10GXLPUSE 3/4 | FOOT | 565 | JERSEY | 8 | 76L56 | 27 |
| 81603063 | UD 4#10 #10GXLP 1P | FOOT | 560 | JERSEY | 8 | 76L56 | 27 |
| 82110008 | LUM LED RDWY H | EACH | 14 | JERSEY | 8 | 76L56 | 27 |
| 82500430 | LT CONT WM 240V 100A | EACH | 1 | JERSEY | 8 | 76L56 | 27 |
| 83060400 | LT P GS 45MH 4MA | EACH | 1 | JERSEY | 8 | 76L56 | 27 |
| 83060440 | LT P GS 45MH 12MA | EACH | 3 | JERSEY | 8 | 76L56 | 27 |
| 83060441 | LT P GS 45MH 12MA-TW | EACH | 4 | JERSEY | 8 | 76L56 | 27 |
| 83060442 | LT P GS 45MH 12 4MATW | EACH | 1 | JERSEY | 8 | 76L56 | 27 |
| 83600358 | LP F M 15BC 8 5/8X8 | EACH | 9 | JERSEY | 8 | 76L56 | 27 |
| 84200600 | REM LT U NO SALV | EACH | 7 | JERSEY | 8 | 76L56 | 27 |
| 84200804 | REM POLE FDN | EACH | 7 | JERSEY | 8 | 76L56 | 27 |
| 84500110 | REMOV LIGHTING CONTR | EACH | 1 | JERSEY | 8 | 76L56 | 27 |
| AR108084 | 1/C #4 XLP-USE | L.F. | 6551 | COLES | 7 | CO067 | 004A |
| AR108108 | 1/C #8 5 KV UG CABLE | L.F. | 4017 | COLES | 7 | CO067 | 004A |
| AR108158 | 1/C #8 5 KV UG CABLE IN UD | L.F. | 4244 | COLES | 7 | CO067 | 004A |
| AR110013 | 3" DIRECTIONAL BORE | L.F. | 1560 | COLES | 7 | CO067 | 004A |
| AR110504 | 4-WAY CONCRETE ENCASED DUCT | L.F. | 310 | COLES | 7 | CO067 | 004A |
| AR115610 | ELECTRICAL HANDHOLE | EACH | 2 | COLES | 7 | CO067 | 004A |
| AR115710 | ELECTRICAL MANHOLE | EACH | 2 | COLES | 7 | CO067 | 004A |
| AR125416 | MITL-BASE MOUNTED-LED | EACH | 9 | COLES | 7 | CO067 | 004A |
| AR125442 | TAXI GUIDANCE SIGN, 2 CHARACTER | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR125443 | TAXI GUIDANCE SIGN, 3 CHARACTER | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR125446 | TAXI GUIDANCE SIGN, 6 CHARACTER | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR125932 | REPLACE SIGN PANEL | EACH | 58 | COLES | 7 | CO067 | 004A |
| AR125943 | ADJUST INPAVEMENT LIGHT | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR125961 | RELOCATE STAKE MOUNTED LIGHT | EACH | 23 | COLES | 7 | CO067 | 004A |
| AR125964 | RELOCATE TAXI GUIDANCE SIGN | EACH | 3 | COLES | 7 | CO067 | 004A |
| AR150510 | ENGINEER'S FIELD OFFICE | L.S. | 1 | COLES | 7 | CO067 | 004A |
| AR150520 | MOBILIZATION | L.S. | 1 | COLES | 7 | CO067 | 004A |
| AR150540 | HAUL ROUTE | L.S. | 1 | COLES | 7 | CO067 | 004A |
| AR152410 | UNCLASSIFIED EXCAVATION | C.Y. | 770 | COLES | 7 | CO067 | 004A |
| AR152480 | SHOULDER ADJUSTMENT | S.Y. | 9575 | COLES | 7 | CO067 | 004A |
| AR156510 | SILT FENCE | L.F. | 688 | COLES | 7 | CO067 | 004A |
| AR156513 | SEPARATION FABRIC | S.Y. | 1710 | COLES | 7 | CO067 | 004A |
| AR156530 | TEMPORARY SEEDING | ACRE | 3 | COLES | 7 | CO067 | 004A |
| AR208540 | OVERSIZE AGGREGATE | TON | 600 | COLES | 7 | CO067 | 004A |
| AR209606 | CRUSHED AGG. BASE COURSE - 6" | S.Y. | 1710 | COLES | 7 | CO067 | 004A |
| AR401614 | BIT. SURF. CSE.-METHOD II, SUPERPA | V TON | 4250 | COLES | 7 | CO067 | 004A |
| AR401630 | BITUMINOUS SURFACE TEST SECTION | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR401640 | BITUMINOUS PAVEMENT GROOVING | S.Y. | 3345 | COLES | 7 | CO067 | 004A |
| AR401650 | BITUMINOUS PAVEMENT MILLING | S.Y. | 1750 | COLES | 7 | CO067 | 004A |
| AR403614 | BIT. BASE CSE.-METHOD II, SUPERPAV | E TON | 4350 | COLES | 7 | CO067 | 004A |
| AR403630 | BITUMINOUS BASE TEST SECTION | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR501120 | RUBBLIZE PAVEMENT | S.Y. | 31935 | COLES | 7 | CO067 | 004A |
| AR501550 | PCC PAVEMENT MILLING | S.Y. | 31935 | COLES | 7 | CO067 | 004A |
| AR501900 | REMOVE PCC PAVEMENT | S.Y. | 1991 | COLES | 7 | CO067 | 004A |
| AR501910 | REMOVE & REPLACE PCC PAVEMENT | S.Y. | 34 | COLES | 7 | CO067 | 004A |
| AR602510 | BITUMINOUS PRIME COAT | GAL. | 577 | COLES | 7 | CO067 | 004A |
| AR603510 | BITUMINOUS TACK COAT | GAL. | 5500 | COLES | 7 | CO067 | 004A |
| AR620520 | PAVEMENT MARKING-WATERBORNE | S.F. | 10538 | COLES | 7 | CO067 | 004A |
| AR620525 | PAVEMENT MARKING-BLACK BORDER | S.F. | 8830 | COLES | 7 | CO067 | 004A |
| AR620900 | PAVEMENT MARKING REMOVAL | S.F. | 351 | COLES | 7 | CO067 | 004A |
| AR701512 | 12" RCP, CLASS IV | L.F. | 64 | COLES | 7 | CO067 | 004A |
| AR705526 | 6" PERFORATED UNDERDRAIN W/SOCK | L.F. | 10240 | COLES | 7 | CO067 | 004A |
| AR705546 | 6" NON PERFORATED UNDERDRAIN | L.F. | 574 | COLES | 7 | CO067 | 004A |
| AR705630 | UNDERDRAIN INSPECTION HOLE | EACH | 7 | COLES | 7 | CO067 | 004A |
| AR705635 | UNDERDRAIN COLLECTION STRUCTURE | EACH | 7 | COLES | 7 | CO067 | 004A |
| AR705640 | UNDERDRAIN CLEANOUT | EACH | 14 | COLES | 7 | CO067 | 004A |
| AR705900 | REMOVE UNDERDRAIN | L.F. | 1656 | COLES | 7 | CO067 | 004A |
| AR705904 | REMOVE UNDERDRAIN CLEANOUT | EACH | 9 | COLES | 7 | CO067 | 004A |
| AR751410 | INLET | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR751550 | MANHOLE 5' | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR751900 | REMOVE INLET | EACH | 1 | COLES | 7 | CO067 | 004A |
| AR760708 | 8" STEEL CASING | L.F. | 108 | COLES | 7 | CO067 | 004A |
| AR901510 | SEEDING | ACRE | 3 | COLES | 7 | CO067 | 004A |
| AR905530 | TOPSOILING | S.Y. | 4500 | COLES | 7 | CO067 | 004A |
| AR908510 | MULCHING | ACRE | 3 | COLES | 7 | CO067 | 004A |
| AR150510 | ENGINEER'S FIELD OFFICE | L.S. | 1 | MACON | 7 | DE083 | 001A |
| AR150520 | MOBILIZATION | L.S. | 1 | MACON | 7 | DE083 | 001A |
| AR150530 | TRAFFIC MAINTENANCE | L.S. | 1 | MACON | 7 | DE083 | 001A |
| AR150540 | HAUL ROUTE | L.S. | 1 | MACON | 7 | DE083 | 001A |
| AR152480 | SHOULDER ADJUSTMENT | S.Y. | 4360 | MACON | 7 | DE083 | 001A |
| AR201661 | CLEAN & SEAL BITUMINOUS CRACKS | L.F. | 10000 | MACON | 7 | DE083 | 001A |
| AR201670 | CRACK CONTROL FABRIC | S.Y. | 680 | MACON | 7 | DE083 | 001A |
| AR401614 | BIT. SURF. CSE.-METHOD II, SUPERPA | V TON | 9800 | MACON | 7 | DE083 | 001A |
| AR401630 | BITUMINOUS SURFACE TEST SECTION | EACH | 1 | MACON | 7 | DE083 | 001A |
| AR401640 | BITUMINOUS PAVEMENT GROOVING | S.Y. | 32500 | MACON | 7 | DE083 | 001A |
| AR401650 | BITUMINOUS PAVEMENT MILLING | S.Y. | 41400 | MACON | 7 | DE083 | 001A |
| AR401660 | SAW & SEAL BIT. JOINTS | L.F. | 4455 | MACON | 7 | DE083 | 001A |
| AR401915 | REM & REP BIT PAVEMENT - TYPE A | S.Y. | 280 | MACON | 7 | DE083 | 001A |
| AR401916 | REM & REP BIT PAVEMENT - TYPE B | S.Y. | 200 | MACON | 7 | DE083 | 001A |
| AR501922 | PCC SPALL REPAIR | S.F. | 950 | MACON | 7 | DE083 | 001A |
| AR603510 | BITUMINOUS TACK COAT | GAL. | 4140 | MACON | 7 | DE083 | 001A |
| AR605540 | CLEAN & SEAL JOINTS | L.F. | 42000 | MACON | 7 | DE083 | 001A |
| AR605541 | CLEAN & SEAL CRACKS | L.F. | 1500 | MACON | 7 | DE083 | 001A |
| AR620520 | PAVEMENT MARKING-WATERBORNE | S.F. | 143227 | MACON | 7 | DE083 | 001A |
| AR620525 | PAVEMENT MARKING-BLACK BORDER | S.F. | 28751 | MACON | 7 | DE083 | 001A |
| AR901510 | SEEDING | ACRE | 0.9 | MACON | 7 | DE083 | 001A |
| AR908510 | MULCHING | ACRE | 0.9 | MACON | 7 | DE083 | 001A |
| AR150520 | MOBILIZATION | L.S. | 1 | DUPAGE | 1 | DU086 | 007A |
| AR150530 | TRAFFIC MAINTENANCE | L.S. | 1 | DUPAGE | 1 | DU086 | 007A |
| AR152410 | UNCLASSIFIED EXCAVATION | C.Y. | 232 | DUPAGE | 1 | DU086 | 007A |
| AR152460 | TOPSOIL STRIPPING | C.Y. | 775 | DUPAGE | 1 | DU086 | 007A |
| AR156510 | SILT FENCE | L.F. | 465 | DUPAGE | 1 | DU086 | 007A |
| AR156515 | STRAW WATTLE | L.F. | 400 | DUPAGE | 1 | DU086 | 007A |
| AR156520 | INLET PROTECTION | EACH | 43 | DUPAGE | 1 | DU086 | 007A |
| AR162220 | CLASS E MANUAL SLIDE GATE-20' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162508 | CLASS E FENCE 8' | L.F. | 4487 | DUPAGE | 1 | DU086 | 007A |
| AR162531 | WALKWAY GATES, CLASS E | EACH | 5 | DUPAGE | 1 | DU086 | 007A |
| AR162610 | CLASS E GATE-10' | EACH | 2 | DUPAGE | 1 | DU086 | 007A |
| AR162614 | CLASS E GATE 14' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162616 | CLASS E GATE-16' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162716 | ELECTRIC GATE-16' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162720 | ELECTRIC GATE-20' | EACH | 3 | DUPAGE | 1 | DU086 | 007A |
| AR162722 | ELECTRIC GATE - 22' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162725 | ELECTRIC GATE-25' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162730 | ELECTRIC GATE-30' | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162900 | REMOVE CLASS E FENCE | L.F. | 4628 | DUPAGE | 1 | DU086 | 007A |
| AR162905 | REMOVE GATE | EACH | 5 | DUPAGE | 1 | DU086 | 007A |
| AR162908 | REMOVE ELECTRIC GATE | EACH | 7 | DUPAGE | 1 | DU086 | 007A |
| AR162910 | REMOVE CLASS E GATE | EACH | 7 | DUPAGE | 1 | DU086 | 007A |
| AR162920 | REMOVE MANUAL SLIDE GATE | EACH | 1 | DUPAGE | 1 | DU086 | 007A |
| AR162948 | ADJUST ELECTRIC GATE | EACH | 6 | DUPAGE | 1 | DU086 | 007A |
| AR209606 | CRUSHED AGG. BASE COURSE - 6" | S.Y. | 4676 | DUPAGE | 1 | DU086 | 007A |
| AR801759 | WILDLIFE DETERRENT BARRIER | L.F. | 10464 | DUPAGE | 1 | DU086 | 007A |
| AR801760 | CONCRETE PAD AT GATES | C.Y. | 2 | DUPAGE | 1 | DU086 | 007A |
| AR801762 | BARBED WIRE 3 STRANDS | L.F. | 19745 | DUPAGE | 1 | DU086 | 007A |
| AR901510 | SEEDING | ACRE | 1.6 | DUPAGE | 1 | DU086 | 007A |
| AR908510 | MULCHING | ACRE | 1.6 | DUPAGE | 1 | DU086 | 007A |
| AS162401 | VINYL FENCE UPGRADE | L.F. | 4713 | DUPAGE | 1 | DU086 | 007A |
| AR150510 | ENGINEER'S FIELD OFFICE | L.S. | 1 | KANKAKEE | 3 | KA049 | 002A |
| AR150520 | MOBILIZATION | L.S. | 1 | KANKAKEE | 3 | KA049 | 002A |
| AR150540 | HAUL ROUTE | L.S. | 1 | KANKAKEE | 3 | KA049 | 002A |
| AR151412 | TREE CLEARING | ACRE | 0.8 | KANKAKEE | 3 | KA049 | 002A |
| AR151420 | CLEARING TREES 0-2.5' BUTT. DIA. | EACH | 13 | KANKAKEE | 3 | KA049 | 002A |
| AR151430 | CLEARING TREES 2.5'-5' BUTT DIA. | EACH | 1 | KANKAKEE | 3 | KA049 | 002A |
| AR151450 | CLEARING AND GRUBBING | ACRE | 2.2 | KANKAKEE | 3 | KA049 | 002A |
| AR152410 | UNCLASSIFIED EXCAVATION | C.Y. | 2550 | KANKAKEE | 3 | KA049 | 002A |
| AR152541 | STABILIZATION GEOGRID | S.Y. | 1350 | KANKAKEE | 3 | KA049 | 002A |
| AR156510 | SILT FENCE | L.F. | 4300 | KANKAKEE | 3 | KA049 | 002A |
| AR156513 | SEPARATION FABRIC | S.Y. | 1350 | KANKAKEE | 3 | KA049 | 002A |
| AR156530 | TEMPORARY SEEDING | ACRE | 3 | KANKAKEE | 3 | KA049 | 002A |
| AR156531 | EROSION CONTROL BLANKET | S.Y. | 3100 | KANKAKEE | 3 | KA049 | 002A |
| AR156543 | RIPRAP-GRADATION NO. 3 | S.Y. | 320 | KANKAKEE | 3 | KA049 | 002A |
| AR156544 | RIPRAP-GRADATION NO. 4 | S.Y. | 100 | KANKAKEE | 3 | KA049 | 002A |
| AR161900 | REMOVE CLASS C FENCE | L.F. | 2250 | KANKAKEE | 3 | KA049 | 002A |
| AR162210 | CLASS E MANUAL SLIDE GATE-10' | EACH | 2 | KANKAKEE | 3 | KA049 | 002A |
| AR162216 | CLASS E MANUAL SLIDE GATE-16' | EACH | 4 | KANKAKEE | 3 | KA049 | 002A |
| AR162220 | CLASS E MANUAL SLIDE GATE-20' | EACH | 3 | KANKAKEE | 3 | KA049 | 002A |
| AR162222 | CLASS E MANUAL SLIDE GATE-22' | EACH | 1 | KANKAKEE | 3 | KA049 | 002A |
| AR162224 | CLASS E MANUAL SLIDE GATE-24' | EACH | 2 | KANKAKEE | 3 | KA049 | 002A |
| AR162530 | WALKWAY GATES, CLASS E (5') | EACH | 1 | KANKAKEE | 3 | KA049 | 002A |
| AR162810 | CLASS E FENCE 10' W/2' BURY | L.F. | 9100 | KANKAKEE | 3 | KA049 | 002A |
| AR162900 | REMOVE CLASS E FENCE | L.F. | 670 | KANKAKEE | 3 | KA049 | 002A |
| AR162910 | REMOVE CLASS E GATE | EACH | 6 | KANKAKEE | 3 | KA049 | 002A |
| AR208515 | POROUS GRANULAR EMBANKMENT | C.Y. | 1660 | KANKAKEE | 3 | KA049 | 002A |
| AR208606 | 6" AGGREGATE BASE COURSE | S.Y. | 930 | KANKAKEE | 3 | KA049 | 002A |
| AR701012 | 12" PVC STORM SEWER | L.F. | 70 | KANKAKEE | 3 | KA049 | 002A |
| AR701173 | PRECAST CONC. BOX CULVERT 7'X3' | L.F. | 40 | KANKAKEE | 3 | KA049 | 002A |
| AR701183 | PRECAST CONC. BOX CULVERT 8'X3' | L.F. | 40 | KANKAKEE | 3 | KA049 | 002A |
| AR701342 | 42" RCP, CLASS II | L.F. | 80 | KANKAKEE | 3 | KA049 | 002A |
| AR752501 | GRATING | S.F. | 195 | KANKAKEE | 3 | KA049 | 002A |
| AR752600 | CONCRETE HEADWALL | EACH | 2 | KANKAKEE | 3 | KA049 | 002A |
| AR754910 | REMOVE PAVED DITCH | L.F. | 150 | KANKAKEE | 3 | KA049 | 002A |
| AR800173 | WILDLIFE DETERRENT BARRIER - PAD | S.F. | 450 | KANKAKEE | 3 | KA049 | 002A |
| AR901510 | SEEDING | ACRE | 7.8 | KANKAKEE | 3 | KA049 | 002A |
| AR908514 | LIGHT-DUTY HYDRAULIC MULCH | ACRE | 7.1 | KANKAKEE | 3 | KA049 | 002A |
| AR108158 | 1/C #8 5 KV UG CABLE IN UD | L.F. | 8635 | WILL | 1 | LE053 | 003A |
| AR108258 | 2/C #8 5 KV UG CABLE IN UD | L.F. | 3361 | WILL | 1 | LE053 | 003A |
| AR108960 | REMOVE CABLE | L.F. | 2101 | WILL | 1 | LE053 | 003A |
| AR109200 | INSTALL ELECTRICAL EQUIPMENT | L.S. | 1 | WILL | 1 | LE053 | 003A |
| AR109311 | 7.5 KW REGULATOR, STYLE 1 | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR109903 | REMOVE REGULATOR | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR110552 | EXTEND 2-WAY DUCT | L.F. | 77 | WILL | 1 | LE053 | 003A |
| AR110554 | EXTEND 4-WAY DUCT | L.F. | 65 | WILL | 1 | LE053 | 003A |
| AR110610 | ELECTRICAL HANDHOLE | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR125410 | MITL-STAKE MOUNTED | EACH | 16 | WILL | 1 | LE053 | 003A |
| AR125411 | MITL-STAKE MOUNTED-LED | EACH | 52 | WILL | 1 | LE053 | 003A |
| AR125415 | MITL-BASE MOUNTED | EACH | 2 | WILL | 1 | LE053 | 003A |
| AR125416 | MITL-BASE MOUNTED-LED | EACH | 8 | WILL | 1 | LE053 | 003A |
| AR125442 | TAXI GUIDANCE SIGN, 2 CHARACTER | EACH | 2 | WILL | 1 | LE053 | 003A |
| AR125443 | TAXI GUIDANCE SIGN, 3 CHARACTER | EACH | 3 | WILL | 1 | LE053 | 003A |
| AR125444 | TAXI GUIDANCE SIGN, 4 CHARACTER | EACH | 2 | WILL | 1 | LE053 | 003A |
| AR125445 | TAXI GUIDANCE SIGN, 5 CHARACTER | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR125446 | TAXI GUIDANCE SIGN, 6 CHARACTER | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR125901 | REMOVE STAKE MOUNTED LIGHT | EACH | 42 | WILL | 1 | LE053 | 003A |
| AR125902 | REMOVE BASE MOUNTED LIGHT | EACH | 12 | WILL | 1 | LE053 | 003A |
| AR125904 | REMOVE TAXI GUIDANCE SIGN | EACH | 10 | WILL | 1 | LE053 | 003A |
| AR150510 | ENGINEER'S FIELD OFFICE | L.S. | 1 | WILL | 1 | LE053 | 003A |
| AR150520 | MOBILIZATION | L.S. | 1 | WILL | 1 | LE053 | 003A |
| AR150530 | TRAFFIC MAINTENANCE | L.S. | 1 | WILL | 1 | LE053 | 003A |
| AR150540 | HAUL ROUTE | L.S. | 1 | WILL | 1 | LE053 | 003A |
| AR152410 | UNCLASSIFIED EXCAVATION | C.Y. | 12195 | WILL | 1 | LE053 | 003A |
| AR152540 | SOIL STABILIZATION FABRIC | S.Y. | 7690 | WILL | 1 | LE053 | 003A |
| AR154606 | GRANULAR DRAINAGE SUBBASE - 6" | S.Y. | 20374 | WILL | 1 | LE053 | 003A |
| AR156510 | SILT FENCE | L.F. | 192 | WILL | 1 | LE053 | 003A |
| AR156513 | SEPARATION FABRIC | S.Y. | 12684 | WILL | 1 | LE053 | 003A |
| AR156520 | INLET PROTECTION | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR156531 | EROSION CONTROL BLANKET | S.Y. | 854 | WILL | 1 | LE053 | 003A |
| AR156533 | TEMPORARY SEED AND MULCH | ACRE | 2.8 | WILL | 1 | LE053 | 003A |
| AR156534 | TURF REINFORCING MAT | S.Y. | 369 | WILL | 1 | LE053 | 003A |
| AR209611 | CRUSHED AGGREGATE BASE COURSE-11" | S.Y. | 20443 | WILL | 1 | LE053 | 003A |
| AR401614 | BIT. SURF. CSE.-METHOD II, SUPERPA | V TON | 2513 | WILL | 1 | LE053 | 003A |
| AR401630 | BITUMINOUS SURFACE TEST SECTION | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR401650 | BITUMINOUS PAVEMENT MILLING | S.Y. | 630 | WILL | 1 | LE053 | 003A |
| AR401660 | SAW & SEAL BIT. JOINTS | L.F. | 727 | WILL | 1 | LE053 | 003A |
| AR401665 | BITUMINOUS PAVEMENT SAWING | L.F. | 1397 | WILL | 1 | LE053 | 003A |
| AR401900 | REMOVE BITUMINOUS PAVEMENT | S.Y. | 13659 | WILL | 1 | LE053 | 003A |
| AR403614 | BIT. BASE CSE.-METHOD II, SUPERPAV | E TON | 5543 | WILL | 1 | LE053 | 003A |
| AR403630 | BITUMINOUS BASE TEST SECTION | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR602510 | BITUMINOUS PRIME COAT | GAL. | 5918 | WILL | 1 | LE053 | 003A |
| AR603510 | BITUMINOUS TACK COAT | GAL. | 6137 | WILL | 1 | LE053 | 003A |
| AR620520 | PAVEMENT MARKING-WATERBORNE | S.F. | 4279 | WILL | 1 | LE053 | 003A |
| AR620525 | PAVEMENT MARKING-BLACK BORDER | S.F. | 5908 | WILL | 1 | LE053 | 003A |
| AR620530 | PAVEMENT MARKING-EPOXY | S.F. | 1164 | WILL | 1 | LE053 | 003A |
| AR620590 | TEMPORARY MARKING | S.F. | 1202 | WILL | 1 | LE053 | 003A |
| AR620900 | PAVEMENT MARKING REMOVAL | S.F. | 1596 | WILL | 1 | LE053 | 003A |
| AR705506 | 6" PERFORATED UNDERDRAIN | L.F. | 5233 | WILL | 1 | LE053 | 003A |
| AR705630 | UNDERDRAIN INSPECTION HOLE | EACH | 4 | WILL | 1 | LE053 | 003A |
| AR705640 | UNDERDRAIN CLEANOUT | EACH | 10 | WILL | 1 | LE053 | 003A |
| AR705900 | REMOVE UNDERDRAIN | L.F. | 5712 | WILL | 1 | LE053 | 003A |
| AR705903 | REMOVE UNDERDRAIN INSP. HOLE | EACH | 4 | WILL | 1 | LE053 | 003A |
| AR705904 | REMOVE UNDERDRAIN CLEANOUT | EACH | 7 | WILL | 1 | LE053 | 003A |
| AR705943 | ADJUST UNDERDRAIN INSP. HOLE | EACH | 1 | WILL | 1 | LE053 | 003A |
| AR800910 | BITUMINOUS PRESSURE RELIEF JOINT | L.F. | 110 | WILL | 1 | LE053 | 003A |
| AR803003 | CONCRETE CABLE BOTTOM | S.Y. | 191 | WILL | 1 | LE053 | 003A |
| AR901510 | SEEDING | ACRE | 3.7 | WILL | 1 | LE053 | 003A |
| AR904510 | SODDING | S.Y. | 305 | WILL | 1 | LE053 | 003A |
| AR905510 | TOPSOILING (FROM ON SITE) | C.Y. | 2075 | WILL | 1 | LE053 | 003A |
| AR908510 | MULCHING | ACRE | 3.6 | WILL | 1 | LE053 | 003A |
| AR910216 | TEMPORARY CONSTRUCTION SIGNS | L.S. | 1 | WILL | 1 | LE053 | 003A |
| AR108108 | 1/C #8 5 KV UG CABLE | L.F. | 952 | CHAMPAIGN | 5 | UN059 | 006A |
| AR108158 | 1/C #8 5 KV UG CABLE IN UD | L.F. | 17102 | CHAMPAIGN | 5 | UN059 | 006A |
| AR108208 | 2/C #8 5 KV UG CABLE | L.F. | 553 | CHAMPAIGN | 5 | UN059 | 006A |
| AR108258 | 2/C #8 5 KV UG CABLE IN UD | L.F. | 4486 | CHAMPAIGN | 5 | UN059 | 006A |
| AR108706 | 1/C #6 COUNTERPOISE | L.F. | 18384 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125100 | ELEVATED RETROREFLECTIVE MARKER | EACH | 17 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125400 | REPLACE ISOLATION TRANSFORMER | EACH | 50 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125401 | REPLACE LIGHT FIXTURE | EACH | 50 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125416 | MITL-BASE MOUNTED-LED | EACH | 272 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125442 | TAXI GUIDANCE SIGN, 2 CHARACTER | EACH | 8 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125443 | TAXI GUIDANCE SIGN, 3 CHARACTER | EACH | 1 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125444 | TAXI GUIDANCE SIGN, 4 CHARACTER | EACH | 12 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125445 | TAXI GUIDANCE SIGN, 5 CHARACTER | EACH | 6 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125448 | TAXI GUIDANCE SIGN, 8 CHARACTER | EACH | 4 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125462 | TAXI GUIDANCE SIGN, UNLIT | EACH | 3 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125565 | SPLICE CAN | EACH | 3 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125904 | REMOVE TAXI GUIDANCE SIGN | EACH | 31 | CHAMPAIGN | 5 | UN059 | 006A |
| AR125913 | REMOVE EDGE LIGHT | EACH | 292 | CHAMPAIGN | 5 | UN059 | 006A |
| AR150520 | MOBILIZATION | L.S. | 1 | CHAMPAIGN | 5 | UN059 | 006A |
| AR401921 | REMOVE PAVEMENT | S.Y. | 6 | CHAMPAIGN | 5 | UN059 | 006A |
| AR610510 | STRUCTURAL PC CONCRETE | C.Y. | 5 | CHAMPAIGN | 5 | UN059 | 006A |
| AR901515 | SEEDING | S.Y. | 1890 | CHAMPAIGN | 5 | UN059 | 006A |
| AR908516 | MULCHING | S.Y. | 1890 | CHAMPAIGN | 5 | UN059 | 006A |
| AR910200 | ROADWAY SIGN | EACH | 3 | CHAMPAIGN | 5 | UN059 | 006A |
| AS108108 | 1/C #8 5 KV UG CABLE | L.F. | 266 | CHAMPAIGN | 5 | UN059 | 006A |
| AS108158 | 1/C #8 5 KV UG CABLE IN UD | L.F. | 3056 | CHAMPAIGN | 5 | UN059 | 006A |
| AS108258 | 2/C #8 5 KV UG CABLE IN UD | L.F. | 522 | CHAMPAIGN | 5 | UN059 | 006A |
| AS108706 | 1/C #6 COUNTERPOISE | L.F. | 3623 | CHAMPAIGN | 5 | UN059 | 006A |
| AS125416 | MITL-BASE MOUNTED-LED | EACH | 72 | CHAMPAIGN | 5 | UN059 | 006A |
| AS125442 | TAXI GUIDANCE SIGN, 2 CHARACTER | EACH | 1 | CHAMPAIGN | 5 | UN059 | 006A |
| AS125444 | TAXI GUIDANCE SIGN, 4 CHARACTER | EACH | 5 | CHAMPAIGN | 5 | UN059 | 006A |
| AS125445 | TAXI GUIDANCE SIGN, 5 CHARACTER | EACH | 2 | CHAMPAIGN | 5 | UN059 | 006A |
| AS125904 | REMOVE TAXI GUIDANCE SIGN | EACH | 8 | CHAMPAIGN | 5 | UN059 | 006A |
| AS125913 | REMOVE EDGE LIGHT | EACH | 68 | CHAMPAIGN | 5 | UN059 | 006A |
| AS150520 | MOBILIZATION | L.S. | 1 | CHAMPAIGN | 5 | UN059 | 006A |
| AS901515 | SEEDING | S.Y. | 323 | CHAMPAIGN | 5 | UN059 | 006A |
| AS908516 | MULCHING | S.Y. | 323 | CHAMPAIGN | 5 | UN059 | 006A |
| AR150510 | ENGINEER'S FIELD OFFICE | L.S. | 1 | LAKE | 1 | WA074 | 008A |
| AR150520 | MOBILIZATION | L.S. | 1 | LAKE | 1 | WA074 | 008A |
| AR152480 | SHOULDER ADJUSTMENT | S.Y. | 50 | LAKE | 1 | WA074 | 008A |
| AR201663 | SAND MIX CRACK REPAIR | L.F. | 300 | LAKE | 1 | WA074 | 008A |
| AR401610 | BITUMINOUS SURFACE COURSE | TON | 8700 | LAKE | 1 | WA074 | 008A |
| AR401630 | BITUMINOUS SURFACE TEST SECTION | EACH | 1 | LAKE | 1 | WA074 | 008A |
| AR401640 | BITUMINOUS PAVEMENT GROOVING | S.Y. | 86390 | LAKE | 1 | WA074 | 008A |
| AR401650 | BITUMINOUS PAVEMENT MILLING | S.Y. | 100005 | LAKE | 1 | WA074 | 008A |
| AR401915 | REM & REP BIT PAVEMENT - TYPE A | S.Y. | 125 | LAKE | 1 | WA074 | 008A |
| AR603510 | BITUMINOUS TACK COAT | GAL. | 12000 | LAKE | 1 | WA074 | 008A |
| AR620520 | PAVEMENT MARKING-WATERBORNE | S.F. | 105200 | LAKE | 1 | WA074 | 008A |